(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 127)
    (no_connects 0)
    (area 94.437999 85.039999 180.898001 139.750001)
    (thickness 1.6)
    (drawings 50)
    (tracks 375)
    (zones 0)
    (modules 57)
    (nets 116)
  )
  (page A)
  (title_block
    (title "BeagleBone Black Cape")
    (date 2016-08-09)
    (rev 1.4)
    (comment 1 "License: GPL v3, https://github.com/bubbapizza/BBBdc")
    (comment 2 "Design by Rob Caruso")
    (comment 3 "Layout by Shawn Wilson")
  )
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.5)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.2286)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.508)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1.27 1.27)
    (mod_text_width 0.254)
    (pad_size 1.524 1.524)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFE77F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory mfg/))
  )
  (net 0 "")
  (net 1 /A0)
  (net 2 /A1)
  (net 3 /A2)
  (net 4 /I2C2_SCL)
  (net 5 /I2C2_SDA)
  (net 6 /SYS_5V)
  (net 7 GND)
  (net 8 +3V3)
  (net 9 +12V)
  (net 10 +5V)
  (net 11 "Net-(D1-Pad2)")
  (net 12 "Net-(D2-Pad2)")
  (net 13 "Net-(D3-Pad1)")
  (net 14 "Net-(D3-Pad2)")
  (net 15 "Net-(D4-Pad1)")
  (net 16 "Net-(D4-Pad2)")
  (net 17 "Net-(D5-Pad1)")
  (net 18 "Net-(D5-Pad2)")
  (net 19 "Net-(D6-Pad1)")
  (net 20 "Net-(D6-Pad2)")
  (net 21 "Net-(D9-Pad1)")
  (net 22 /MMC1_DAT6)
  (net 23 /MMC1_DAT7)
  (net 24 /MMC1_DAT2)
  (net 25 /MMC1_DAT3)
  (net 26 /GPIO_66)
  (net 27 /GPIO_67)
  (net 28 /GPIO_69)
  (net 29 /GPIO_68)
  (net 30 /GPIO_45)
  (net 31 /GPIO_44)
  (net 32 /EHRPWM2B)
  (net 33 /GPIO_26)
  (net 34 /LOCK_RELAYS/R1_ENGAGE)
  (net 35 /LOCK_RELAYS/R1_READ)
  (net 36 /LOCK_RELAYS/R2_ENGAGE)
  (net 37 /LOCK_RELAYS/R2_READ)
  (net 38 /EHRPWM2A)
  (net 39 /MMC1_CMD)
  (net 40 /MMC1_CLK)
  (net 41 /MMC1_DAT5)
  (net 42 /MMC1_DAT4)
  (net 43 /MMC1_DAT1)
  (net 44 /MMC1_DAT0)
  (net 45 /GPIO_61)
  (net 46 /LCD_VSYNC)
  (net 47 /LCD_PCLK)
  (net 48 /LCD_HSYNC)
  (net 49 /LCD_AC_BIAS)
  (net 50 /LCD_DATA14)
  (net 51 /LCD_DATA15)
  (net 52 /LCD_DATA13)
  (net 53 /LCD_DATA11)
  (net 54 /LCD_DATA12)
  (net 55 /LCD_DATA10)
  (net 56 /LCD_DATA8)
  (net 57 /LCD_DATA9)
  (net 58 /LCD_DATA6)
  (net 59 /LCD_DATA7)
  (net 60 /LCD_DATA4)
  (net 61 /LCD_DATA5)
  (net 62 /LCD_DATA2)
  (net 63 /LCD_DATA3)
  (net 64 /LCD_DATA0)
  (net 65 /LCD_DATA1)
  (net 66 /PWR_BUT)
  (net 67 /SYS_RESETn)
  (net 68 /UART4_RXD)
  (net 69 /GPIO_60)
  (net 70 /UART4_TXD)
  (net 71 /EHRPWM1A)
  (net 72 /GPIO_48)
  (net 73 /EHRPWM1B)
  (net 74 /SPIO_CSO)
  (net 75 /SPIO_D1)
  (net 76 /SPIO_DO)
  (net 77 /SPIO_SLCK)
  (net 78 /GPIO_49)
  (net 79 /UART1_TXD)
  (net 80 /GPIO_117)
  (net 81 /UART1_RXD)
  (net 82 /GPIO_115)
  (net 83 /SPI1_CS0)
  (net 84 /SPI1_D0)
  (net 85 /GPIO_112)
  (net 86 /SPI1_SCLK)
  (net 87 /VADC)
  (net 88 /AIN4)
  (net 89 /AGND)
  (net 90 /AIN6)
  (net 91 /AIN5)
  (net 92 /AIN2)
  (net 93 /AIN3)
  (net 94 /AIN0)
  (net 95 /AIN1)
  (net 96 /GPIO_20)
  (net 97 /ECAPWMO)
  (net 98 "Net-(P6-Pad2)")
  (net 99 "Net-(P7-Pad1)")
  (net 100 "Net-(P7-Pad2)")
  (net 101 "Net-(P8-Pad1)")
  (net 102 "Net-(P8-Pad3)")
  (net 103 "Net-(Q1-Pad2)")
  (net 104 "Net-(Q2-Pad2)")
  (net 105 "Net-(Q3-Pad2)")
  (net 106 "Net-(Q4-Pad2)")
  (net 107 "Net-(R20-Pad2)")
  (net 108 "Net-(R21-Pad2)")
  (net 109 "Net-(RLY1-Pad6)")
  (net 110 "Net-(RLY1-Pad7)")
  (net 111 "Net-(RLY2-Pad7)")
  (net 112 "Net-(U1-Pad7)")
  (net 113 "Net-(U3-Pad6)")
  (net 114 "Net-(U4-Pad6)")
  (net 115 "Net-(RLY2-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2286)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /AGND)
    (add_net /AIN0)
    (add_net /AIN1)
    (add_net /AIN2)
    (add_net /AIN3)
    (add_net /AIN4)
    (add_net /AIN5)
    (add_net /AIN6)
    (add_net /ECAPWMO)
    (add_net /EHRPWM1A)
    (add_net /EHRPWM1B)
    (add_net /EHRPWM2A)
    (add_net /EHRPWM2B)
    (add_net /GPIO_112)
    (add_net /GPIO_115)
    (add_net /GPIO_117)
    (add_net /GPIO_20)
    (add_net /GPIO_26)
    (add_net /GPIO_44)
    (add_net /GPIO_45)
    (add_net /GPIO_48)
    (add_net /GPIO_49)
    (add_net /GPIO_60)
    (add_net /GPIO_61)
    (add_net /GPIO_66)
    (add_net /GPIO_67)
    (add_net /GPIO_68)
    (add_net /GPIO_69)
    (add_net /I2C2_SCL)
    (add_net /I2C2_SDA)
    (add_net /LCD_AC_BIAS)
    (add_net /LCD_DATA0)
    (add_net /LCD_DATA1)
    (add_net /LCD_DATA10)
    (add_net /LCD_DATA11)
    (add_net /LCD_DATA12)
    (add_net /LCD_DATA13)
    (add_net /LCD_DATA14)
    (add_net /LCD_DATA15)
    (add_net /LCD_DATA2)
    (add_net /LCD_DATA3)
    (add_net /LCD_DATA4)
    (add_net /LCD_DATA5)
    (add_net /LCD_DATA6)
    (add_net /LCD_DATA7)
    (add_net /LCD_DATA8)
    (add_net /LCD_DATA9)
    (add_net /LCD_HSYNC)
    (add_net /LCD_PCLK)
    (add_net /LCD_VSYNC)
    (add_net /LOCK_RELAYS/R1_ENGAGE)
    (add_net /LOCK_RELAYS/R1_READ)
    (add_net /LOCK_RELAYS/R2_ENGAGE)
    (add_net /LOCK_RELAYS/R2_READ)
    (add_net /MMC1_CLK)
    (add_net /MMC1_CMD)
    (add_net /MMC1_DAT0)
    (add_net /MMC1_DAT1)
    (add_net /MMC1_DAT2)
    (add_net /MMC1_DAT3)
    (add_net /MMC1_DAT4)
    (add_net /MMC1_DAT5)
    (add_net /MMC1_DAT6)
    (add_net /MMC1_DAT7)
    (add_net /PWR_BUT)
    (add_net /SPI1_CS0)
    (add_net /SPI1_D0)
    (add_net /SPI1_SCLK)
    (add_net /SPIO_CSO)
    (add_net /SPIO_D1)
    (add_net /SPIO_DO)
    (add_net /SPIO_SLCK)
    (add_net /SYS_RESETn)
    (add_net /UART1_RXD)
    (add_net /UART1_TXD)
    (add_net /UART4_RXD)
    (add_net /UART4_TXD)
    (add_net /VADC)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(R20-Pad2)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(RLY1-Pad6)")
    (add_net "Net-(RLY1-Pad7)")
    (add_net "Net-(RLY2-Pad4)")
    (add_net "Net-(RLY2-Pad7)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U4-Pad6)")
  )
  (net_class "12V Power" ""
    (clearance 0.2286)
    (trace_width 2)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +12V)
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P7-Pad2)")
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(P8-Pad3)")
  )
  (net_class "3.3V Power" ""
    (clearance 0.2286)
    (trace_width 0.5)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
  )
  (net_class "5V Power" ""
    (clearance 0.2286)
    (trace_width 1.5)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /SYS_5V)
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 0)
    (at 156.21 130.77 90)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at -2.453 0 180) (layer F.SilkS))
    (fp_text value "10 uF (25V)" (at 1.25 3.8 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 0)
    (at 138.43 130.77 90)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at -2.58 0 180) (layer F.SilkS))
    (fp_text value "22 uF (16V)" (at 1.25 3.8 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 57A794A3)
    (at 156.21 123.19 270)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at 3.048 -2.921 360) (layer F.SilkS))
    (fp_text value "PWR +12V" (at 1.3 -2.9 270) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 57A79522)
    (at 138.43 123.19 270)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D2 (at 2.54 3.048 360) (layer F.SilkS))
    (fp_text value "PWR +5V" (at 1.3 -2.9 270) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5684426D)
    (at 169.1005 92.456 270)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at 1.5875 2.7305 270) (layer F.SilkS))
    (fp_text value RED (at 1.3 -2.9 270) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 56844271)
    (at 169.1005 98.425 270)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D4 (at 1.27 2.921 450) (layer F.SilkS))
    (fp_text value GREEN (at 1.3 -2.9 270) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 552FFCCE)
    (at 133.985 107.44454 180)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D7 (at 5.715 0.12954 180) (layer F.SilkS))
    (fp_text value 1N4007 (at 4.37134 -3.55854 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D5-Pad1)"))
    (pad 1 thru_hole rect (at 0 -0.00254) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 552FFCCE)
    (at 133.985 110.49 180)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D8 (at 5.715 -0.00254 180) (layer F.SilkS))
    (fp_text value 1N4007 (at 4.37134 -3.55854 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D6-Pad1)"))
    (pad 1 thru_hole rect (at 0 -0.00254) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 5676ED67)
    (at 161.163 125.73254)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D9 (at 5.5118 -0.00254) (layer F.SilkS))
    (fp_text value 1N4007 (at 4.37134 -3.55854) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254 180) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 1 thru_hole rect (at 0 -0.00254 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D9-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 57A782A6)
    (at 118.745 114.681 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 2.413 4.826 270) (layer F.SilkS) hide)
    (fp_text value "RTC MODULE" (at 2.286 5.207 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(P6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /I2C2_SCL))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /I2C2_SDA))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57A784C0)
    (at 170.8785 121.2215 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0.635 -2.54 180) (layer F.SilkS) hide)
    (fp_text value "NC/NO JUMPER" (at 0 -3.1 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(P7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(P7-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57A784E7)
    (at 167.3225 121.2215 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at -1.524 -2.413 180) (layer F.SilkS) hide)
    (fp_text value "NC/NO JUMPER" (at 0 -3.1 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(P8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(P8-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5676EFCD)
    (at 164.338 92.7735 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at -2.159 1.3335 360) (layer F.SilkS))
    (fp_text value 2N7000 (at 0 3 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D3-Pad1)"))
    (pad 1 thru_hole oval (at 0 0) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5676EFD7)
    (at 158.369 92.7735 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at -1.7145 1.5875 360) (layer F.SilkS))
    (fp_text value 2N7000 (at 0 3 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D4-Pad1)"))
    (pad 1 thru_hole oval (at 0 0) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 54F24281)
    (at 127.1905 93.0275 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 1.905 -3.4925 180) (layer F.SilkS))
    (fp_text value 2N7000 (at 0 3 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(Q3-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D5-Pad1)"))
    (pad 1 thru_hole oval (at 0 0) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 54F24281)
    (at 131.572 124.46 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at 5.08 -0.635 180) (layer F.SilkS))
    (fp_text value 2N7000 (at 0 3 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(Q4-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D6-Pad1)"))
    (pad 1 thru_hole oval (at 0 0) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm (layer F.Cu) (tedit 5681A802)
    (at 134.112 103.251 180)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U3 (at 3.683 2.286 270) (layer F.SilkS))
    (fp_text value 4N25 (at 0 -3.72 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(R20-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(RLY1-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 /LOCK_RELAYS/R1_READ))
    (pad 5 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (pad 6 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(U3-Pad6)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm (layer F.Cu) (tedit 5681A80A)
    (at 133.985 120.142 180)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U4 (at 3.81 2.032 270) (layer F.SilkS))
    (fp_text value 4N25 (at 0 -3.72 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(R21-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(P7-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 /LOCK_RELAYS/R2_READ))
    (pad 5 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (pad 6 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(U4-Pad6)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 57A78255)
    (at 101.6 134.112 90)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 3.937 3.81 180) (layer F.SilkS) hide)
    (fp_text value 24C256 (at 3.937 3.81 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /A0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 /A1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 /A2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /I2C2_SDA))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /I2C2_SCL))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(U1-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 106.426 122.428 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R1 (at 2.7305 -0.0635 360) (layer F.SilkS))
    (fp_text value 4.7k (at -1.143 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /A2))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 103.378 122.428 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R2 (at 2.7305 0 360) (layer F.SilkS))
    (fp_text value 4.7k (at -1.143 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /A1))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 100.33 122.428 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R3 (at 2.794 0 360) (layer F.SilkS))
    (fp_text value 4.7k (at -1.143 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /A0))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 109.474 122.428 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R4 (at 2.667 -0.127 540) (layer F.SilkS))
    (fp_text value 5.6k (at -1.143 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /I2C2_SCL))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 112.522 122.428 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R5 (at 2.667 -0.1905 360) (layer F.SilkS))
    (fp_text value 5.6k (at -1.143 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /I2C2_SDA))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5676EE62)
    (at 166.878 129.54 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R6 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 1k (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D1-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 133.096 129.54 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R7 (at -3.81 0.254 180) (layer F.SilkS))
    (fp_text value 330 (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D2-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5676F00F)
    (at 146.05 93.5228 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R8 (at 2.54 -0.1016 180) (layer F.SilkS))
    (fp_text value 330 (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /GPIO_69))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5676F012)
    (at 149.1488 93.5228 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R9 (at 2.54 -0.0508 180) (layer F.SilkS))
    (fp_text value 10k (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5676EE7C)
    (at 169.1005 109.982 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R10 (at -1.016 -2.6035 270) (layer F.SilkS))
    (fp_text value 1k (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D3-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5676F018)
    (at 152.2476 93.5228 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R11 (at 2.6416 0.4064 180) (layer F.SilkS))
    (fp_text value 330 (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(Q2-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /GPIO_45))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5676F00C)
    (at 142.9512 93.5228 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R12 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 10k (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(Q2-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5676EE75)
    (at 169.1005 104.902 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R13 (at -1.0795 -2.6035 270) (layer F.SilkS))
    (fp_text value 1k (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D4-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 127 129.54 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R14 (at -3.81 0.127 180) (layer F.SilkS))
    (fp_text value 330 (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D5-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 130.048 129.54 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R15 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 330 (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(D6-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 130.4544 93.5228 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R16 (at 2.54 0.0508 180) (layer F.SilkS))
    (fp_text value 330 (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(Q3-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /LOCK_RELAYS/R1_ENGAGE))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 136.7028 93.5228 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R17 (at 2.54 0.3048 180) (layer F.SilkS))
    (fp_text value 330 (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(Q4-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /LOCK_RELAYS/R2_ENGAGE))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 133.604 93.5228 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R18 (at 2.54 0.0508 180) (layer F.SilkS))
    (fp_text value 10k (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(Q3-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 139.8524 93.5228 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R19 (at 2.5908 0.2032 180) (layer F.SilkS))
    (fp_text value 10k (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(Q4-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5676EE5D)
    (at 160.655 129.54 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R20 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 1k (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(R20-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5676EE59)
    (at 163.7665 129.54 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R21 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 1k (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(R21-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 121.793 93.5228 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R22 (at 2.54 0.2286 180) (layer F.SilkS))
    (fp_text value 2k (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /LOCK_RELAYS/R1_READ))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 0)
    (at 97.536 128.524 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 4.445 0 360) (layer F.SilkS))
    (fp_text value "0.1uF (25V)" (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
  )
  (module beagleboard:BEAGLEBONE_BLACK_NO_PERIMETER (layer F.Cu) (tedit 56844887)
    (at 94.488 139.7)
    (fp_text reference P1 (at 8.255 -22.225) (layer F.SilkS) hide)
    (fp_text value BEAGLEBONE_BLACK (at 7.62 -37.465) (layer F.SilkS) hide)
    (pad A1 thru_hole rect (at 19.685 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad A2 thru_hole circle (at 19.685 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad A3 thru_hole circle (at 22.225 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /MMC1_DAT6))
    (pad A4 thru_hole circle (at 22.225 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /MMC1_DAT7))
    (pad A5 thru_hole circle (at 24.765 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /MMC1_DAT2))
    (pad A6 thru_hole circle (at 24.765 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /MMC1_DAT3))
    (pad A7 thru_hole circle (at 27.305 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /GPIO_66))
    (pad A8 thru_hole circle (at 27.305 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /GPIO_67))
    (pad A9 thru_hole circle (at 29.845 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /GPIO_69))
    (pad A10 thru_hole circle (at 29.845 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /GPIO_68))
    (pad A11 thru_hole circle (at 32.385 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /GPIO_45))
    (pad A12 thru_hole circle (at 32.385 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /GPIO_44))
    (pad A13 thru_hole circle (at 34.925 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /EHRPWM2B))
    (pad A14 thru_hole circle (at 34.925 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /GPIO_26))
    (pad A15 thru_hole circle (at 37.465 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /LOCK_RELAYS/R1_ENGAGE))
    (pad A16 thru_hole circle (at 37.465 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /LOCK_RELAYS/R1_READ))
    (pad A17 thru_hole circle (at 40.005 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /LOCK_RELAYS/R2_ENGAGE))
    (pad A18 thru_hole circle (at 40.005 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /LOCK_RELAYS/R2_READ))
    (pad A19 thru_hole circle (at 42.545 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /EHRPWM2A))
    (pad A20 thru_hole circle (at 42.545 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /MMC1_CMD))
    (pad A21 thru_hole circle (at 45.085 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /MMC1_CLK))
    (pad A22 thru_hole circle (at 45.085 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /MMC1_DAT5))
    (pad A23 thru_hole circle (at 47.625 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /MMC1_DAT4))
    (pad A24 thru_hole circle (at 47.625 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /MMC1_DAT1))
    (pad A25 thru_hole circle (at 50.165 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /MMC1_DAT0))
    (pad A26 thru_hole circle (at 50.165 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /GPIO_61))
    (pad A27 thru_hole circle (at 52.705 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /LCD_VSYNC))
    (pad A28 thru_hole circle (at 52.705 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /LCD_PCLK))
    (pad A29 thru_hole circle (at 55.245 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /LCD_HSYNC))
    (pad A30 thru_hole circle (at 55.245 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /LCD_AC_BIAS))
    (pad A31 thru_hole circle (at 57.785 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /LCD_DATA14))
    (pad A32 thru_hole circle (at 57.785 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /LCD_DATA15))
    (pad A33 thru_hole circle (at 60.325 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /LCD_DATA13))
    (pad A34 thru_hole circle (at 60.325 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /LCD_DATA11))
    (pad A35 thru_hole circle (at 62.865 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /LCD_DATA12))
    (pad A36 thru_hole circle (at 62.865 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 /LCD_DATA10))
    (pad A37 thru_hole circle (at 65.405 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 /LCD_DATA8))
    (pad A38 thru_hole circle (at 65.405 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 /LCD_DATA9))
    (pad A39 thru_hole circle (at 67.945 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 /LCD_DATA6))
    (pad A40 thru_hole circle (at 67.945 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /LCD_DATA7))
    (pad A41 thru_hole circle (at 70.485 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /LCD_DATA4))
    (pad A42 thru_hole circle (at 70.485 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 /LCD_DATA5))
    (pad A43 thru_hole circle (at 73.025 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /LCD_DATA2))
    (pad A44 thru_hole circle (at 73.025 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 /LCD_DATA3))
    (pad A45 thru_hole circle (at 75.565 -50.165) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 /LCD_DATA0))
    (pad A46 thru_hole circle (at 75.565 -52.705) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 /LCD_DATA1))
    (pad B2 thru_hole circle (at 19.685 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad B3 thru_hole circle (at 22.225 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (pad B4 thru_hole circle (at 22.225 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (pad B5 thru_hole circle (at 24.765 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad B6 thru_hole circle (at 24.765 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad B7 thru_hole circle (at 27.305 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SYS_5V))
    (pad B8 thru_hole circle (at 27.305 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SYS_5V))
    (pad B9 thru_hole circle (at 29.845 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 /PWR_BUT))
    (pad B10 thru_hole circle (at 29.845 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 /SYS_RESETn))
    (pad B11 thru_hole circle (at 32.385 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 /UART4_RXD))
    (pad B12 thru_hole circle (at 32.385 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 /GPIO_60))
    (pad B13 thru_hole circle (at 34.925 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 /UART4_TXD))
    (pad B14 thru_hole circle (at 34.925 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 /EHRPWM1A))
    (pad B15 thru_hole circle (at 37.465 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 /GPIO_48))
    (pad B16 thru_hole circle (at 37.465 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 /EHRPWM1B))
    (pad B17 thru_hole circle (at 40.005 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 /SPIO_CSO))
    (pad B18 thru_hole circle (at 40.005 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 /SPIO_D1))
    (pad B19 thru_hole circle (at 42.545 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /I2C2_SCL))
    (pad B20 thru_hole circle (at 42.545 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /I2C2_SDA))
    (pad B21 thru_hole circle (at 45.085 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 76 /SPIO_DO))
    (pad B22 thru_hole circle (at 45.085 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 77 /SPIO_SLCK))
    (pad B23 thru_hole circle (at 47.625 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 78 /GPIO_49))
    (pad B24 thru_hole circle (at 47.625 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 /UART1_TXD))
    (pad B25 thru_hole circle (at 50.165 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 /GPIO_117))
    (pad B26 thru_hole circle (at 50.165 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 81 /UART1_RXD))
    (pad B27 thru_hole circle (at 52.705 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 82 /GPIO_115))
    (pad B28 thru_hole circle (at 52.705 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 83 /SPI1_CS0))
    (pad B29 thru_hole circle (at 55.245 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 84 /SPI1_D0))
    (pad B30 thru_hole circle (at 55.245 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 85 /GPIO_112))
    (pad B31 thru_hole circle (at 57.785 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 86 /SPI1_SCLK))
    (pad B32 thru_hole circle (at 57.785 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 87 /VADC))
    (pad B33 thru_hole circle (at 60.325 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 88 /AIN4))
    (pad B34 thru_hole circle (at 60.325 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 89 /AGND))
    (pad B35 thru_hole circle (at 62.865 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 90 /AIN6))
    (pad B36 thru_hole circle (at 62.865 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 91 /AIN5))
    (pad B37 thru_hole circle (at 65.405 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 92 /AIN2))
    (pad B38 thru_hole circle (at 65.405 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 93 /AIN3))
    (pad B39 thru_hole circle (at 67.945 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 94 /AIN0))
    (pad B40 thru_hole circle (at 67.945 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 95 /AIN1))
    (pad B41 thru_hole circle (at 70.485 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 96 /GPIO_20))
    (pad B42 thru_hole circle (at 70.485 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 97 /ECAPWMO))
    (pad B43 thru_hole circle (at 73.025 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad B44 thru_hole circle (at 73.025 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad B45 thru_hole circle (at 75.565 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad B46 thru_hole circle (at 75.565 -4.445) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad B1 thru_hole rect (at 19.685 -1.905) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
  )
  (module Symbols:Symbol_GNU-Logo_SilkscreenTop (layer B.Cu) (tedit 5691825B)
    (at 145.415 102.9335 180)
    (descr "GNU-Logo, GNU-Head, GNU-Kopf, Silkscreen,")
    (tags "GNU-Logo, GNU-Head, GNU-Kopf, Silkscreen,")
    (fp_text reference REF** (at 0 6.05028 180) (layer B.SilkS) hide)
    (fp_text value Symbol_GNU-Logo_SilkscreenTop (at 0 -9.14908 180) (layer B.Fab))
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 57A793FC)
    (at 122.8725 102.0445 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D5 (at 1.5875 -3.175 90) (layer F.SilkS))
    (fp_text value "RELAY ON" (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D5-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02 (layer F.Cu) (tedit 57AA928E)
    (at 115.824 131.572 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 1.0668 -2.1844 180) (layer F.SilkS) hide)
    (fp_text value JUMPERS (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /A0))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /A1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x02.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 0)
    (at 118.6688 93.5228 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R23 (at 2.54 -0.1016 180) (layer F.SilkS))
    (fp_text value 2k (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /LOCK_RELAYS/R2_READ))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module abracadabra:Panasonic_JW (layer F.Cu) (tedit 57A3CD02)
    (at 152.695 102.175)
    (descr "MINIATURE RELAY DPDT")
    (tags RELAY)
    (attr virtual)
    (fp_text reference RLY1 (at 6.182 0.06) (layer F.SilkS))
    (fp_text value JW2SN-DC5V (at -7.28 -0.067) (layer F.SilkS))
    (pad 1 thru_hole circle (at -14.5 3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 2 thru_hole circle (at 0.5 3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(P8-Pad3)"))
    (pad 3 thru_hole circle (at 5.5 3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D9-Pad1)"))
    (pad 4 thru_hole circle (at 10.5 3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(P8-Pad1)"))
    (pad 5 thru_hole circle (at 10.5 -3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 6 thru_hole circle (at 5.5 -3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(RLY1-Pad6)"))
    (pad 7 thru_hole circle (at 0.5 -3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(RLY1-Pad7)"))
    (pad 8 thru_hole circle (at -14.5 -3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D5-Pad1)"))
    (model ${KIPRJMOD}/packages3d/Panasonic_JW2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module abracadabra:Panasonic_JW (layer F.Cu) (tedit 57A3CD02)
    (at 152.676 116)
    (descr "MINIATURE RELAY DPDT")
    (tags RELAY)
    (attr virtual)
    (fp_text reference RLY2 (at 6.201 -0.557) (layer F.SilkS))
    (fp_text value JW2SN-DC5V (at -7.388 -0.557) (layer F.SilkS))
    (pad 1 thru_hole circle (at -14.5 3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 2 thru_hole circle (at 0.5 3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(P8-Pad3)"))
    (pad 3 thru_hole circle (at 5.5 3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D9-Pad1)"))
    (pad 4 thru_hole circle (at 10.5 3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(RLY2-Pad4)"))
    (pad 5 thru_hole circle (at 10.5 -3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 6 thru_hole circle (at 5.5 -3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(P7-Pad1)"))
    (pad 7 thru_hole circle (at 0.5 -3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(RLY2-Pad7)"))
    (pad 8 thru_hole circle (at -14.5 -3.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D6-Pad1)"))
    (model ${KIPRJMOD}/packages3d/Panasonic_JW2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module abracadabra:V78XX-2000 (layer F.Cu) (tedit 565B1D33)
    (at 147.32 130.81 270)
    (descr "SWITCHING REGULATOR")
    (tags V78XX)
    (fp_text reference U2 (at -5.08 0 360) (layer F.SilkS))
    (fp_text value V7805-2000 (at -2.413 -0.254 360) (layer F.SilkS))
    (pad VI thru_hole circle (at 0 -2.54 270) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad GND thru_hole rect (at 0 0 270) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad VO thru_hole circle (at 0 2.54 270) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (model ${KIPRJMOD}/packages3d/V7805_2000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module abracadabra:BUTTON_MJTP1230 (layer F.Cu) (tedit 57A791AB)
    (at 108.458 93.345 270)
    (fp_text reference SW1 (at 0.25 -4 270) (layer F.SilkS) hide)
    (fp_text value PWR_SWITCH (at 0 4 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.25 -2.25 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 66 /PWR_BUT))
    (pad 2 thru_hole circle (at 3.25 2.25 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 1 thru_hole circle (at -3.25 -2.25 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 66 /PWR_BUT))
    (pad 2 thru_hole circle (at -3.25 2.25 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model ${KIPRJMOD}/packages3d/BUTTON_MJTP1230.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module abracadabra:BUTTON_MJTP1230 (layer F.Cu) (tedit 57A791A4)
    (at 99.568 93.345 270)
    (fp_text reference SW2 (at 0.25 -4 270) (layer F.SilkS) hide)
    (fp_text value RESET_SWITCH (at 0 4 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.25 -2.25 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 67 /SYS_RESETn))
    (pad 2 thru_hole circle (at 3.25 2.25 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 1 thru_hole circle (at -3.25 -2.25 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 67 /SYS_RESETn))
    (pad 2 thru_hole circle (at -3.25 2.25 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model ${KIPRJMOD}/packages3d/BUTTON_MJTP1230.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module abracadabra:TERM_BLOCK_ED2609 (layer F.Cu) (tedit 57AA93F9)
    (at 176.53 133.35 90)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P2 (at 0.2 -4.89 90) (layer F.SilkS) hide)
    (fp_text value 12V (at 0.47 5.19 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0.4 90) (size 2.3 2.3) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 1 thru_hole circle (at -2.54 0.4 90) (size 2.3 2.3) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
  )
  (module abracadabra:TERM_BLOCK_ED2609 (layer F.Cu) (tedit 57A797A6)
    (at 176.53 91.44 90)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P3 (at 0.2 -4.89 90) (layer F.SilkS) hide)
    (fp_text value RED_LIGHT (at 0.47 5.19 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0.4 90) (size 2.3 2.3) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 1 thru_hole circle (at -2.54 0.4 90) (size 2.3 2.3) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D3-Pad1)"))
  )
  (module abracadabra:TERM_BLOCK_ED2609 (layer F.Cu) (tedit 57A7979F)
    (at 176.53 103.505 90)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P5 (at 0.2 -4.89 90) (layer F.SilkS) hide)
    (fp_text value GREEN_LIGHT (at 0.47 5.19 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0.4 90) (size 2.3 2.3) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 1 thru_hole circle (at -2.54 0.4 90) (size 2.3 2.3) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D4-Pad1)"))
  )
  (module abracadabra:TERM_BLOCK_ED2609 (layer F.Cu) (tedit 57AA9349)
    (at 176.53 119.38 90)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P9 (at 0.2 -4.89 90) (layer F.SilkS) hide)
    (fp_text value "DOOR STRIKE/MAGNET" (at 0.47 5.19 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0.4 90) (size 2.3 2.3) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(P7-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 0.4 90) (size 2.3 2.3) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D9-Pad1)"))
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 57A79A09)
    (at 122.809 116.205 270)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D6 (at 1.91 3.06 270) (layer F.SilkS))
    (fp_text value "RELAY ON" (at 1.3 -2.9 270) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(D6-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "DOOR LCK +" (at 176.5808 126.0348) (layer F.SilkS))
  (gr_text "Abracadabra PCB v1.4" (at 103.7844 138.4808) (layer B.SilkS))
  (gr_text "Abracadabra PCB v1.4" (at 103.886 138.4808) (layer F.SilkS))
  (gr_text . (at 134.4676 121.1072) (layer F.SilkS))
  (gr_text . (at 134.5692 104.2416) (layer F.SilkS))
  (gr_text . (at 99.9236 134.0104) (layer F.SilkS))
  (gr_text RLY2 (at 122.8852 120.5992) (layer F.SilkS))
  (gr_text RLY1 (at 122.936 97.7392) (layer F.SilkS))
  (gr_text +12V (at 160.147 123.444) (layer F.SilkS))
  (gr_text +5V (at 134.62 123.698) (layer F.SilkS))
  (gr_text "DOOR LCK -" (at 176.7332 112.8268) (layer F.SilkS))
  (gr_text "- 12V +" (at 171.958 133.477 90) (layer F.SilkS))
  (gr_text "- RED +" (at 171.958 91.059 90) (layer F.SilkS))
  (gr_text "- GREEN +" (at 171.831 102.87 90) (layer F.SilkS))
  (gr_text POWER (at 112.776 93.345 90) (layer F.SilkS))
  (gr_text RESET (at 103.759 93.345 90) (layer F.SilkS))
  (gr_text N/O (at 169.164 123.571) (layer F.SilkS))
  (gr_text "GREEN LIGHT" (at 174.371 103.3145 90) (layer B.SilkS))
  (gr_text "RED LIGHT" (at 174.244 91.5035 90) (layer B.SilkS))
  (gr_text "+      -" (at 179.2605 91.694 90) (layer B.SilkS))
  (gr_text "+      -" (at 179.2605 103.759 90) (layer B.SilkS))
  (gr_text "+      -" (at 179.3875 133.477 90) (layer B.SilkS))
  (gr_text 12V (at 174.3075 133.4135 90) (layer B.SilkS))
  (gr_text "+      -" (at 179.451 119.38 270) (layer B.SilkS))
  (gr_text "DOOR LOCK" (at 174.244 119.4435 90) (layer B.SilkS))
  (gr_text "© R.C., S.W.  2016" (at 103.632 136.8044) (layer B.SilkS))
  (gr_text "© R.C. S.W.  2016" (at 103.4796 136.8044) (layer F.SilkS))
  (gr_text V3 (at 145.288 111.379) (layer B.SilkS))
  (gr_text POWER (at 108.458 98.806 180) (layer F.SilkS))
  (gr_text POWER (at 108.077 88.011) (layer F.SilkS))
  (gr_text RESET (at 99.695 98.806 180) (layer F.SilkS))
  (gr_text RESET (at 99.568 88.011) (layer F.SilkS))
  (gr_text N/C (at 168.9735 113.792) (layer F.SilkS))
  (gr_text A0 (at 118.618 131.699) (layer F.SilkS))
  (gr_text A1 (at 118.6815 128.9685) (layer F.SilkS))
  (gr_text SCL (at 121.4755 109.728) (layer F.SilkS))
  (gr_text SDA (at 121.539 106.9975) (layer F.SilkS))
  (gr_text 3.3V (at 121.793 104.7115) (layer F.SilkS))
  (gr_text N/C (at 121.6025 112.4585) (layer F.SilkS))
  (gr_text GND (at 121.6025 114.554) (layer F.SilkS))
  (gr_line (start 94.488 85.09) (end 94.488 100.965) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.488 85.09) (end 100.203 85.09) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.203 100.965) (end 94.488 100.965) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.488 139.7) (end 94.488 118.745) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.848 139.7) (end 94.488 139.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.848 85.09) (end 180.848 139.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.203 85.09) (end 180.848 85.09) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.808 100.965) (end 100.203 100.965) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.808 118.745) (end 114.808 100.965) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.488 118.745) (end 114.808 118.745) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.488 85.09) (xy 180.848 85.09) (xy 180.848 139.7) (xy 94.488 139.7) (xy 94.488 118.745)
        (xy 114.808 118.745) (xy 114.808 100.965) (xy 94.488 100.965)
      )
    )
  )
)
