(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "D")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 124.99 249.99)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 114.99 249.99)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 311 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 179 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 203 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 213 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 223 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 301 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 159 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 291 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "F.Cu")
    (at 83.99 249.99 -90)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 -4.75 90) (layer "F.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.75 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 270) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 270) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 267 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 134.99 249.99)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 257 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 247 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 169 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:Resistor-link-loop-small" (layer "B.Cu")
    (at 323 250 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Resistor-link-loop" (at -2.54 5.08 270 unlocked) (layer "B.Fab") hide)
    (pad "1" connect roundrect (at 0 6 180) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "2" connect roundrect (at 0 -6) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "3" thru_hole circle (at -2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at -2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" connect roundrect (at -2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "3" thru_hole circle (at -2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" connect roundrect (at 2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "4" thru_hole circle (at 2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:Resistor-link-loop-small" (layer "B.Cu")
    (at 279 250 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Resistor-link-loop" (at -2.54 5.08 270 unlocked) (layer "B.Fab") hide)
    (pad "1" connect roundrect (at 0 6 180) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "2" connect roundrect (at 0 -6) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "3" thru_hole circle (at -2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at -2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" connect roundrect (at -2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "3" thru_hole circle (at -2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" connect roundrect (at 2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "4" thru_hole circle (at 2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 323 282 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 191 238.2 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:Resistor-link-loop-small" (layer "B.Cu")
    (at 235 250 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Resistor-link-loop" (at -2.54 5.08 270 unlocked) (layer "B.Fab") hide)
    (pad "1" connect roundrect (at 0 6 180) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "2" connect roundrect (at 0 -6) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "3" thru_hole circle (at -2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at -2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" connect roundrect (at -2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "3" thru_hole circle (at -2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" connect roundrect (at 2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "4" thru_hole circle (at 2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 279 238.2 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 323 218 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 235 261.8 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 323 238.2 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 147 261.8 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:Resistor-link-loop-small" (layer "B.Cu")
    (at 191 250 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Resistor-link-loop" (at -2.54 5.08 270 unlocked) (layer "B.Fab") hide)
    (pad "1" connect roundrect (at 0 6 180) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "2" connect roundrect (at 0 -6) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "3" thru_hole circle (at -2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at -2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" connect roundrect (at -2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "3" thru_hole circle (at -2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" connect roundrect (at 2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "4" thru_hole circle (at 2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 235 218 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 147 238.2 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 279 218 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 235 282 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 279 261.8 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 235 238.2 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 323 261.8 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 147 282 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 279 282 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 147 218 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 191 282 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 191 218 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:Resistor-link-loop-small" (layer "B.Cu")
    (at 147 250 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Resistor-link-loop" (at -2.54 5.08 270 unlocked) (layer "B.Fab") hide)
    (pad "1" connect roundrect (at 0 6 180) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "2" connect roundrect (at 0 -6) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "3" thru_hole circle (at -2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at -2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" connect roundrect (at -2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "3" thru_hole circle (at -2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" connect roundrect (at 2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "4" thru_hole circle (at 2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 191 261.8 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (gr_arc (start 321.675 247.51) (mid 323 246.185) (end 324.325 247.51)
    (layer "Edge.Cuts"))
  (gr_circle (center 235 250.01) (end 235.01 250.01)
    (fill solid) (layer "Edge.Cuts"))
  (gr_arc (start 326.790019 253.708492) (mid 326.052003 255.056744) (end 324.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_arc (start 192.86 258.268757) (mid 194.423449 259.741184) (end 195 261.81)
    (layer "Edge.Cuts"))
  (gr_line (start 283 261.81) (end 283 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 194.790019 253.708492) (mid 194.052003 255.056744) (end 192.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_arc (start 187.209981 246.311508) (mid 186.847492 246.816698) (end 186.256518 247.01)
    (layer "Edge.Cuts"))
  (gr_line (start 186.256518 253.01) (end 151.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 148.857663 243.995784) (mid 150.052003 244.963256) (end 150.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_arc (start 143.209981 246.311508) (mid 143.947997 244.963256) (end 145.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 231 218.01) (mid 235 214.01) (end 239 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 319 218.01) (mid 323 214.01) (end 327 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 231.209981 246.311508) (mid 231.947997 244.963256) (end 233.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 145.142337 256.024216) (mid 145.531545 256.392221) (end 145.675 256.908295)
    (layer "Edge.Cuts"))
  (gr_line (start 327 261.81) (end 327 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 321.14 241.751243) (mid 321.530878 242.119339) (end 321.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_arc (start 151 238.21) (mid 150.423449 240.278816) (end 148.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_arc (start 236.857663 243.995784) (mid 236.468455 243.627779) (end 236.325 243.111705)
    (layer "Edge.Cuts"))
  (gr_arc (start 236.325 252.51) (mid 235 253.835) (end 233.675 252.51)
    (layer "Edge.Cuts"))
  (gr_line (start 274.256518 253.01) (end 239.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_line (start 189.675 252.51) (end 189.675 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 277.14 241.751243) (mid 275.576551 240.278816) (end 275 238.21)
    (layer "Edge.Cuts"))
  (gr_line (start 231 261.81) (end 231 282.01)
    (layer "Edge.Cuts"))
  (gr_line (start 230.256518 247.01) (end 195.743482 247.01)
    (layer "Edge.Cuts"))
  (gr_line (start 192.325 243.111705) (end 192.325 242.636553)
    (layer "Edge.Cuts"))
  (gr_arc (start 277.675 257.383447) (mid 277.530854 257.900646) (end 277.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_line (start 277.675 256.908295) (end 277.675 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 145.675 243.111705) (mid 145.531543 243.627777) (end 145.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 277.142337 256.024216) (mid 277.531545 256.392221) (end 277.675 256.908295)
    (layer "Edge.Cuts"))
  (gr_arc (start 189.142337 256.024216) (mid 187.947997 255.056744) (end 187.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_arc (start 280.86 258.268757) (mid 282.423449 259.741184) (end 283 261.81)
    (layer "Edge.Cuts"))
  (gr_arc (start 277.675 247.51) (mid 279 246.185) (end 280.325 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 319 261.81) (mid 319.576551 259.741184) (end 321.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_line (start 280.325 256.908295) (end 280.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 192.325 252.51) (mid 191 253.835) (end 189.675 252.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 148.857663 243.995784) (mid 148.468455 243.627779) (end 148.325 243.111705)
    (layer "Edge.Cuts"))
  (gr_arc (start 192.857663 243.995784) (mid 194.052003 244.963256) (end 194.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_arc (start 194.790019 253.708492) (mid 195.152508 253.203302) (end 195.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 239.743482 247.01) (mid 239.152518 246.816685) (end 238.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_arc (start 319.209981 246.311508) (mid 318.847492 246.816698) (end 318.256518 247.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 145.142337 256.024216) (mid 143.947997 255.056744) (end 143.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_line (start 280.325 252.51) (end 280.325 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 187 261.81) (mid 187.576551 259.741184) (end 189.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_arc (start 280.325 256.908295) (mid 280.468457 256.392223) (end 280.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_arc (start 274.256518 253.01) (mid 274.847482 253.203315) (end 275.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_arc (start 189.675 247.51) (mid 191 246.185) (end 192.325 247.51)
    (layer "Edge.Cuts"))
  (gr_line (start 275 261.81) (end 275 282.01)
    (layer "Edge.Cuts"))
  (gr_line (start 239 261.81) (end 239 282.01)
    (layer "Edge.Cuts"))
  (gr_line (start 230.256518 253.01) (end 195.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_line (start 324.325 243.111705) (end 324.325 242.636553)
    (layer "Edge.Cuts"))
  (gr_line (start 148.325 252.51) (end 148.325 247.51)
    (layer "Edge.Cuts"))
  (gr_circle (center 323 250.01) (end 323.01 250.01)
    (fill solid) (layer "Edge.Cuts"))
  (gr_line (start 236.325 256.908295) (end 236.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 236.325 256.908295) (mid 236.468457 256.392223) (end 236.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_arc (start 148.325 242.636553) (mid 148.469114 242.119335) (end 148.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_arc (start 231.209981 246.311508) (mid 230.847492 246.816698) (end 230.256518 247.01)
    (layer "Edge.Cuts"))
  (gr_line (start 186.256518 247.01) (end 151.743482 247.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 236.857663 243.995784) (mid 238.052003 244.963256) (end 238.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_arc (start 275.209981 246.311508) (mid 275.947997 244.963256) (end 277.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 283 282.01) (mid 279 286.01) (end 275 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 192.325 242.636553) (mid 192.469146 242.119354) (end 192.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_arc (start 321.14 241.751243) (mid 319.576551 240.278816) (end 319 238.21)
    (layer "Edge.Cuts"))
  (gr_arc (start 150.790019 253.708492) (mid 150.052003 255.056744) (end 148.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_arc (start 280.857663 243.995784) (mid 282.052003 244.963256) (end 282.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_arc (start 321.675 257.383447) (mid 321.530854 257.900646) (end 321.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_arc (start 275.209981 246.311508) (mid 274.847492 246.816698) (end 274.256518 247.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 283 238.21) (mid 282.423449 240.278816) (end 280.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_arc (start 319.209981 246.311508) (mid 319.947997 244.963256) (end 321.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 187 218.01) (mid 191 214.01) (end 195 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 148.86 258.268757) (mid 150.423449 259.741184) (end 151 261.81)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.325 256.908295) (mid 324.468457 256.392223) (end 324.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_line (start 318.256518 253.01) (end 283.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 192.325 256.908295) (mid 192.468457 256.392223) (end 192.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_line (start 145.675 256.908295) (end 145.675 257.383447)
    (layer "Edge.Cuts"))
  (gr_line (start 192.325 252.51) (end 192.325 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 143 218.01) (mid 147 214.01) (end 151 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.325 242.636553) (mid 324.469146 242.119354) (end 324.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_arc (start 277.14 241.751243) (mid 277.530878 242.119339) (end 277.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_arc (start 318.256518 253.01) (mid 318.847482 253.203315) (end 319.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_arc (start 236.325 242.636553) (mid 236.469146 242.119354) (end 236.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_arc (start 143.209981 246.311508) (mid 142.847492 246.816698) (end 142.256518 247.01)
    (layer "Edge.Cuts"))
  (gr_line (start 324.325 256.908295) (end 324.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_line (start 143 261.81) (end 143 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 280.857663 243.995784) (mid 280.468455 243.627779) (end 280.325 243.111705)
    (layer "Edge.Cuts"))
  (gr_line (start 195 238.21) (end 195 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 283.743482 247.01) (mid 283.152518 246.816685) (end 282.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_arc (start 186.256518 253.01) (mid 186.847482 253.203315) (end 187.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_arc (start 148.325 256.908295) (mid 148.468457 256.392223) (end 148.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_arc (start 233.675 247.51) (mid 235 246.185) (end 236.325 247.51)
    (layer "Edge.Cuts"))
  (gr_line (start 187 238.21) (end 187 218.01)
    (layer "Edge.Cuts"))
  (gr_line (start 142.256518 247.01) (end 87 247.01)
    (layer "Edge.Cuts"))
  (gr_line (start 277.675 252.51) (end 277.675 247.51)
    (layer "Edge.Cuts"))
  (gr_line (start 195 261.81) (end 195 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 192.857663 243.995784) (mid 192.468455 243.627779) (end 192.325 243.111705)
    (layer "Edge.Cuts"))
  (gr_line (start 236.325 243.111705) (end 236.325 242.636553)
    (layer "Edge.Cuts"))
  (gr_line (start 239 238.21) (end 239 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 277.675 243.111705) (mid 277.531543 243.627777) (end 277.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 230.256518 253.01) (mid 230.847482 253.203315) (end 231.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_arc (start 195 282.01) (mid 191 286.01) (end 187 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 233.14 241.751243) (mid 231.576551 240.278816) (end 231 238.21)
    (layer "Edge.Cuts"))
  (gr_arc (start 189.142337 256.024216) (mid 189.531545 256.392221) (end 189.675 256.908295)
    (layer "Edge.Cuts"))
  (gr_line (start 321.675 243.111705) (end 321.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_line (start 280.325 243.111705) (end 280.325 242.636553)
    (layer "Edge.Cuts"))
  (gr_arc (start 195 238.21) (mid 194.423449 240.278816) (end 192.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_line (start 233.675 243.111705) (end 233.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_arc (start 327 282.01) (mid 323 286.01) (end 319 282.01)
    (layer "Edge.Cuts"))
  (gr_line (start 151 261.81) (end 151 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 239 238.21) (mid 238.423449 240.278816) (end 236.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_arc (start 282.790019 253.708492) (mid 283.152508 253.203302) (end 283.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 233.142337 256.024216) (mid 233.531545 256.392221) (end 233.675 256.908295)
    (layer "Edge.Cuts"))
  (gr_arc (start 321.142337 256.024216) (mid 319.947997 255.056744) (end 319.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.857663 243.995784) (mid 326.052003 244.963256) (end 326.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_arc (start 321.675 243.111705) (mid 321.531543 243.627777) (end 321.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_line (start 277.675 243.111705) (end 277.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_arc (start 87 247.01) (mid 86.683772 246.958683) (end 86.4 246.81)
    (layer "Edge.Cuts"))
  (gr_line (start 321.675 252.51) (end 321.675 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 277.142337 256.024216) (mid 275.947997 255.056744) (end 275.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_arc (start 195.743482 247.01) (mid 195.152518 246.816685) (end 194.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_line (start 283 238.21) (end 283 218.01)
    (layer "Edge.Cuts"))
  (gr_line (start 233.675 252.51) (end 233.675 247.51)
    (layer "Edge.Cuts"))
  (gr_line (start 143 238.21) (end 143 218.01)
    (layer "Edge.Cuts"))
  (gr_line (start 151 238.21) (end 151 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 239 282.01) (mid 235 286.01) (end 231 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 189.14 241.751243) (mid 187.576551 240.278816) (end 187 238.21)
    (layer "Edge.Cuts"))
  (gr_line (start 318.256518 247.01) (end 283.743482 247.01)
    (layer "Edge.Cuts"))
  (gr_line (start 187 261.81) (end 187 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 282.790019 253.708492) (mid 282.052003 255.056744) (end 280.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_line (start 189.675 256.908295) (end 189.675 257.383447)
    (layer "Edge.Cuts"))
  (gr_line (start 233.675 256.908295) (end 233.675 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 187.209981 246.311508) (mid 187.947997 244.963256) (end 189.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 145.14 241.751243) (mid 143.576551 240.278816) (end 143 238.21)
    (layer "Edge.Cuts"))
  (gr_line (start 148.325 256.908295) (end 148.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_line (start 275 238.21) (end 275 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 86.4 253.21) (mid 80 250.01) (end 86.4 246.81)
    (layer "Edge.Cuts"))
  (gr_arc (start 233.675 257.383447) (mid 233.530854 257.900646) (end 233.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_line (start 321.675 256.908295) (end 321.675 257.383447)
    (layer "Edge.Cuts"))
  (gr_line (start 274.256518 247.01) (end 239.743482 247.01)
    (layer "Edge.Cuts"))
  (gr_line (start 324.325 252.51) (end 324.325 247.51)
    (layer "Edge.Cuts"))
  (gr_line (start 189.675 243.111705) (end 189.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_line (start 319 261.81) (end 319 282.01)
    (layer "Edge.Cuts"))
  (gr_line (start 236.325 252.51) (end 236.325 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 238.790019 253.708492) (mid 239.152508 253.203302) (end 239.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 238.790019 253.708492) (mid 238.052003 255.056744) (end 236.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_arc (start 280.325 252.51) (mid 279 253.835) (end 277.675 252.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 236.86 258.268757) (mid 238.423449 259.741184) (end 239 261.81)
    (layer "Edge.Cuts"))
  (gr_arc (start 327 238.21) (mid 326.423449 240.278816) (end 324.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_arc (start 142.256518 253.01) (mid 142.847482 253.203315) (end 143.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_arc (start 189.14 241.751243) (mid 189.530878 242.119339) (end 189.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_arc (start 233.14 241.751243) (mid 233.530878 242.119339) (end 233.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_line (start 148.325 243.111705) (end 148.325 242.636553)
    (layer "Edge.Cuts"))
  (gr_arc (start 143 261.81) (mid 143.576551 259.741184) (end 145.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_arc (start 280.325 242.636553) (mid 280.469146 242.119354) (end 280.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.325 252.51) (mid 323 253.835) (end 321.675 252.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 148.325 252.51) (mid 147 253.835) (end 145.675 252.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 236.86 258.268757) (mid 236.469122 257.900661) (end 236.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_line (start 319 238.21) (end 319 218.01)
    (layer "Edge.Cuts"))
  (gr_line (start 231 238.21) (end 231 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 86.4 253.21) (mid 86.683772 253.061317) (end 87 253.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 280.86 258.268757) (mid 280.469122 257.900661) (end 280.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 233.142337 256.024216) (mid 231.947997 255.056744) (end 231.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_arc (start 321.142337 256.024216) (mid 321.531545 256.392221) (end 321.675 256.908295)
    (layer "Edge.Cuts"))
  (gr_arc (start 151.743482 247.01) (mid 151.152518 246.816685) (end 150.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_circle (center 279 250.01) (end 279.01 250.01)
    (fill solid) (layer "Edge.Cuts"))
  (gr_line (start 145.675 243.111705) (end 145.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_circle (center 191 250.01) (end 191.01 250.01)
    (fill solid) (layer "Edge.Cuts"))
  (gr_line (start 145.675 252.51) (end 145.675 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 150.790019 253.708492) (mid 151.152508 253.203302) (end 151.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 145.14 241.751243) (mid 145.530877 242.11934) (end 145.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.857663 243.995784) (mid 324.468455 243.627779) (end 324.325 243.111705)
    (layer "Edge.Cuts"))
  (gr_line (start 192.325 256.908295) (end 192.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 148.86 258.268757) (mid 148.469123 257.90066) (end 148.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 145.675 247.51) (mid 147 246.185) (end 148.325 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 151 282.01) (mid 147 286.01) (end 143 282.01)
    (layer "Edge.Cuts"))
  (gr_line (start 327 238.21) (end 327 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 189.675 243.111705) (mid 189.531543 243.627777) (end 189.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 231 261.81) (mid 231.576551 259.741184) (end 233.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_arc (start 275 261.81) (mid 275.576551 259.741184) (end 277.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.86 258.268757) (mid 324.469122 257.900661) (end 324.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 145.675 257.383447) (mid 145.530841 257.900638) (end 145.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_circle (center 147 250.01) (end 147.01 250.01)
    (fill solid) (layer "Edge.Cuts"))
  (gr_arc (start 192.86 258.268757) (mid 192.469122 257.900661) (end 192.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.86 258.268757) (mid 326.423449 259.741184) (end 327 261.81)
    (layer "Edge.Cuts"))
  (gr_line (start 142.256518 253.01) (end 87 253.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 189.675 257.383447) (mid 189.530854 257.900646) (end 189.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_line (start 326.790019 246.311508) (end 326.790019 253.708492)
    (layer "Edge.Cuts"))
  (gr_arc (start 233.675 243.111705) (mid 233.531543 243.627777) (end 233.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 275 218.01) (mid 279 214.01) (end 283 218.01)
    (layer "Edge.Cuts"))
  (zone (net 0) (net_name "") (layers "*.Mask") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 350 300)
        (xy 350 205)
        (xy 55 205)
        (xy 55 300)
      )
    )
  )
)
