(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g0214c9d)")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 17)
    (zones 0)
    (modules 3)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.048 30)
    (pad_drill 1.524)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF1F)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(P1-Pad3)")
  (net 4 "Net-(P1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
  )
  (module Connectors_JST:JST_PH_S4B-PH-K_04x2.00mm_Angled (layer F.Cu) (tedit 5C581B8B)
    (at 149 66 180)
    (descr "JST PH series connector, S4B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference P1 (at 1.5 -2.45 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 3 7.25 180) (layer F.Fab))
    (fp_text user %R (at 3 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 4 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 6 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad4)"))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S4B-PH-K_04x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module paper:paper (layer F.Cu) (tedit 5C5398A6)
    (at 145.76 101.12)
    (fp_text reference P2 (at 0 0.5) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -0.5) (layer F.Fab))
    (pad 3 thru_hole rect (at 10.84 -15.16) (size 3.048 30) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole rect (at -2.54 -15.24) (size 3.048 30) (drill 1.524) (layers *.Cu *.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 1 thru_hole rect (at -10.16 -15.24) (size 3.048 30) (drill 1.524) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad4)"))
  )
  (module paper:Bela_logo (layer B.Cu) (tedit 0)
    (at 155.067 64.897 135)
    (fp_text reference G*** (at 0 0 135) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 135) (layer B.SilkS) hide)
  )
  (gr_line (start 132 101) (end 160 101) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131 62) (end 131 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 59) (end 134 59) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161 100) (end 161 62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158 62) (end 158 59) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 134 62) (end 131 62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 132 100) (end 132 101) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160 100) (end 161 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text signal (at 156.52 69.24) (layer F.SilkS))
  (gr_text GND (at 143.11 69.35) (layer F.SilkS))
  (gr_text 3v3 (at 135.62 69.24) (layer F.SilkS))
)
