(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(gr_line
		(start 142.24 112.776)
		(end 146.05 112.776)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 125.095 107.315)
		(end 166.878 120.269)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.43 113.157)
		(end 142.24 113.157)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127 118.491)
		(end 165.1 118.491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149.86 112.014)
		(end 153.67 112.014)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.48 111.252)
		(end 161.29 111.252)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.62 113.538)
		(end 138.43 113.538)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.05 112.395)
		(end 149.86 112.395)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.67 111.633)
		(end 157.48 111.633)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127 114.3)
		(end 127 118.491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149.86 112.395)
		(end 149.86 112.014)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.62 113.919)
		(end 134.62 113.538)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.05 112.776)
		(end 146.05 112.395)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.48 111.633)
		(end 157.48 111.252)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.29 110.871)
		(end 165.1 110.871)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.1 110.871)
		(end 165.1 118.491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.67 112.014)
		(end 153.67 111.633)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.24 113.157)
		(end 142.24 112.776)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.29 111.252)
		(end 161.29 110.871)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127 114.3)
		(end 130.81 114.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.81 113.919)
		(end 134.62 113.919)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.43 113.538)
		(end 138.43 113.157)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.81 114.3)
		(end 130.81 113.919)
		(layer "Edge.Cuts")
	)
	(gr_text "SCHLAGE PIN GAUGE"
		(at 150.368 110.744 0)
		(layer "B.SilkS")
	)
	(gr_text "8"
		(at 158.369 110.744 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 139.573 112.649 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 147.066 111.887 0)
		(layer "F.SilkS")
	)
	(gr_text "CUT OUT"
		(at 144.78 116.713 0)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 150.876 111.506 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 135.636 113.03 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 131.826 113.538 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 154.686 111.125 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 143.129 112.268 0)
		(layer "F.SilkS")
	)
	(gr_text "9"
		(at 162.306 110.363 0)
		(layer "F.SilkS")
	)
	(gr_text "0"
		(at 128.016 113.919 0)
		(layer "F.SilkS")
	)
)
