(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6002)
    (drawings 10)
    (tracks 274)
    (zones 0)
    (modules 12)
    (nets 24)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 5.7 5.7)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.25)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 159.9792 119.2974)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAM/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /Anode)
  (net 4 /Din)
  (net 5 /HV6)
  (net 6 /HV5)
  (net 7 /HV10)
  (net 8 /HV4)
  (net 9 /HV9)
  (net 10 /HV3)
  (net 11 /HV8)
  (net 12 /HV2)
  (net 13 /HV7)
  (net 14 /HV1)
  (net 15 "Net-(J2-Pad4)")
  (net 16 "Net-(LED1-Pad2-DO)")
  (net 17 "Net-(LED2-Pad2-DO)")
  (net 18 "Net-(J1-Pad16)")
  (net 19 /DP)
  (net 20 "Net-(J1-Pad4)")
  (net 21 "Net-(J2-Pad16)")
  (net 22 "Net-(NX1-PadP$2)")
  (net 23 "Net-(NX1-PadP$10)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /Anode)
    (add_net /DP)
    (add_net /Din)
    (add_net /HV1)
    (add_net /HV10)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net GND)
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(LED1-Pad2-DO)")
    (add_net "Net-(LED2-Pad2-DO)")
    (add_net "Net-(NX1-PadP$10)")
    (add_net "Net-(NX1-PadP$2)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 5C5B7ED3)
    (at 159.9384 110.9348)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0.0816 4.6352) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 5C5B8F68)
    (at 159.9792 128.7974)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0.0408 4.5526) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 153.6292 131.3624 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AA1E063)
    (at 170.9792 120.5674 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.4 0.05 270) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at -0.4 2 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AA1E05B)
    (at 148.9792 120.5674 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.25 180) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 170.18 101.6 90)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J2 (at 1.27 2.33 90) (layer B.SilkS))
    (fp_text value NL7037 (at 1.27 -22.65 90) (layer B.Fab))
    (fp_text user %R (at 1.27 -10.16) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV6))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV5))
    (pad 6 thru_hole oval (at 2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /DP))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV4))
    (pad 8 thru_hole oval (at 2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV10))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV3))
    (pad 10 thru_hole oval (at 2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV9))
    (pad 11 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV2))
    (pad 12 thru_hole oval (at 2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV8))
    (pad 13 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV1))
    (pad 14 thru_hole oval (at 2.54 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV7))
    (pad 15 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Din))
    (pad 16 thru_hole oval (at 2.54 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad16)"))
    (pad 17 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 18 thru_hole oval (at 2.54 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:adafruit-WS2812B (layer F.Cu) (tedit 5AA1D6C0)
    (at 170.9792 124.3774)
    (attr smd)
    (fp_text reference LED1 (at 3.8989 0.4445 270) (layer F.SilkS))
    (fp_text value WS2812B5050 (at 0 0) (layer F.SilkS) hide)
    (pad 1-VD smd rect (at 2.44856 1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2-DO smd rect (at 2.44856 -1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(LED1-Pad2-DO)"))
    (pad 3-GN smd rect (at -2.44856 -1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4-DI smd rect (at -2.44856 1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 4 /Din))
  )
  (module adafruit:adafruit-WS2812B (layer F.Cu) (tedit 5AA1D6C8)
    (at 148.9792 124.3774)
    (attr smd)
    (fp_text reference LED2 (at 3.8989 0.4445 270) (layer F.SilkS))
    (fp_text value WS2812B5050 (at 0 0) (layer F.SilkS) hide)
    (pad 1-VD smd rect (at 2.44856 1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2-DO smd rect (at 2.44856 -1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(LED2-Pad2-DO)"))
    (pad 3-GN smd rect (at -2.44856 -1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4-DI smd rect (at -2.44856 1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(LED1-Pad2-DO)"))
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 5C5B8F9C)
    (at 175.2192 137.0774 270)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 6.35 2.66 270) (layer B.SilkS) hide)
    (fp_text value 4k7 (at 6.35 -2.66 270) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(NX1-PadP$2)"))
    (pad 2 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 149.86 147.32 270)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J1 (at 1.27 2.33 270) (layer B.SilkS))
    (fp_text value Z568M (at 1.27 -22.65 270) (layer B.Fab))
    (fp_text user %R (at 1.27 -10.16 180) (layer B.Fab))
    (pad 18 thru_hole oval (at 2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 16 thru_hole oval (at 2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Din))
    (pad 14 thru_hole oval (at 2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV7))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV1))
    (pad 12 thru_hole oval (at 2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV8))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV2))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV9))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV3))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV10))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV4))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /DP))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV5))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV6))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer B.Cu) (tedit 5C5B8F87)
    (at 175.2192 98.9774 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 2.31 270) (layer B.SilkS) hide)
    (fp_text value D.P. (at 5.08 -2.31 270) (layer B.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(NX1-PadP$10)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /DP))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module mynixies:mynixies-RTS-5-DUAL-ALLPINS (layer F.Cu) (tedit 5C5F170C)
    (at 160.02 124.46)
    (attr virtual)
    (fp_text reference NX1 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value RTS-5 (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user "NL7037 Front" (at -0.0408 13.8874) (layer F.SilkS))
    (fp_text user "Z568M Front" (at -0.0408 -14.0526 180 unlocked) (layer F.SilkS))
    (pad P$2 thru_hole circle (at 5.97154 16.4084) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Mask)
      (net 22 "Net-(NX1-PadP$2)"))
    (pad P$3 thru_hole circle (at 11.22426 13.37564) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Mask)
      (net 5 /HV6))
    (pad P$4 thru_hole circle (at 15.12062 8.72998) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Mask)
      (net 7 /HV10))
    (pad P$7 thru_hole circle (at 15.12062 -8.72998) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Mask)
      (net 12 /HV2))
    (pad P$8 thru_hole circle (at 11.22426 -13.37564) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Mask)
      (net 8 /HV4))
    (pad P$9 thru_hole circle (at 5.97154 -16.4084) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Mask)
      (net 14 /HV1))
    (pad P$10 thru_hole circle (at 0 -17.4625) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Mask)
      (net 23 "Net-(NX1-PadP$10)"))
    (pad P$12 thru_hole circle (at -11.22426 -13.37564) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Mask)
      (net 11 /HV8))
    (pad P$13 thru_hole circle (at -15.12062 -8.72998) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Mask)
      (net 9 /HV9))
    (pad P$14 thru_hole circle (at -17.1958 -3.03022) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Mask)
      (net 6 /HV5))
    (pad P$16 thru_hole circle (at -15.12062 8.72998) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Mask)
      (net 13 /HV7))
    (pad P$17 thru_hole circle (at -11.22426 13.37564) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Mask)
      (net 10 /HV3))
    (pad "" np_thru_hole circle (at 0 0) (size 10.16 10.16) (drill 10.16) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 17.4625) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 17.1958 3.03022) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 17.1958 -3.03022) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.97154 -16.4084) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -17.1958 3.03022) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
  )
  (dimension 57.15 (width 0.127) (layer Dwgs.User)
    (gr_text "2.2500 in" (at 191.3132 124.3774 270) (layer Dwgs.User))
    (feature1 (pts (xy 189.8242 152.9524) (xy 191.045621 152.9524)))
    (feature2 (pts (xy 189.8242 95.8024) (xy 191.045621 95.8024)))
    (crossbar (pts (xy 190.4592 95.8024) (xy 190.4592 152.9524)))
    (arrow1a (pts (xy 190.4592 152.9524) (xy 189.872779 151.825896)))
    (arrow1b (pts (xy 190.4592 152.9524) (xy 191.045621 151.825896)))
    (arrow2a (pts (xy 190.4592 95.8024) (xy 189.872779 96.928904)))
    (arrow2b (pts (xy 190.4592 95.8024) (xy 191.045621 96.928904)))
  )
  (gr_arc (start 145.3742 100.8824) (end 145.3742 95.8024) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 174.5842 100.8824) (end 179.6642 100.8824) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 145.3742 147.8724) (end 140.2942 147.8724) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 174.5842 147.8724) (end 174.5842 152.9524) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 174.5842 95.8024) (end 145.3742 95.8024) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 179.6642 147.8724) (end 179.6642 100.8824) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 145.3742 152.9524) (end 174.5842 152.9524) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 140.2942 100.8824) (end 140.2942 147.8724) (layer Edge.Cuts) (width 0.127))
  (gr_text "nixies.us\nNL7037, NL934,\nZ568M, R|Z568M" (at 152.3592 130.0924 270) (layer B.Mask))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 192.9992 94.3774) (xy 126.9388 94.2511) (xy 126.9796 153.2337) (xy 193.04 153.36)
      )
    )
  )
)
