(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "Encoder Readout Board")
		(date "2024-05-23")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(ENC1-A)")
	(net 2 "Net-(ENC1-B)")
	(net 3 "Net-(ENC1-Idx)")
	(net 4 "Net-(ENC2-Idx)")
	(net 5 "Net-(ENC2-B)")
	(net 6 "Net-(ENC2-A)")
	(net 7 "+5V")
	(net 8 "GND")
	(net 9 "Net-(ENC3-Idx)")
	(net 10 "Net-(ENC3-A)")
	(net 11 "Net-(ENC3-B)")
	(net 12 "Net-(ENC4-B)")
	(net 13 "Net-(ENC4-A)")
	(net 14 "Net-(ENC4-Idx)")
	(net 15 "Net-(ENC5-B)")
	(net 16 "Net-(ENC5-A)")
	(net 17 "Net-(ENC5-Idx)")
	(net 18 "Net-(ENC6-Idx)")
	(net 19 "Net-(ENC6-A)")
	(net 20 "Net-(ENC6-B)")
	(net 21 "Net-(ENC7-B)")
	(net 22 "Net-(ENC7-A)")
	(net 23 "Net-(ENC7-Idx)")
	(net 24 "Net-(ENC8-A)")
	(net 25 "Net-(ENC8-B)")
	(net 26 "Net-(ENC8-Idx)")
	(net 27 "Net-(U1-B1)")
	(net 28 "Net-(U1-B2)")
	(net 29 "Net-(U1-B4)")
	(net 30 "Net-(U1-B6)")
	(net 31 "Net-(U1-B5)")
	(net 32 "Net-(U1-B3)")
	(net 33 "Net-(U2-B2)")
	(net 34 "Net-(U2-B6)")
	(net 35 "Net-(U2-B3)")
	(net 36 "Net-(U2-B1)")
	(net 37 "Net-(U2-B4)")
	(net 38 "Net-(U2-B5)")
	(net 39 "Net-(U3-A4)")
	(net 40 "Net-(U3-A5)")
	(net 41 "Net-(U3-A3)")
	(net 42 "Net-(U3-A6)")
	(net 43 "Net-(U3-A2)")
	(net 44 "Net-(U3-A1)")
	(net 45 "Net-(U4-A6)")
	(net 46 "Net-(U4-A4)")
	(net 47 "Net-(U4-A5)")
	(net 48 "Net-(U4-A1)")
	(net 49 "Net-(U4-A3)")
	(net 50 "Net-(U4-A2)")
	(net 51 "+3.3V")
	(net 52 "unconnected-(U1-B8-Pad14)")
	(net 53 "unconnected-(U1-B7-Pad15)")
	(net 54 "unconnected-(U2-B7-Pad15)")
	(net 55 "unconnected-(U2-B8-Pad14)")
	(net 56 "unconnected-(U3-A7-Pad9)")
	(net 57 "unconnected-(U3-A8-Pad10)")
	(net 58 "unconnected-(U4-A8-Pad10)")
	(net 59 "unconnected-(U4-A7-Pad9)")
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 67.564 131.572 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at -0.508 3.429 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 84.914 101.092)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -0.078 -1.778 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 96.52 104.14)
		(descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x03 2.54mm double row")
		(property "Reference" "ENCOUT1"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 1.27 7.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(U1-B1)")
			(pinfunction "1")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(U1-B6)")
			(pinfunction "2")
			(pintype "output")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(U1-B2)")
			(pinfunction "3")
			(pintype "output")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(U1-B5)")
			(pinfunction "4")
			(pintype "output")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(U1-B3)")
			(pinfunction "5")
			(pintype "output")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(U1-B4)")
			(pinfunction "6")
			(pintype "output")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 73.66 124.46)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "ENC7"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(ENC7-A)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(ENC7-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(ENC7-Idx)")
			(pinfunction "Idx")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 99.06 149.86)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01"
			(at 0 2.33 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 53.34 104.14)
		(descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x03 2.54mm double row")
		(property "Reference" "ENCOUT3"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 1.27 7.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(U3-A6)")
			(pinfunction "1")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(U3-A1)")
			(pinfunction "2")
			(pintype "output")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(U3-A5)")
			(pinfunction "3")
			(pintype "output")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(U3-A2)")
			(pinfunction "4")
			(pintype "output")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(U3-A4)")
			(pinfunction "5")
			(pintype "output")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(U3-A3)")
			(pinfunction "6")
			(pintype "output")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 84.836 131.445)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "encoder_library:SOP65P640X120-24N"
		(layer "F.Cu")
		(at 65.913 106.68)
		(property "Reference" "U3"
			(at -1.651 -5.085 0)
			(layer "F.SilkS")
		)
		(property "Value" "SN74LVC8T245"
			(at 6.89 7.625 0)
			(layer "F.Fab")
		)
		(property "Footprint" "encoder_library:SOP65P640X120-24N"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc8t245.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*5.3x8.2mm* SSOP*3.9x8.7mm* TSSOP*4.4x7.8mm* TVSOP*4.4x5.0mm* Texas*VQFN*RHL*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -2.87 -3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 51 "+3.3V")
			(pinfunction "V_{CCA}")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -2.87 -2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "DIR")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -2.87 -2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 44 "Net-(U3-A1)")
			(pinfunction "A1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at -2.87 -1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 43 "Net-(U3-A2)")
			(pinfunction "A2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at -2.87 -0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 41 "Net-(U3-A3)")
			(pinfunction "A3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd roundrect
			(at -2.87 -0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 39 "Net-(U3-A4)")
			(pinfunction "A4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd roundrect
			(at -2.87 0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 40 "Net-(U3-A5)")
			(pinfunction "A5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd roundrect
			(at -2.87 0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 42 "Net-(U3-A6)")
			(pinfunction "A6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd roundrect
			(at -2.87 1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 56 "unconnected-(U3-A7-Pad9)")
			(pinfunction "A7")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd roundrect
			(at -2.87 2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 57 "unconnected-(U3-A8-Pad10)")
			(pinfunction "A8")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd roundrect
			(at -2.87 2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd roundrect
			(at -2.87 3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd roundrect
			(at 2.87 3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd roundrect
			(at 2.87 2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "B8")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd roundrect
			(at 2.87 2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "B7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd roundrect
			(at 2.87 1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 18 "Net-(ENC6-Idx)")
			(pinfunction "B6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd roundrect
			(at 2.87 0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 20 "Net-(ENC6-B)")
			(pinfunction "B5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd roundrect
			(at 2.87 0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 19 "Net-(ENC6-A)")
			(pinfunction "B4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "19" smd roundrect
			(at 2.87 -0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 17 "Net-(ENC5-Idx)")
			(pinfunction "B3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "20" smd roundrect
			(at 2.87 -0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 15 "Net-(ENC5-B)")
			(pinfunction "B2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "21" smd roundrect
			(at 2.87 -1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 16 "Net-(ENC5-A)")
			(pinfunction "B1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "22" smd roundrect
			(at 2.87 -2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "23" smd roundrect
			(at 2.87 -2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 7 "+5V")
			(pinfunction "V_{CCB}")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "24" smd roundrect
			(at 2.87 -3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 7 "+5V")
			(pinfunction "V_{CCB}")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 92.71 144.145 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.85 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 8 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 51 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 68.58 118.364 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 78.74 124.46)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "ENC3"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(ENC3-A)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(ENC3-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(ENC3-Idx)")
			(pinfunction "Idx")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 73.66 139.7)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "ENC8"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(ENC8-A)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(ENC8-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(ENC8-Idx)")
			(pinfunction "Idx")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 67.437 101.092 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 78.74 93.98)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "ENC1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(ENC1-A)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(ENC1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(ENC1-Idx)")
			(pinfunction "Idx")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 83.82 148.59 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at -3.175 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "encoder_library:SOP65P640X120-24N"
		(layer "F.Cu")
		(at 86.36 106.68)
		(property "Reference" "U1"
			(at 1.905 -4.953 0)
			(layer "F.SilkS")
		)
		(property "Value" "SN74LVC8T245"
			(at 6.89 5.085 0)
			(layer "F.Fab")
		)
		(property "Footprint" "encoder_library:SOP65P640X120-24N"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc8t245.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*5.3x8.2mm* SSOP*3.9x8.7mm* TSSOP*4.4x7.8mm* TVSOP*4.4x5.0mm* Texas*VQFN*RHL*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -2.87 -3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 7 "+5V")
			(pinfunction "V_{CCA}")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -2.87 -2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 7 "+5V")
			(pinfunction "DIR")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -2.87 -2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 1 "Net-(ENC1-A)")
			(pinfunction "A1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at -2.87 -1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 2 "Net-(ENC1-B)")
			(pinfunction "A2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at -2.87 -0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 3 "Net-(ENC1-Idx)")
			(pinfunction "A3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd roundrect
			(at -2.87 -0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 6 "Net-(ENC2-A)")
			(pinfunction "A4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd roundrect
			(at -2.87 0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 5 "Net-(ENC2-B)")
			(pinfunction "A5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd roundrect
			(at -2.87 0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 4 "Net-(ENC2-Idx)")
			(pinfunction "A6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd roundrect
			(at -2.87 1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "A7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd roundrect
			(at -2.87 2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "A8")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd roundrect
			(at -2.87 2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd roundrect
			(at -2.87 3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd roundrect
			(at 2.87 3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd roundrect
			(at 2.87 2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 52 "unconnected-(U1-B8-Pad14)")
			(pinfunction "B8")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd roundrect
			(at 2.87 2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 53 "unconnected-(U1-B7-Pad15)")
			(pinfunction "B7")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd roundrect
			(at 2.87 1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 30 "Net-(U1-B6)")
			(pinfunction "B6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd roundrect
			(at 2.87 0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 31 "Net-(U1-B5)")
			(pinfunction "B5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd roundrect
			(at 2.87 0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 29 "Net-(U1-B4)")
			(pinfunction "B4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "19" smd roundrect
			(at 2.87 -0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 32 "Net-(U1-B3)")
			(pinfunction "B3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "20" smd roundrect
			(at 2.87 -0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 28 "Net-(U1-B2)")
			(pinfunction "B2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "21" smd roundrect
			(at 2.87 -1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 27 "Net-(U1-B1)")
			(pinfunction "B1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "22" smd roundrect
			(at 2.87 -2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "23" smd roundrect
			(at 2.87 -2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 51 "+3.3V")
			(pinfunction "V_{CCB}")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "24" smd roundrect
			(at 2.87 -3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 51 "+3.3V")
			(pinfunction "V_{CCB}")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 83.82 118.364 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 78.74 109.22)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "ENC2"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(ENC2-A)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(ENC2-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(ENC2-Idx)")
			(pinfunction "Idx")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 78.74 139.7)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "ENC4"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(ENC4-A)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(ENC4-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(ENC4-Idx)")
			(pinfunction "Idx")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 68.58 148.59 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at -3.302 -0.381 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 83.82 91.694 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.33 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at -6.985 4.87 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "encoder_library:SOP65P640X120-24N"
		(layer "F.Cu")
		(at 66.04 137.16)
		(property "Reference" "U4"
			(at -1.778 -5.08 0)
			(layer "F.SilkS")
		)
		(property "Value" "SN74LVC8T245"
			(at -0.94 -1.03 0)
			(layer "F.Fab")
		)
		(property "Footprint" "encoder_library:SOP65P640X120-24N"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc8t245.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*5.3x8.2mm* SSOP*3.9x8.7mm* TSSOP*4.4x7.8mm* TVSOP*4.4x5.0mm* Texas*VQFN*RHL*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -2.87 -3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 51 "+3.3V")
			(pinfunction "V_{CCA}")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -2.87 -2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "DIR")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -2.87 -2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 48 "Net-(U4-A1)")
			(pinfunction "A1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at -2.87 -1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 50 "Net-(U4-A2)")
			(pinfunction "A2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at -2.87 -0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 49 "Net-(U4-A3)")
			(pinfunction "A3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd roundrect
			(at -2.87 -0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 46 "Net-(U4-A4)")
			(pinfunction "A4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd roundrect
			(at -2.87 0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 47 "Net-(U4-A5)")
			(pinfunction "A5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd roundrect
			(at -2.87 0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 45 "Net-(U4-A6)")
			(pinfunction "A6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd roundrect
			(at -2.87 1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 59 "unconnected-(U4-A7-Pad9)")
			(pinfunction "A7")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd roundrect
			(at -2.87 2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 58 "unconnected-(U4-A8-Pad10)")
			(pinfunction "A8")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd roundrect
			(at -2.87 2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd roundrect
			(at -2.87 3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd roundrect
			(at 2.87 3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd roundrect
			(at 2.87 2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "B8")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd roundrect
			(at 2.87 2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "B7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd roundrect
			(at 2.87 1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 26 "Net-(ENC8-Idx)")
			(pinfunction "B6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd roundrect
			(at 2.87 0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 25 "Net-(ENC8-B)")
			(pinfunction "B5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd roundrect
			(at 2.87 0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 24 "Net-(ENC8-A)")
			(pinfunction "B4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "19" smd roundrect
			(at 2.87 -0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 23 "Net-(ENC7-Idx)")
			(pinfunction "B3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "20" smd roundrect
			(at 2.87 -0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 21 "Net-(ENC7-B)")
			(pinfunction "B2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "21" smd roundrect
			(at 2.87 -1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 22 "Net-(ENC7-A)")
			(pinfunction "B1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "22" smd roundrect
			(at 2.87 -2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "23" smd roundrect
			(at 2.87 -2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 7 "+5V")
			(pinfunction "V_{CCB}")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "24" smd roundrect
			(at 2.87 -3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 7 "+5V")
			(pinfunction "V_{CCB}")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 53.34 119.38)
		(descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x03 2.54mm double row")
		(property "Reference" "ENCOUT4"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 1.27 7.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(U4-A6)")
			(pinfunction "1")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(U4-A1)")
			(pinfunction "2")
			(pintype "output")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(U4-A5)")
			(pinfunction "3")
			(pintype "output")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(U4-A2)")
			(pinfunction "4")
			(pintype "output")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(U4-A4)")
			(pinfunction "5")
			(pintype "output")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(U4-A3)")
			(pinfunction "6")
			(pintype "output")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 96.52 119.38)
		(descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x03 2.54mm double row")
		(property "Reference" "ENCOUT2"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 1.27 7.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(U2-B1)")
			(pinfunction "1")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(U2-B6)")
			(pinfunction "2")
			(pintype "output")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(U2-B2)")
			(pinfunction "3")
			(pintype "output")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(U2-B5)")
			(pinfunction "4")
			(pintype "output")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(U2-B3)")
			(pinfunction "5")
			(pintype "output")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(U2-B4)")
			(pinfunction "6")
			(pintype "output")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "encoder_library:SOP65P640X120-24N"
		(layer "F.Cu")
		(at 86.36 137.16)
		(property "Reference" "U2"
			(at 2.413 -5.207 0)
			(layer "F.SilkS")
		)
		(property "Value" "SN74LVC8T245"
			(at 6.89 5.085 0)
			(layer "F.Fab")
		)
		(property "Footprint" "encoder_library:SOP65P640X120-24N"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc8t245.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*5.3x8.2mm* SSOP*3.9x8.7mm* TSSOP*4.4x7.8mm* TVSOP*4.4x5.0mm* Texas*VQFN*RHL*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -2.87 -3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 7 "+5V")
			(pinfunction "V_{CCA}")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -2.87 -2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 7 "+5V")
			(pinfunction "DIR")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -2.87 -2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 10 "Net-(ENC3-A)")
			(pinfunction "A1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at -2.87 -1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 11 "Net-(ENC3-B)")
			(pinfunction "A2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at -2.87 -0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 9 "Net-(ENC3-Idx)")
			(pinfunction "A3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd roundrect
			(at -2.87 -0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 13 "Net-(ENC4-A)")
			(pinfunction "A4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd roundrect
			(at -2.87 0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 12 "Net-(ENC4-B)")
			(pinfunction "A5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd roundrect
			(at -2.87 0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 14 "Net-(ENC4-Idx)")
			(pinfunction "A6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd roundrect
			(at -2.87 1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "A7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd roundrect
			(at -2.87 2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "A8")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd roundrect
			(at -2.87 2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd roundrect
			(at -2.87 3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd roundrect
			(at 2.87 3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd roundrect
			(at 2.87 2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 55 "unconnected-(U2-B8-Pad14)")
			(pinfunction "B8")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd roundrect
			(at 2.87 2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 54 "unconnected-(U2-B7-Pad15)")
			(pinfunction "B7")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd roundrect
			(at 2.87 1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 34 "Net-(U2-B6)")
			(pinfunction "B6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd roundrect
			(at 2.87 0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 38 "Net-(U2-B5)")
			(pinfunction "B5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd roundrect
			(at 2.87 0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 37 "Net-(U2-B4)")
			(pinfunction "B4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "19" smd roundrect
			(at 2.87 -0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 35 "Net-(U2-B3)")
			(pinfunction "B3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "20" smd roundrect
			(at 2.87 -0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 33 "Net-(U2-B2)")
			(pinfunction "B2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "21" smd roundrect
			(at 2.87 -1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 36 "Net-(U2-B1)")
			(pinfunction "B1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "22" smd roundrect
			(at 2.87 -2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 8 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "23" smd roundrect
			(at 2.87 -2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 51 "+3.3V")
			(pinfunction "V_{CCB}")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "24" smd roundrect
			(at 2.87 -3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.125)
			(net 51 "+3.3V")
			(pinfunction "V_{CCB}")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 96.52 144.145 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 8 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 51 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 99.06 139.7)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01"
			(at 0 2.33 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 73.66 109.22)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "ENC6"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(ENC6-A)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(ENC6-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(ENC6-Idx)")
			(pinfunction "Idx")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 73.66 93.98)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "ENC5"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "encoder_converter_x8.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(ENC5-A)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(ENC5-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(ENC5-Idx)")
			(pinfunction "Idx")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 50.8 88.9)
		(end 101.6 152.4)
		(fill none)
		(layer "Edge.Cuts")
	)
)
