(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 29)
    (tracks 301)
    (zones 0)
    (modules 19)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.41)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.01)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.2)
    (via_min_drill 0.254)
    (user_via 0.51 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.8 0.8)
    (pad_drill 0.5)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 PAEN)
  (net 3 VBIAS)
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net PAEN)
    (add_net VBIAS)
  )
  (module baum_rf:SMA_Samtec_SMA-J-P-H-ST-EM1_EdgeMount (layer F.Cu) (tedit 5C671C25)
    (at 117 85 180)
    (descr http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)
    (tags SMA)
    (attr smd)
    (fp_text reference J1 (at -3.5 0 270) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at 5 5.9 180) (layer F.Fab))
    (fp_text user "PCB Edge" (at 2.6 0 270) (layer Dwgs.User))
    (fp_text user %R (at 4.79 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.2 0 270) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0 -2.825 270) (size 1.35 4.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 2.825 270) (size 1.35 4.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -2.825 270) (size 1.35 4.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 2.825 270) (size 1.35 4.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/MMCX_Molex_73415-0961_Horizontal.step
      (offset (xyz 2.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module baum_rf:SMA_Samtec_SMA-J-P-H-ST-EM1_EdgeMount (layer F.Cu) (tedit 5C6726C4)
    (at 138 86.75)
    (descr http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)
    (tags SMA)
    (attr smd)
    (fp_text reference J2 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at 5 5.9) (layer F.Fab) hide)
    (fp_text user "PCB Edge" (at 2.6 0 90) (layer Dwgs.User))
    (fp_text user %R (at 4.79 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0.2 0 90) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 0 -2.825 90) (size 1.35 4.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 2.825 90) (size 1.35 4.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -2.825 90) (size 1.35 4.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 2.825 90) (size 1.35 4.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/MMCX_Molex_73415-0961_Horizontal.step
      (offset (xyz 2.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module baum_rf:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C648CBC)
    (at 137.5 71.5 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (attr smd)
    (fp_text reference J3 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 smd roundrect (at 0 5 270) (size 4 4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 6 "Net-(J3-Pad2)"))
    (pad 1 smd roundrect (at 0 0 270) (size 4 4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 2 PAEN))
  )
  (module baum_rf:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C671BED)
    (at 123 71.5 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (attr smd)
    (fp_text reference J4 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 smd roundrect (at 0 5 270) (size 4 4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 1 GND))
    (pad 1 smd roundrect (at 0 0 270) (size 4 4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 3 VBIAS))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_Pad_Via (layer F.Cu) (tedit 5C648653)
    (at 137 78.5)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7 90) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_Pad_Via (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module baum_rf:QFN-16_EP_5.3x5.3_Pitch0.8mm (layer F.Cu) (tedit 5C671BC8)
    (at 126.5675 85.5225)
    (attr smd)
    (fp_text reference U1 (at 0 -3.985) (layer F.SilkS) hide)
    (fp_text value SKY66295 (at 0 3.985) (layer F.Fab))
    (pad 1 smd rect (at -2.315 -1.2 90) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.315 -0.4 90) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 3 smd rect (at -2.315 0.4 90) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.315 1.2 90) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -1.2 2.315) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 3 VBIAS))
    (pad 6 smd rect (at -0.4 2.315) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 2 PAEN))
    (pad 7 smd rect (at 0.4 2.315) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 1.2 2.315) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 2.315 1.2 90) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 10 smd rect (at 2.315 0.4 90) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 2.315 -0.4 90) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 2.315 -1.2 90) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 3 VBIAS))
    (pad 13 smd rect (at 1.2 -2.315) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 0.4 -2.315) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 3 VBIAS))
    (pad 15 smd rect (at -0.4 -2.315) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -1.2 -2.315) (size 0.5 0.67) (layers F.Cu F.Paste F.Mask)
      (net 3 VBIAS))
    (pad 17 smd rect (at -1.2975 -1.2975) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at -1.2975 -0.4325) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at -1.2975 0.4325) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at -1.2975 1.2975) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at -0.4325 -1.2975) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at -0.4325 -0.4325) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at -0.4325 0.4325) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at -0.4325 1.2975) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at 0.4325 -1.2975) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at 0.4325 -0.4325) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at 0.4325 0.4325) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at 0.4325 1.2975) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at 1.2975 -1.2975) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at 1.2975 -0.4325) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at 1.2975 0.4325) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 smd rect (at 1.2975 1.2975) (size 0.865 0.865) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.1))
    (pad 17 thru_hole circle (at -1.2975 -1.2975) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at -1.2975 -0.4325) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at -1.2975 0.4325) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at -1.2975 1.2975) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at -0.4325 -1.2975) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at -0.4325 -0.4325) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at -0.4325 0.4325) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at -0.4325 1.2975) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0.4325 -1.2975) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0.4325 -0.4325) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0.4325 0.4325) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0.4325 1.2975) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 1.2975 -1.2975) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 1.2975 -0.4325) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 1.2975 0.4325) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 1.2975 1.2975) (size 0.4325 0.4325) (drill 0.21625) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_4x4mm_Pitch0.65mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.2 1.2 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 128 91.875 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at -2.275 0) (layer F.SilkS))
    (fp_text value 3.3n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 PAEN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 125.5 91.875 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at -2.275 0.1) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBIAS))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 132.814725 82.91669)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -2.514725 -0.01669) (layer F.SilkS))
    (fp_text value 100p (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBIAS))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 132.814725 80.91669)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -2.514725 -0.01669) (layer F.SilkS))
    (fp_text value 3.3n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBIAS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 132.5 76.5 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0.1 -1.7 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 VBIAS))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 128.51 80)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 -1.21) (layer F.SilkS))
    (fp_text value 3.3n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBIAS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 127.4875 77)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0.1125 -1.6) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 VBIAS))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 124.875 80.01)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 0 -1.285) (layer F.SilkS))
    (fp_text value 3.3n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBIAS))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 121.5125 77 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at 0 -1.8 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 VBIAS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 127 71.875 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 2.125 0) (layer F.SilkS))
    (fp_text value 15k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(J3-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBIAS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5C632CDC)
    (at 129 71.875 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -2.125 0.3 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(J3-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_Pad_Via (layer F.Cu) (tedit 5C6726BF)
    (at 121.5 91)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (attr virtual)
    (fp_text reference REF** (at -0.19 6.42) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_Pad_Via (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 130.5 91.875 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -2.075 0.1) (layer F.SilkS))
    (fp_text value 200k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 PAEN))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 115.2 93.8) (end 115 93.8) (angle -90) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 139.8 93.8) (end 139.8 94) (angle -90) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 139.8 69.2) (end 140 69.2) (angle -90) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 115.2 69.2) (end 115.2 69) (angle -90) (layer Edge.Cuts) (width 0.01))
  (gr_text 5V (at 123 74.6) (layer F.SilkS))
  (gr_text GND (at 118 74.6) (layer F.SilkS))
  (gr_text ENABLE (at 136.4 74.4) (layer F.SilkS))
  (gr_text DB4UM (at 116.6 91.6 270) (layer F.SilkS))
  (gr_text OUT (at 137.6 82.4) (layer F.SilkS))
  (gr_text IN (at 116.6 80.2) (layer F.SilkS))
  (gr_text "2W\n35dB\n2.4GHz\n" (at 132.2 91.6) (layer F.SilkS))
  (gr_line (start 139.8 94) (end 115.2 94) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 140 69.2) (end 140 93.8) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 115.2 69) (end 139.8 69) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 115 93.8) (end 115 69.2) (layer Edge.Cuts) (width 0.01))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124 86.47) (xy 124 86.16) (xy 123.92 85.68) (xy 123.4 86.4) (xy 119.5 86.4)
        (xy 119.1 87.15) (xy 117.3 88.48) (xy 124 88.48)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.9 84.375) (xy 117.975 85.625) (xy 118.6 85.63) (xy 119.42 85.32) (xy 119.42 84.92)
        (xy 118.6 84.37)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115 81.6) (xy 119.1 82.85) (xy 119.5 83.8) (xy 123.4 83.8) (xy 123.92 84.57)
        (xy 125 82.6) (xy 122.11 80.9) (xy 119.09 80.9) (xy 115 80.9)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.9 88.9) (xy 135.5 87.99) (xy 129.3 88) (xy 129 87.6) (xy 128 87.6)
        (xy 128 88.5) (xy 128 89.3) (xy 131.31 90.25) (xy 135.9 90.25) (xy 135.9 90.21)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.21 84.88) (xy 129.21 85.67) (xy 129.21 86.17) (xy 129.71 85.42) (xy 135.5 85.42)
        (xy 135.9 84.6) (xy 135.91 83.26) (xy 135.36 83.72) (xy 131.02 83.72)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115 69) (xy 115 82.5) (xy 140 82.5) (xy 140 69)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140 94) (xy 140 89) (xy 115 89) (xy 115 94)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115 94) (xy 115 88.5) (xy 115 88.2) (xy 128 88.2) (xy 128 94)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120 83.5) (xy 120.5 80) (xy 140 80.5) (xy 139.5 84.5) (xy 130.5 84.5)
        (xy 129 85) (xy 124.5 84.5) (xy 123.5 83.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115 69) (xy 115 94) (xy 140 94) (xy 140 69)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115 69) (xy 115 94) (xy 140 94) (xy 140 69)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115 69) (xy 115 94) (xy 140 94) (xy 140 69)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115 88.3) (xy 115 89.2) (xy 121.5 89.2) (xy 121.5 88.3)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140 90.2) (xy 140 91.2) (xy 135.2 91.2) (xy 135.2 90.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140 83.3) (xy 140 81.9) (xy 135.3 82) (xy 135.3 83.7)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.95 87.37) (xy 136.68 86.12) (xy 136.4 86.12) (xy 135.6 86.52) (xy 135.6 86.92)
        (xy 136.4 87.38)
      )
    )
  )
)
