(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4~bpo8+1)
  (general
    (links 36)
    (no_connects 0)
    (area 166.802999 51.486999 192.861001 82.625001)
    (thickness 1.6)
    (drawings 30)
    (tracks 82)
    (zones 0)
    (modules 20)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2352 2.2352)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 141.986 109.982)
    (grid_origin 141.986 109.982)
    (visible_elements FFFEDE7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 VCC_IN)
  (net 2 GND)
  (net 3 INT)
  (net 4 RST)
  (net 5 "Net-(R1-Pad1)")
  (net 6 LED1)
  (net 7 "Net-(R2-Pad1)")
  (net 8 LED2)
  (net 9 SW1)
  (net 10 SW2)
  (net 11 SCL)
  (net 12 SDA)
  (net 13 "Net-(IC1-Pad2)")
  (net 14 "Net-(IC1-Pad3)")
  (net 15 "Net-(IC1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad4)")
  )
  (net_class DATA ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net INT)
    (add_net LED1)
    (add_net LED2)
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net RST)
    (add_net SCL)
    (add_net SDA)
    (add_net SW1)
    (add_net SW2)
  )
  (net_class PWR ""
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC_IN)
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58F218CD)
    (at 190.5 53.848)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58F218CD)
    (at 169.164 53.848)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58F218CD)
    (at 169.418 80.01)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module n39-SWITCH_SRKL_LED (layer B.Cu) (tedit 58CDB319)
    (at 186.182 67.31 180)
    (descr SWITCH)
    (tags SWITCH)
    (attr virtual)
    (fp_text reference S1 (at 0.127 10.033 180) (layer B.SilkS))
    (fp_text value n39-SWITCH_SRKL_LED (at -0.635 -2.794 180) (layer B.SilkS) hide)
    (pad + thru_hole oval (at -1.27 5.08) (size 1.3208 2.6416) (drill 0.8128) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(R1-Pad1)"))
    (pad - thru_hole oval (at 1.27 5.08) (size 1.3208 2.6416) (drill 0.8128) (layers *.Cu *.Paste *.Mask)
      (net 2 GND))
    (pad 1 thru_hole oval (at -3.81 -5.08) (size 1.3208 2.6416) (drill 0.8128) (layers *.Cu *.Paste *.Mask)
      (net 9 SW1))
    (pad 2 thru_hole oval (at -3.81 0) (size 1.3208 2.6416) (drill 0.8128) (layers *.Cu *.Paste *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 3.81 0) (size 1.3208 2.6416) (drill 0.8128) (layers *.Cu *.Paste *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 3.81 -5.08) (size 1.3208 2.6416) (drill 0.8128) (layers *.Cu *.Paste *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 3.81 7.62 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu)
      (zone_connect 0))
    (pad "" np_thru_hole circle (at -3.81 -7.62 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu)
      (zone_connect 0))
  )
  (module n39-SWITCH_SRKL_LED (layer B.Cu) (tedit 58CDB317)
    (at 173.482 67.31 180)
    (descr SWITCH)
    (tags SWITCH)
    (attr virtual)
    (fp_text reference S2 (at 0.127 10.033 180) (layer B.SilkS))
    (fp_text value n39-SWITCH_SRKL_LED (at -0.635 -2.794 180) (layer B.SilkS) hide)
    (pad + thru_hole oval (at -1.27 5.08) (size 1.3208 2.6416) (drill 0.8128) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(R2-Pad1)"))
    (pad - thru_hole oval (at 1.27 5.08) (size 1.3208 2.6416) (drill 0.8128) (layers *.Cu *.Paste *.Mask)
      (net 2 GND))
    (pad 1 thru_hole oval (at -3.81 -5.08) (size 1.3208 2.6416) (drill 0.8128) (layers *.Cu *.Paste *.Mask)
      (net 10 SW2))
    (pad 2 thru_hole oval (at -3.81 0) (size 1.3208 2.6416) (drill 0.8128) (layers *.Cu *.Paste *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 3.81 0) (size 1.3208 2.6416) (drill 0.8128) (layers *.Cu *.Paste *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 3.81 -5.08) (size 1.3208 2.6416) (drill 0.8128) (layers *.Cu *.Paste *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 3.81 7.62 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu)
      (zone_connect 0))
    (pad "" np_thru_hole circle (at -3.81 -7.62 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu)
      (zone_connect 0))
  )
  (module Housings_DFN_QFN:QFN-20-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 58F21D85)
    (at 186.182 69.85 135)
    (descr "20-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference IC1 (at 3.412497 1.257236 225) (layer F.SilkS))
    (fp_text value ATTINY84-M (at 0 3.33 135) (layer F.Fab))
    (pad 1 smd rect (at -1.965 -1 135) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 SCL))
    (pad 2 smd rect (at -1.965 -0.5 135) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -1.965 0 135) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at -1.965 0.5 135) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad4)"))
    (pad 5 smd rect (at -1.965 1 135) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 SW1))
    (pad 6 smd rect (at -1 1.965 225) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -0.5 1.965 225) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 0 1.965 225) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 0.5 1.965 225) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC_IN))
    (pad 10 smd rect (at 1 1.965 225) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 1.965 1 135) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 LED1))
    (pad 12 smd rect (at 1.965 0.5 135) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 LED2))
    (pad 13 smd rect (at 1.965 0 135) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 RST))
    (pad 14 smd rect (at 1.965 -0.5 135) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 1.965 -1 135) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 SW2))
    (pad 16 smd rect (at 1 -1.965 225) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 SDA))
    (pad 17 smd rect (at 0.5 -1.965 225) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 0 -1.965 225) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at -0.5 -1.965 225) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at -1 -1.965 225) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 INT))
    (pad 21 smd rect (at 0.625 0.625 135) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at 0.625 -0.625 135) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at -0.625 0.625 135) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at -0.625 -0.625 135) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 58F20F64)
    (at 173.482 57.15)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R2 (at -1.27 -2.032) (layer F.SilkS))
    (fp_text value R (at -0.39878 4.20116) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at -2.413 0) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R2-Pad1)"))
    (pad 2 smd trapezoid (at 2.413 0 180) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 8 LED2))
    (pad 1 thru_hole rect (at -5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 7 "Net-(R2-Pad1)"))
    (pad 2 thru_hole rect (at 5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 8 LED2))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 58F20F71)
    (at 186.182 57.15 180)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R1 (at -1.778 2.032 180) (layer F.SilkS))
    (fp_text value R (at -0.39878 4.20116 180) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at -2.413 0 180) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R1-Pad1)"))
    (pad 2 smd trapezoid (at 2.413 0) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 6 LED1))
    (pad 1 thru_hole rect (at -5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 "Net-(R1-Pad1)"))
    (pad 2 thru_hole rect (at 5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 6 LED1))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58F2255A)
    (at 188.214 64.77)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.524) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC_IN))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 58CDACE0)
    (at 180.086 54.102)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference T1 (at -1.905 -1.27) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 RST))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58F250A1)
    (at 173.482 72.39 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0.127 -1.397 180) (layer F.SilkS))
    (fp_text value 3u3 (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC_IN))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 58F224B6)
    (at 185.166 79.502 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -1.016 12.954 360) (layer F.SilkS) hide)
    (fp_text value CONN_01X05 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 SCL))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 SDA))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 INT))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC_IN))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58F21D99)
    (at 179.578 65.786 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -3.048 0 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC_IN))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 RST))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58F21993)
    (at 186.944 76.454 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at -2.032 1.778 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.8 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58F219A8)
    (at 189.484 76.454 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at -2.032 1.778 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.8 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58F2199E)
    (at 188.214 76.454 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at -2.032 1.778 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.8 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58F218CD)
    (at 190.246 80.01)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 58F22153)
    (at 175.006 54.102)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_1mmDrill (at -1.905 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 58F2215E)
    (at 185.166 54.102)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_1mmDrill (at -1.905 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask))
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 173.482 67.564)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (gr_text "Tapper Rev. 2" (at 180.086 76.962) (layer F.SilkS))
  (gr_text RST (at 180.086 52.578) (layer F.SilkS))
  (gr_text SCL (at 185.166 81.788) (layer F.SilkS))
  (gr_text SDA (at 182.626 81.788) (layer F.SilkS))
  (gr_text INT (at 180.086 81.788) (layer F.SilkS))
  (gr_text VCC (at 177.546 81.788) (layer F.SilkS))
  (gr_text GND (at 175.006 81.788) (layer F.SilkS))
  (gr_text "Tapper Rev. 2 by penguineer\n" (at 190.246 76.962) (layer B.SilkS))
  (gr_text I2C (at 186.436 73.914) (layer F.SilkS))
  (gr_text Addr (at 186.436 74.93) (layer F.SilkS))
  (gr_arc (start 190.246 80.01) (end 192.786 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 192.786 54.102) (end 192.786 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.878 80.01) (end 166.878 54.102) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190.246 82.55) (end 169.418 82.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.418 51.562) (end 190.246 51.562) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 190.246 54.102) (end 190.246 51.562) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 169.418 54.102) (end 166.878 54.102) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 169.418 80.01) (end 169.418 82.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 195.326 84.582) (xy 164.846 84.582) (xy 164.846 49.022) (xy 195.326 49.022)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 195.326 84.582) (xy 164.846 84.582) (xy 164.846 49.022) (xy 195.326 49.022)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 189.103 68.326) (xy 188.214 68.326) (xy 188.214 66.929) (xy 189.103 66.929)
      )
    )
  )
)
