<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="17.78" x2="0" y2="10.16" width="0" layer="20"/>
<wire x1="0" y1="7.62" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="40.64" y2="0" width="0" layer="20"/>
<wire x1="40.64" y1="0" x2="40.64" y2="17.78" width="0" layer="20"/>
<wire x1="40.64" y1="17.78" x2="0" y2="17.78" width="0" layer="20"/>
<wire x1="0" y1="10.16" x2="0" y2="7.62" width="0" layer="20" curve="-180"/>
<text>Connect to WE
FC - Cart Pin 47
NES - Cart Pin 56
</text>
<text>By: GoodTofuFriday

Lift Rom CE pin31 and connect to 5v pin 32! </text>
<text>IS61C256AL</text>
</plain>
<libraries>
<library name="MMC5">
<description>Generated from &lt;b&gt;FlashAdapter.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="DIL32-3">
<description>&lt;B&gt;Dual In Line&lt;/b&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="issi-sram">
<description>&lt;b&gt;Static RAMs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TSOP1-28">
<description>&lt;b&gt;TSOP 1-28&lt;/b&gt; 28-pin Thin Small Outline Package Type 1 (8 x 13.4 mm) (51-85071)&lt;p&gt;
Source: http://download.cypress.com.edgesuite.net/design_resources/datasheets/contents/cy62256_8.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="MMC5" package="DIL32-3" value="29F040TECHP">
<attribute name="VALUE"/>
</element>
<element name="IC3" library="issi-sram" package="TSOP1-28" value="CY62256LL-ZC">
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="WRITE-ENABLE" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="MMC5-A3">
<contactref element="IC1" pad="9"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="MMC5-A2">
<contactref element="IC1" pad="10"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="MMC5-A4">
<contactref element="IC1" pad="8"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="MMC5-A5">
<contactref element="IC1" pad="7"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="MMC5-A6">
<contactref element="IC1" pad="6"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="MMC5-A7">
<contactref element="IC1" pad="5"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="MMC5-A8">
<contactref element="IC1" pad="27"/>
<contactref element="IC3" pad="25"/>
</signal>
<signal name="MMC5-A9">
<contactref element="IC1" pad="26"/>
<contactref element="IC3" pad="24"/>
</signal>
<signal name="MMC5-A10">
<contactref element="IC1" pad="23"/>
<contactref element="IC3" pad="21"/>
</signal>
<signal name="MMC5-A11">
<contactref element="IC1" pad="25"/>
<contactref element="IC3" pad="23"/>
</signal>
<signal name="MMC5-A12">
<contactref element="IC1" pad="4"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="MMC5-A13">
<contactref element="IC1" pad="28"/>
<contactref element="IC3" pad="26"/>
</signal>
<signal name="MMC5-A1">
<contactref element="IC1" pad="11"/>
<contactref element="IC3" pad="9"/>
</signal>
<signal name="MMC5-A0">
<contactref element="IC1" pad="12"/>
<contactref element="IC3" pad="10"/>
</signal>
<signal name="MMC5-D7">
<contactref element="IC1" pad="21"/>
<contactref element="IC3" pad="19"/>
</signal>
<signal name="MMC5-D6">
<contactref element="IC1" pad="20"/>
<contactref element="IC3" pad="18"/>
</signal>
<signal name="MMC5-D5">
<contactref element="IC1" pad="19"/>
<contactref element="IC3" pad="17"/>
</signal>
<signal name="MMC5-D4">
<contactref element="IC1" pad="18"/>
<contactref element="IC3" pad="16"/>
</signal>
<signal name="MMC5-D3">
<contactref element="IC1" pad="17"/>
<contactref element="IC3" pad="15"/>
</signal>
<signal name="MMC5-D2">
<contactref element="IC1" pad="15"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="MMC5-D1">
<contactref element="IC1" pad="14"/>
<contactref element="IC3" pad="12"/>
</signal>
<signal name="MMC5-D0">
<contactref element="IC1" pad="13"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="MMC5-VSS">
<contactref element="IC1" pad="16"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="MMC5-VCC">
<contactref element="IC1" pad="32"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC3" pad="28"/>
</signal>
<signal name="CEROMPIN31">
<contactref element="IC1" pad="31"/>
<contactref element="IC3" pad="20"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="22"/>
<contactref element="IC3" pad="22"/>
</signal>
<signal name="WRITE-ENABLE">
<contactref element="IC3" pad="27"/>
<contactref element="WRITE-ENABLE" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
