(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 222)
    (zones 0)
    (modules 39)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.8128)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.59944 0.29972)
    (user_via 0.8382 0.4318)
    (user_via 1.1684 0.762)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(Q1-Pad1)")
  (net 7 "Net-(C2-Pad2)")
  (net 8 "Net-(C2-Pad1)")
  (net 9 "Net-(D4-Pad2)")
  (net 10 "Net-(D4-Pad1)")
  (net 11 "Net-(D6-Pad2)")
  (net 12 "Net-(Q4-Pad1)")
  (net 13 +5V)
  (net 14 WA)
  (net 15 GND)
  (net 16 WG)
  (net 17 RA)
  (net 18 R)
  (net 19 RG)
  (net 20 HA)
  (net 21 H)
  (net 22 HG)
  (net 23 MD1)
  (net 24 MD2)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +5V)
    (add_net GND)
    (add_net H)
    (add_net HA)
    (add_net HG)
    (add_net MD1)
    (add_net MD2)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net R)
    (add_net RA)
    (add_net RG)
    (add_net WA)
    (add_net WG)
  )
  (module TerminalBlock_Altech:Altech_AK300_1x03_P5.00mm_45-Degree (layer F.Cu) (tedit 5C27907F)
    (at 51.054 65.96 90)
    (descr "Altech AK300 serie terminal block (Script generated with StandardBox.py) (http://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
    (tags "Altech AK300 serie connector")
    (fp_text reference J4 (at -3.89 -5.334 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 5 7.5 90) (layer F.Fab))
    (fp_text user %R (at 5 0.25 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 10 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 24 MD2))
    (pad 2 thru_hole circle (at 5 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 23 MD1))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x03_P5.00mm_45-Degree.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Altech:Altech_AK300_1x03_P5.00mm_45-Degree (layer F.Cu) (tedit 5C27907F)
    (at 50.8 50.8 90)
    (descr "Altech AK300 serie terminal block (Script generated with StandardBox.py) (http://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
    (tags "Altech AK300 serie connector")
    (fp_text reference J3 (at 13.97 -5.08 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 5 7.5 90) (layer F.Fab))
    (fp_text user %R (at 5 0.25 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 10 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 2 thru_hole circle (at 5 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 16 WG))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 14 WA))
    (model ${KISYS3DMOD}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x03_P5.00mm_45-Degree.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 39.8525 44.45 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at 0.2285 1.524) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 35.56 44.45)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 35.526 62.23)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D5 (at 0 1.651) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 39.844 62.23 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D4 (at 0 -1.651) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 35.56 69.85 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C2-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-3-3.5-H_1x03_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294F3F)
    (at 54.61 62.88 90)
    (descr "Terminal Block Phoenix PT-1,5-3-3.5-H, 3 pins, pitch 3.5mm, size 10.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PT-1,5-3-3.5-H pitch 3.5mm size 10.5x7.6mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference J12 (at 3.5 -4.16 90) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 3.5 5.56 90) (layer F.Fab))
    (fp_text user %R (at 3.5 2.4 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 MD2))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 MD1))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-1,5-3-3.5-H_1x03_P3.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-3-3.5-H_1x03_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294F3F)
    (at 54.61 52.324 90)
    (descr "Terminal Block Phoenix PT-1,5-3-3.5-H, 3 pins, pitch 3.5mm, size 10.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PT-1,5-3-3.5-H pitch 3.5mm size 10.5x7.6mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference J11 (at 3.5 -4.16 90) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 3.5 5.56 90) (layer F.Fab))
    (fp_text user %R (at 3.5 2.4 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 WG))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 WA))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-1,5-3-3.5-H_1x03_P3.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 46.99 59.69 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 MD2))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 MD1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 46.99 52.07 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 WG))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 WA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 24.13 54.61)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 HA))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 H))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 HG))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 24.13 46.99)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 RA))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 R))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 RG))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-3-3.5-H_1x03_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294F3F)
    (at 16.51 55.88 270)
    (descr "Terminal Block Phoenix PT-1,5-3-3.5-H, 3 pins, pitch 3.5mm, size 10.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PT-1,5-3-3.5-H pitch 3.5mm size 10.5x7.6mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference J6 (at 3.5 -4.16 90) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 3.5 5.56 90) (layer F.Fab))
    (fp_text user %R (at 3.5 2.4 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 HA))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 H))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 HG))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-1,5-3-3.5-H_1x03_P3.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-3-3.5-H_1x03_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294F3F)
    (at 16.51 45.324 270)
    (descr "Terminal Block Phoenix PT-1,5-3-3.5-H, 3 pins, pitch 3.5mm, size 10.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PT-1,5-3-3.5-H pitch 3.5mm size 10.5x7.6mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference J5 (at 3.5 -4.16 90) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 3.5 5.56 90) (layer F.Fab))
    (fp_text user %R (at 3.5 2.4 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 RA))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 R))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 RG))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-1,5-3-3.5-H_1x03_P3.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 56D1B4CB)
    (at 50.8 33.528)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference H4 (at 0.508 -6.096) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 56D1B4CB)
    (at 20.32 73.152)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference H3 (at 0 -5.3) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 56D1B4CB)
    (at 50.8 73.152)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference H2 (at 0 -5.3) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 56D1B4CB)
    (at 20.32 33.528)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference H1 (at 0 -5.3) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 39.8525 69.85)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 1.524) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 WA))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 39.8525 36.83)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 WG))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Altech:Altech_AK300_1x03_P5.00mm_45-Degree (layer F.Cu) (tedit 5C27907F)
    (at 20.32 55.88 270)
    (descr "Altech AK300 serie terminal block (Script generated with StandardBox.py) (http://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
    (tags "Altech AK300 serie connector")
    (fp_text reference J2 (at 13.97 -5.08 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 5 7.5 90) (layer F.Fab))
    (fp_text user %R (at 5 0.25 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 10 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 20 HA))
    (pad 2 thru_hole circle (at 5 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 21 H))
    (pad 1 thru_hole rect (at 0 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 22 HG))
    (model ${KISYS3DMOD}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x03_P5.00mm_45-Degree.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Altech:Altech_AK300_1x03_P5.00mm_45-Degree (layer F.Cu) (tedit 5C27907F)
    (at 20.32 40.894 270)
    (descr "Altech AK300 serie terminal block (Script generated with StandardBox.py) (http://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
    (tags "Altech AK300 serie connector")
    (fp_text reference J1 (at -4.064 -5.08 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 5 7.5 90) (layer F.Fab))
    (fp_text user %R (at 5 0.25 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 10 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 17 RA))
    (pad 2 thru_hole circle (at 5 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 18 R))
    (pad 1 thru_hole rect (at 0 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 19 RG))
    (model ${KISYS3DMOD}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x03_P5.00mm_45-Degree.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 31.2675 69.85 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.651) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(Q4-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 WA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 34.29 66.2685 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -2.1845 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 31.2675 62.23 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0.0255 -1.4605) (layer F.SilkS))
    (fp_text value 470 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D6-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 36.83 66.2685 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2.1845 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 31.43 66.024 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at -0.066 -2.429) (layer F.SilkS))
    (fp_text value BSS84 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 39.64 66.101 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -0.111 -2.4155) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 38.1 74.4475 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D6 (at -0.0255 -1.778 180) (layer F.SilkS))
    (fp_text value "LED rot" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D6-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 36.83 40.9195 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.5655 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 31.2675 44.45 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -0.0255 1.27) (layer F.SilkS))
    (fp_text value 470R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 34.29 40.9195 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.5655 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 31.2675 36.83)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 WG))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 39.64 40.64)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -0.016 -2.413) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 -270) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 31.43 40.64)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -0.061 -2.413) (layer F.SilkS))
    (fp_text value BSS84 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_SMD:Relay_DPDT_Omron_G6SK-2F (layer F.Cu) (tedit 5A59BF6A)
    (at 35.56 53.34)
    (descr "Relay Omron G6SK-2F, see http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6s.pdf")
    (tags "Relay Omron G6SK-2F")
    (attr smd)
    (fp_text reference K1 (at 0 0) (layer F.SilkS))
    (fp_text value TX2SA-LT-4.5V (at -0.04 8.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 7 smd rect (at 4 6.35) (size 2.2 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 6 smd rect (at -4 6.35) (size 2.2 1) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 5 smd rect (at -4 3.81) (size 2.2 1) (layers F.Cu F.Paste F.Mask)
      (net 20 HA))
    (pad 8 smd rect (at 4 3.81) (size 2.2 1) (layers F.Cu F.Paste F.Mask)
      (net 17 RA))
    (pad 3 smd rect (at -4 -1.27) (size 2.2 1) (layers F.Cu F.Paste F.Mask)
      (net 22 HG))
    (pad 1 smd rect (at -4 -6.35) (size 2.2 1) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 10 smd rect (at 4 -1.27) (size 2.2 1) (layers F.Cu F.Paste F.Mask)
      (net 19 RG))
    (pad 12 smd rect (at 4 -6.35) (size 2.2 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 4 smd rect (at -4 1.27) (size 2.2 1) (layers F.Cu F.Paste F.Mask)
      (net 21 H))
    (pad 9 smd rect (at 4 1.27) (size 2.2 1) (layers F.Cu F.Paste F.Mask)
      (net 18 R))
    (model ${KISYS3DMOD}/Relay_SMD.3dshapes/Relay_DPDT_Omron_G6SK-2F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 38.1 33.02 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 1.778 180) (layer F.SilkS))
    (fp_text value "LED grün" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 35.5345 36.83)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "rev 1.1\n" (at 41.91 76.2) (layer F.SilkS))
  (gr_text Weichenrückmelder (at 35.56 30.48) (layer F.SilkS))
  (gr_text Umschalter (at 43.18 48.26 90) (layer F.SilkS))
  (gr_text Decoder (at 43.18 58.42 90) (layer F.SilkS))
  (gr_text 5V (at 43.18 66.04 90) (layer F.SilkS))
  (gr_text GND (at 43.18 40.894 90) (layer F.SilkS))
  (gr_text Abzweigend (at 32.512 74.422) (layer F.SilkS))
  (gr_text Gerade (at 34.29 33.02) (layer F.SilkS))
  (gr_text Herzstück (at 27.94 60.96 90) (layer F.SilkS))
  (gr_text Rückmeldung (at 27.94 45.72 90) (layer F.SilkS))
  (gr_line (start 12.7 77.47) (end 12.7 29.21) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 58.42 77.47) (end 12.7 77.47) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 58.42 29.21) (end 58.42 77.47) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 12.7 29.21) (end 58.42 29.21) (layer Edge.Cuts) (width 0.05))
  (zone (net 15) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.42 77.47) (xy 12.7 77.47) (xy 12.7 29.21) (xy 58.42 29.21)
      )
    )
  )
  (zone (net 15) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.42 77.47) (xy 12.7 77.47) (xy 12.7 29.21) (xy 58.42 29.21)
      )
    )
  )
)
