(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~86~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 35)
    (tracks 236)
    (zones 0)
    (modules 17)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Vref)
  (net 2 GND)
  (net 3 "Net-(D1-Pad2)")
  (net 4 RXD)
  (net 5 TXD)
  (net 6 ~TReset)
  (net 7 TDI)
  (net 8 TDO)
  (net 9 TCK)
  (net 10 TMS)
  (net 11 GPIO15)
  (net 12 GPIO2)
  (net 13 CH_PD)
  (net 14 GPIO0)
  (net 15 "Net-(R6-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CH_PD)
    (add_net GND)
    (add_net GPIO0)
    (add_net GPIO15)
    (add_net GPIO2)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net RXD)
    (add_net TCK)
    (add_net TDI)
    (add_net TDO)
    (add_net TMS)
    (add_net TXD)
    (add_net ~TReset)
  )
  (net_class VCC ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 1)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Vref)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 133.5 113.25)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -2.5 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab))
    (fp_text user %R (at -2.5 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 Vref))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch1.27mm (layer F.Cu) (tedit 59650536)
    (at 149.25 106.5 180)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (fp_text reference DBG (at 0.75 -1.75) (layer F.SilkS))
    (fp_text value T_DBG (at -0.635 7.215) (layer F.Fab))
    (fp_text user %R (at -0.635 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 Vref))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 TMS))
    (pad 3 thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 1.27 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 TCK))
    (pad 5 thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 1.27 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 TDO))
    (pad 7 thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 1.27 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 TDI))
    (pad 9 thru_hole oval (at 0 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 1.27 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 ~TReset))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ESP8266:ESP-12E_SMD (layer F.Cu) (tedit 58FB7FFE)
    (at 118.5 110 90)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U1 (at 6.35 2.54 90) (layer F.SilkS))
    (fp_text value ESP-12F (at 6.35 6.35 90) (layer F.Fab) hide)
    (fp_text user "No Copper" (at 6.892 -5.4 90) (layer F.CrtYd))
    (pad 22 smd rect (at 11.99 15 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 9.99 15 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 7.99 15 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 5.99 15 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 3.99 15 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 1.99 15 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 14 0 90) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 5 TXD))
    (pad 15 smd rect (at 14 2 90) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 4 RXD))
    (pad 14 smd rect (at 14 4 90) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 10 TMS))
    (pad 13 smd rect (at 14 6 90) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 9 TCK))
    (pad 12 smd rect (at 14 8 90) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 14 GPIO0))
    (pad 11 smd rect (at 14 10 90) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 12 GPIO2))
    (pad 10 smd rect (at 14 12 90) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 11 GPIO15))
    (pad 9 smd rect (at 14 14 90) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 0 14 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 Vref))
    (pad 7 smd rect (at 0 12 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 8 TDO))
    (pad 6 smd rect (at 0 10 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 TDI))
    (pad 5 smd rect (at 0 8 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 6 ~TReset))
    (pad 4 smd rect (at 0 6 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 4 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 13 CH_PD))
    (pad 2 smd rect (at 0 2 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0 0 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module BVH_Logos:SkyIron_logo_Back (layer F.Cu) (tedit 5EC1B53B)
    (at 123 103.5 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module BVH_Switches:Tac_SMD_6.4mm_Side_SPST_NO (layer F.Cu) (tedit 5EC803C5)
    (at 139.5 93 180)
    (descr "side smd tac switch")
    (tags "switch tac rightangle side smd")
    (attr smd)
    (fp_text reference SW2 (at 0 0) (layer F.Fab))
    (fp_text value BOOT (at 0 -2.7) (layer F.Fab))
    (pad 1 smd rect (at 2.8 -0.85 180) (size 1.2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.8 0.85 180) (size 1.2 1) (layers F.Cu F.Paste F.Mask)
      (net 14 GPIO0))
    (pad 2 smd rect (at -2.8 0.85 180) (size 1.2 1) (layers F.Cu F.Paste F.Mask)
      (net 14 GPIO0))
    (pad 1 smd rect (at -2.8 -0.75 180) (size 1.2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 1.375 180) (size 0.75 0.75) (drill 0.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -1.375 180) (size 0.75 0.75) (drill 0.75) (layers *.Cu *.Mask))
  )
  (module BVH_Switches:Tac_SMD_6.4mm_Side_SPST_NO (layer F.Cu) (tedit 5EC803C5)
    (at 139.5 113.5)
    (descr "side smd tac switch")
    (tags "switch tac rightangle side smd")
    (attr smd)
    (fp_text reference SW1 (at 0 0) (layer F.Fab))
    (fp_text value RST (at 0 -2.7) (layer F.Fab))
    (pad 1 smd rect (at 2.8 -0.85) (size 1.2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.8 0.85) (size 1.2 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (pad 2 smd rect (at -2.8 0.85) (size 1.2 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (pad 1 smd rect (at -2.8 -0.75) (size 1.2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 1.375) (size 0.75 0.75) (drill 0.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -1.375) (size 0.75 0.75) (drill 0.75) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 118.5 113.95 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 1.05 -1.5 270) (layer F.SilkS))
    (fp_text value 10k (at 0.05 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 Vref))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 139.45 98.5)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 2.55 0) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 GPIO15))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 126.5 92.05 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -2.45 0 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 Vref))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 GPIO0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 122.5 113.95 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 1.05 -1.5 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 Vref))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 CH_PD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 128.5 92.05 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 Vref))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 GPIO2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 130.5 92.05 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 GPIO15))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A422)
    (at 154.5 110.5 180)
    (descr "Through hole straight socket strip, 2x04, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x04 2.54mm double row")
    (fp_text reference J3 (at -1.27 -2.77) (layer F.SilkS) hide)
    (fp_text value JTAG (at -1.27 10.39) (layer F.Fab))
    (fp_text user %R (at -1.27 3.81 90) (layer F.Fab))
    (fp_text user VCC (at -5 8 270) (layer F.SilkS))
    (fp_text user GND (at -5 -1 270) (layer F.SilkS))
    (fp_text user TCK (at -5 2 270) (layer F.SilkS))
    (fp_text user TMS (at -5 5 270) (layer F.SilkS))
    (fp_text user TDO (at 2.5 -1 270) (layer F.SilkS))
    (fp_text user TDI (at 2.5 2 270) (layer F.SilkS))
    (fp_text user ~RST (at 2.5 5 270) (layer F.SilkS))
    (pad 8 thru_hole oval (at -2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Vref))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 TMS))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 ~TReset))
    (pad 4 thru_hole oval (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 TCK))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 TDI))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 TDO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A429)
    (at 150 94 90)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 2.5 2.5 180) (layer F.SilkS) hide)
    (fp_text value ESP_Serial (at 0 7.85 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 TXD))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 RXD))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803)
    (at 139.4 96.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 3.6 0) (layer F.SilkS))
    (fp_text value STAT (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x10 (layer F.Cu) (tedit 58AA9153)
    (at 140.5 105.5 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C3 (at 0 5.45 90) (layer F.SilkS) hide)
    (fp_text value 100uF (at 0 -5.45 90) (layer F.Fab))
    (fp_text user + (at -2.31 -0.08 90) (layer F.Fab))
    (fp_text user + (at -4.78 3.9 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 Vref))
    (pad 2 smd rect (at 3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 133.5 115)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.5 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 0) (layer F.Fab))
    (fp_text user %R (at -2.5 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 Vref))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text RST (at 144 113.5 90) (layer F.SilkS))
  (gr_text . (at 150 107.5) (layer F.SilkS))
  (gr_text "BVH - AB4EN\nESP8266 BMP Board\nv1 - 2020-06" (at 114.25 103 90) (layer B.SilkS))
  (gr_arc (start 110.5 91) (end 110.5 90) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 110.5 115.5) (end 109.5 115.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 159.5 115.5) (end 159.5 116.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 159.5 91) (end 160.5 91) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text BOOT (at 144.5 93 90) (layer F.SilkS))
  (gr_text "3.3V\nONLY" (at 148.25 112.25 90) (layer F.SilkS))
  (gr_line (start 109.5 115.5) (end 109.5 91) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 159.5 116.5) (end 110.5 116.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 160.5 91) (end 160.5 115.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.5 90) (end 159.5 90) (layer Edge.Cuts) (width 0.05))
  (gr_text GND (at 155 97 90) (layer F.SilkS))
  (gr_text RX (at 150 96.5 90) (layer F.SilkS))
  (gr_text TX (at 152.5 96.5 90) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.5 116.5) (xy 116.5 116.5) (xy 116.5 112.5) (xy 116.5 93.5) (xy 116.5 90)
        (xy 160.5 90)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.5 116.5) (xy 116.5 116.5) (xy 116.5 90) (xy 160.5 90)
      )
    )
  )
)
