<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<hole x="35.941" y="3.7592" drill="2.5"/>
<text>V G O G V</text>
<text>V G O G V</text>
<hole x="14.859" y="3.7338" drill="2.5"/>
<hole x="46.4566" y="21.9964" drill="2.5"/>
<hole x="35.941" y="40.2336" drill="2.5"/>
<hole x="14.859" y="40.2336" drill="2.5"/>
<hole x="4.318" y="21.9964" drill="2.5"/>
<text>V G O G V</text>
<text>V G O G V</text>
<text>V G O G V</text>
<wire x1="14.605" y1="0" x2="35.8775" y2="0" width="0.254" layer="20"/>
<wire x1="35.8775" y1="0" x2="39.0525" y2="1.7145" width="0.254" layer="20" curve="56.738082"/>
<wire x1="39.0525" y1="1.7145" x2="49.784" y2="20.193" width="0.254" layer="20"/>
<wire x1="49.784" y1="20.193" x2="49.657" y2="23.9395" width="0.254" layer="20" curve="64.175245"/>
<wire x1="49.657" y1="23.9395" x2="39.116" y2="42.2275" width="0.254" layer="20"/>
<wire x1="39.116" y1="42.2275" x2="36.068" y2="44.0055" width="0.254" layer="20" curve="59.56979"/>
<wire x1="36.068" y1="44.0055" x2="14.732" y2="44.0055" width="0.254" layer="20"/>
<wire x1="14.732" y1="44.0055" x2="11.684" y2="42.2275" width="0.254" layer="20" curve="60.512868"/>
<wire x1="11.684" y1="42.2275" x2="1.0795" y2="23.876" width="0.254" layer="20"/>
<wire x1="1.0795" y1="23.876" x2="1.016" y2="20.2565" width="0.254" layer="20" curve="58.033184"/>
<wire x1="1.016" y1="20.2565" x2="11.6205" y2="1.905" width="0.254" layer="20"/>
<wire x1="11.6205" y1="1.905" x2="14.605" y2="0" width="0.254" layer="20" curve="54.856645"/>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="0805">
</package>
<package name="EIA3216">
</package>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP44">
</package>
</packages>
</library>
<library name="SMD_Button_Custom">
<packages>
<package name="SW2-4.0X3.0X2.0">
</package>
</packages>
</library>
<library name="Seeed-LED-2016">
<packages>
<package name="LED-0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="1X05_NO_SILK">
<description>No outline in silkscreen</description>
</package>
<package name="1X05_LONGPADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C10" library="SparkFun" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun" package="HC49US" value="16MHz">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun" package="0805" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun" package="0805" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun" package="0805" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun" package="0805" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ATMEGA32U4" library="SparkFun-DigitalIC" package="TQFP44" value="ATMEGA32U4TQFP-44">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="SMD_Button_Custom" package="SW2-4.0X3.0X2.0" value="B3U-1000P-2P-SMD">
<attribute name="MPN" value="B3U-1000P-2P-SMD"/>
<attribute name="NAME"/>
</element>
<element name="D1" library="Seeed-LED-2016" package="LED-0805" value="GREEN-0805">
<attribute name="MPN" value="17-215SYGC/S530-E2/TR8"/>
<attribute name="NAME"/>
</element>
<element name="PRG" library="SparkFun-Connectors" package="2X3" value="AVR_SPI_PRG_6PTH">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="USB-MINIB" value="USB-MINIB-5PIN">
<attribute name="PROD_ID" value="CONN-08193"/>
</element>
<element name="C7" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X05_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X05_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X05_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X05_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J11" library="SparkFun-Connectors" package="1X05_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C13" pad="C"/>
<contactref element="C10" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="ATMEGA32U4" pad="15"/>
<contactref element="ATMEGA32U4" pad="23"/>
<contactref element="ATMEGA32U4" pad="35"/>
<contactref element="ATMEGA32U4" pad="43"/>
<contactref element="ATMEGA32U4" pad="33"/>
<contactref element="ATMEGA32U4" pad="5"/>
<contactref element="RESET" pad="1"/>
<contactref element="PRG" pad="6"/>
<contactref element="J3" pad="GND"/>
<contactref element="C7" pad="C"/>
<contactref element="C9" pad="C"/>
<contactref element="C8" pad="C"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="2"/>
<contactref element="J4" pad="4"/>
<contactref element="J4" pad="2"/>
<contactref element="J2" pad="4"/>
<contactref element="J2" pad="2"/>
<contactref element="J5" pad="4"/>
<contactref element="J5" pad="2"/>
<contactref element="J6" pad="4"/>
<contactref element="J6" pad="2"/>
<contactref element="J7" pad="4"/>
<contactref element="J7" pad="2"/>
<contactref element="J8" pad="4"/>
<contactref element="J8" pad="2"/>
<contactref element="J9" pad="4"/>
<contactref element="J9" pad="2"/>
<contactref element="J10" pad="4"/>
<contactref element="J10" pad="2"/>
<contactref element="J11" pad="4"/>
<contactref element="J11" pad="2"/>
</signal>
<signal name="AREF">
<contactref element="C1" pad="2"/>
<contactref element="ATMEGA32U4" pad="42"/>
</signal>
<signal name="RESET">
<contactref element="R2" pad="1"/>
<contactref element="ATMEGA32U4" pad="13"/>
<contactref element="RESET" pad="2"/>
<contactref element="PRG" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="ATMEGA32U4" pad="9"/>
<contactref element="PRG" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="ATMEGA32U4" pad="11"/>
<contactref element="PRG" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="ATMEGA32U4" pad="10"/>
<contactref element="PRG" pad="4"/>
</signal>
<signal name="TXO">
<contactref element="ATMEGA32U4" pad="21"/>
</signal>
<signal name="D9">
<contactref element="ATMEGA32U4" pad="29"/>
</signal>
<signal name="D8">
<contactref element="ATMEGA32U4" pad="28"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="A5">
<contactref element="ATMEGA32U4" pad="41"/>
</signal>
<signal name="A4">
<contactref element="ATMEGA32U4" pad="40"/>
</signal>
<signal name="A3">
<contactref element="ATMEGA32U4" pad="39"/>
</signal>
<signal name="A2">
<contactref element="ATMEGA32U4" pad="38"/>
</signal>
<signal name="A1">
<contactref element="ATMEGA32U4" pad="37"/>
</signal>
<signal name="A0">
<contactref element="ATMEGA32U4" pad="36"/>
</signal>
<signal name="D2_SDA">
<contactref element="ATMEGA32U4" pad="19"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="D3_SCL">
<contactref element="ATMEGA32U4" pad="18"/>
</signal>
<signal name="D4">
<contactref element="ATMEGA32U4" pad="25"/>
</signal>
<signal name="D5">
<contactref element="ATMEGA32U4" pad="31"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="D6">
<contactref element="ATMEGA32U4" pad="27"/>
</signal>
<signal name="D7">
<contactref element="ATMEGA32U4" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="D10">
<contactref element="ATMEGA32U4" pad="30"/>
</signal>
<signal name="N$1">
<contactref element="Y1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="ATMEGA32U4" pad="16"/>
</signal>
<signal name="N$2">
<contactref element="Y1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="ATMEGA32U4" pad="17"/>
</signal>
<signal name="RXI">
<contactref element="ATMEGA32U4" pad="20"/>
</signal>
<signal name="UCAP">
<contactref element="C5" pad="2"/>
<contactref element="ATMEGA32U4" pad="6"/>
</signal>
<signal name="D-">
<contactref element="R7" pad="1"/>
<contactref element="ATMEGA32U4" pad="3"/>
</signal>
<signal name="D+">
<contactref element="R5" pad="1"/>
<contactref element="ATMEGA32U4" pad="4"/>
</signal>
<signal name="D11">
<contactref element="ATMEGA32U4" pad="12"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="D12">
<contactref element="ATMEGA32U4" pad="26"/>
</signal>
<signal name="D13">
<contactref element="ATMEGA32U4" pad="32"/>
</signal>
<signal name="D14">
<contactref element="ATMEGA32U4" pad="8"/>
</signal>
<signal name="TXLED">
<contactref element="R6" pad="1"/>
<contactref element="ATMEGA32U4" pad="22"/>
</signal>
<signal name="N$6">
<contactref element="R7" pad="2"/>
<contactref element="J3" pad="D-"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="2"/>
<contactref element="J3" pad="D+"/>
</signal>
<signal name="N$7">
<contactref element="R6" pad="2"/>
<contactref element="D1" pad="-"/>
</signal>
<signal name="5V">
<contactref element="ATMEGA32U4" pad="7"/>
<contactref element="ATMEGA32U4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="C13" pad="A"/>
<contactref element="ATMEGA32U4" pad="14"/>
<contactref element="ATMEGA32U4" pad="34"/>
<contactref element="ATMEGA32U4" pad="24"/>
<contactref element="ATMEGA32U4" pad="44"/>
<contactref element="D1" pad="+"/>
<contactref element="PRG" pad="2"/>
<contactref element="J3" pad="VBUS"/>
<contactref element="R2" pad="2"/>
<contactref element="C7" pad="A"/>
<contactref element="C9" pad="A"/>
<contactref element="C8" pad="A"/>
<contactref element="J4" pad="1"/>
<contactref element="J4" pad="5"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="J5" pad="5"/>
<contactref element="J2" pad="5"/>
<contactref element="J2" pad="1"/>
<contactref element="J7" pad="1"/>
<contactref element="J7" pad="5"/>
<contactref element="J6" pad="5"/>
<contactref element="J6" pad="1"/>
<contactref element="J9" pad="1"/>
<contactref element="J9" pad="5"/>
<contactref element="J8" pad="5"/>
<contactref element="J8" pad="1"/>
<contactref element="J11" pad="1"/>
<contactref element="J11" pad="5"/>
<contactref element="J10" pad="5"/>
<contactref element="J10" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="J4" pad="3"/>
<contactref element="J1" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="J5" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="J7" pad="3"/>
<contactref element="J6" pad="3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="J9" pad="3"/>
<contactref element="J8" pad="3"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="J11" pad="3"/>
<contactref element="J10" pad="3"/>
<contactref element="R9" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
