(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 26)
    (zones 0)
    (modules 4)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 6033B16C)
    (at 62.23 55.88 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value PinHeader_1x05_P2.54mm_Vertical (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08 180) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_Micro-B_Amphenol_10118194_Horizontal (layer F.Cu) (tedit 6033B02B)
    (at 67.31 60.96)
    (descr "USB Micro-B receptacle, horizontal, SMD, 10118194, https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10118194.pdf")
    (tags "USB Micro B horizontal SMD")
    (attr smd)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value USB_Micro-B_Amphenol_10118194_Horizontal (at 0 4.75) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.75) (layer Dwgs.User))
    (fp_text user %R (at 0 -0.05) (layer F.Fab))
    (pad "" smd oval (at 2.5 -1.4) (size 1.25 0.95) (layers F.Paste))
    (pad "" smd oval (at -2.5 -1.4) (size 1.25 0.95) (layers F.Paste))
    (pad 6 thru_hole oval (at 3.5 1.3) (size 0.89 1.55) (drill oval 0.5 1.15) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -3.5 1.3) (size 0.89 1.55) (drill oval 0.5 1.15) (layers *.Cu *.Mask))
    (pad "" smd oval (at 3.5 1.3) (size 0.89 1.55) (layers F.Paste))
    (pad 6 thru_hole oval (at 2.5 -1.4) (size 1.25 0.95) (drill oval 0.85 0.55) (layers *.Cu *.Mask))
    (pad "" smd oval (at -3.5 1.3) (size 0.89 1.55) (layers F.Paste))
    (pad 6 thru_hole oval (at -2.5 -1.4) (size 1.25 0.95) (drill oval 0.85 0.55) (layers *.Cu *.Mask))
    (pad 5 smd rect (at 1.3 -1.4) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.65 -1.4) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -1.4) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.65 -1.4) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.3 -1.4) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Amphenol_10118194_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 62.23 58.928 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at 0 1.65 270) (layer B.SilkS) hide)
    (fp_text value R_0805_2012Metric (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.243902))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.243902))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 72.39 59.436 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at 0 1.65 270) (layer B.SilkS) hide)
    (fp_text value R_0805_2012Metric (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.243902))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.243902))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 72.644 58.674 90) (layer F.SilkS))
  (gr_text id (at 70.104 57.912 180) (layer F.SilkS))
  (gr_text D+ (at 67.564 57.912 180) (layer F.SilkS))
  (gr_text D- (at 64.77 57.912 180) (layer F.SilkS))
  (gr_text V+ (at 62.23 58.166 90) (layer F.SilkS))
  (gr_line (start 73.66 54.61) (end 60.96 54.61) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 73.66 63.754) (end 73.66 54.61) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 60.96 63.754) (end 73.66 63.754) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 60.96 63.5) (end 60.96 63.754) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 60.96 54.61) (end 60.96 63.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73.66 63.754) (xy 60.96 63.754) (xy 60.96 54.61) (xy 73.66 54.61)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73.66 63.754) (xy 60.96 63.754) (xy 60.96 54.61) (xy 73.66 54.61)
      )
    )
  )
)
