(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 0)
    (no_connects 0)
    (area 75.198381 75.19838 124.80162 124.801619)
    (thickness 1.6)
    (drawings 54)
    (tracks 429)
    (zones 0)
    (modules 7)
    (nets 49)
  )
  (page USLetter)
  (title_block
    (title "PSRAM Test")
    (date 2017-11-30)
    (rev 0)
    (comment 1 "BGA Solderability Test")
    (comment 2 "Also a breakout board")
  )
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.381)
    (via_drill 0.254)
    (via_min_size 0.381)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /LB#)
  (net 2 /DQ8)
  (net 3 /DQ9)
  (net 4 /VSSQ)
  (net 5 /VDDQ)
  (net 6 /DQ14)
  (net 7 /DQ15)
  (net 8 /A18)
  (net 9 /OE#)
  (net 10 /UB#)
  (net 11 /DQ10)
  (net 12 /DQ11)
  (net 13 /DQ12)
  (net 14 /DQ13)
  (net 15 /A19)
  (net 16 /A8)
  (net 17 /A0)
  (net 18 /A3)
  (net 19 /A5)
  (net 20 /A17)
  (net 21 /A21)
  (net 22 /A14)
  (net 23 /A12)
  (net 24 /A9)
  (net 25 /A1)
  (net 26 /A4)
  (net 27 /A6)
  (net 28 /A7)
  (net 29 /A16)
  (net 30 /A15)
  (net 31 /A13)
  (net 32 /A10)
  (net 33 /A2)
  (net 34 /CE#)
  (net 35 /DQ1)
  (net 36 /DQ3)
  (net 37 /DQ4)
  (net 38 /DQ5)
  (net 39 /WE#)
  (net 40 /A11)
  (net 41 /ZZ#)
  (net 42 /DQ0)
  (net 43 /DQ2)
  (net 44 /VDD)
  (net 45 /VSS)
  (net 46 /DQ6)
  (net 47 /DQ7)
  (net 48 /A20)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.381)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A19)
    (add_net /A2)
    (add_net /A20)
    (add_net /A21)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CE#)
    (add_net /DQ0)
    (add_net /DQ1)
    (add_net /DQ10)
    (add_net /DQ11)
    (add_net /DQ12)
    (add_net /DQ13)
    (add_net /DQ14)
    (add_net /DQ15)
    (add_net /DQ2)
    (add_net /DQ3)
    (add_net /DQ4)
    (add_net /DQ5)
    (add_net /DQ6)
    (add_net /DQ7)
    (add_net /DQ8)
    (add_net /DQ9)
    (add_net /LB#)
    (add_net /OE#)
    (add_net /UB#)
    (add_net /VDD)
    (add_net /VDDQ)
    (add_net /VSS)
    (add_net /VSSQ)
    (add_net /WE#)
    (add_net /ZZ#)
  )
  (net_class 4.5/4.5 ""
    (clearance 0.1143)
    (trace_width 0.1143)
    (via_dia 0.381)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class 5/5 ""
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.381)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class 6/6 ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.381)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Customs:TFBGA-48 (layer F.Cu) (tedit 5A1C4695)
    (at 100 100)
    (fp_text reference U1 (at 6 6) (layer F.SilkS))
    (fp_text value IS66WVE4M16EBLL-70BLI (at 0 5.08) (layer F.Fab))
    (fp_text user "Ensure copper registration marks are visible" (at 44.55 -2.15) (layer Cmts.User))
    (pad A1 smd circle (at -1.875 -2.625) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /LB#))
    (pad B1 smd circle (at -1.875 -1.875) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /DQ8))
    (pad C1 smd circle (at -1.875 -1.125) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /DQ9))
    (pad D1 smd circle (at -1.875 -0.375) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /VSSQ))
    (pad E1 smd circle (at -1.875 0.375) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDDQ))
    (pad F1 smd circle (at -1.875 1.125) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /DQ14))
    (pad G1 smd circle (at -1.875 1.875) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /DQ15))
    (pad H1 smd circle (at -1.875 2.625) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /A18))
    (pad A2 smd circle (at -1.125 -2.625) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /OE#))
    (pad B2 smd circle (at -1.125 -1.875) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /UB#))
    (pad C2 smd circle (at -1.125 -1.125) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /DQ10))
    (pad D2 smd circle (at -1.125 -0.375) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /DQ11))
    (pad E2 smd circle (at -1.125 0.375) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /DQ12))
    (pad F2 smd circle (at -1.125 1.125) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /DQ13))
    (pad G2 smd circle (at -1.125 1.875) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /A19))
    (pad H2 smd circle (at -1.125 2.625) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /A8))
    (pad A3 smd circle (at -0.375 -2.625) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /A0))
    (pad B3 smd circle (at -0.375 -1.875) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /A3))
    (pad C3 smd circle (at -0.375 -1.125) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /A5))
    (pad D3 smd circle (at -0.375 -0.375) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /A17))
    (pad E3 smd circle (at -0.375 0.375) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /A21))
    (pad F3 smd circle (at -0.375 1.125) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /A14))
    (pad G3 smd circle (at -0.375 1.875) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /A12))
    (pad H3 smd circle (at -0.375 2.625) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /A9))
    (pad A4 smd circle (at 0.375 -2.625) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /A1))
    (pad B4 smd circle (at 0.375 -1.875) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /A4))
    (pad C4 smd circle (at 0.375 -1.125) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /A6))
    (pad D4 smd circle (at 0.375 -0.375) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /A7))
    (pad E4 smd circle (at 0.375 0.375) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /A16))
    (pad F4 smd circle (at 0.375 1.125) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /A15))
    (pad G4 smd circle (at 0.375 1.875) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /A13))
    (pad H4 smd circle (at 0.375 2.625) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 /A10))
    (pad A5 smd circle (at 1.125 -2.625) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /A2))
    (pad B5 smd circle (at 1.125 -1.875) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 /CE#))
    (pad C5 smd circle (at 1.125 -1.125) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 /DQ1))
    (pad D5 smd circle (at 1.125 -0.375) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /DQ3))
    (pad E5 smd circle (at 1.125 0.375) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 /DQ4))
    (pad F5 smd circle (at 1.125 1.125) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 /DQ5))
    (pad G5 smd circle (at 1.125 1.875) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 /WE#))
    (pad H5 smd circle (at 1.125 2.625) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 /A11))
    (pad A6 smd circle (at 1.875 -2.625) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 /ZZ#))
    (pad B6 smd circle (at 1.875 -1.875) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 /DQ0))
    (pad C6 smd circle (at 1.875 -1.125) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 /DQ2))
    (pad D6 smd circle (at 1.875 -0.375) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 /VDD))
    (pad E6 smd circle (at 1.875 0.375) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 /VSS))
    (pad F6 smd circle (at 1.875 1.125) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 /DQ6))
    (pad G6 smd circle (at 1.875 1.875) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 /DQ7))
    (pad H6 smd circle (at 1.875 2.625) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 /A20))
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 120 86 180)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 180) (layer B.SilkS))
    (fp_text value Conn_01x12 (at 0 -30.27 180) (layer B.Fab))
    (fp_text user %R (at 0 -13.97 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /DQ0))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /DQ1))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /DQ2))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /DQ3))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /DQ4))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /DQ5))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /DQ6))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /DQ7))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /DQ8))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /DQ9))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /DQ10))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /DQ11))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 80 114)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J2 (at 0 2.33) (layer B.SilkS))
    (fp_text value Conn_01x12 (at 0 -30.27) (layer B.Fab))
    (fp_text user %R (at 0 -13.97 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /A13))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /A12))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /A11))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /A10))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /A9))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /A8))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /A7))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /A6))
    (pad 9 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /A5))
    (pad 10 thru_hole oval (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /A4))
    (pad 11 thru_hole oval (at 0 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /A3))
    (pad 12 thru_hole oval (at 0 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /A2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 114 120 90)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J3 (at 0 2.33 90) (layer B.SilkS))
    (fp_text value Conn_01x12 (at 0 -30.27 90) (layer B.Fab))
    (fp_text user %R (at 0 -7.65 360) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /DQ12))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /DQ13))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /DQ14))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /DQ15))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /A21))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /A20))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /A19))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /A18))
    (pad 9 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /A17))
    (pad 10 thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /A16))
    (pad 11 thru_hole oval (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /A15))
    (pad 12 thru_hole oval (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /A14))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 86 80 270)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J4 (at 0 2.33 270) (layer B.SilkS))
    (fp_text value Conn_01x12 (at 0 -30.27 270) (layer B.Fab))
    (fp_text user %R (at 0 -13.97 540) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /A1))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /A0))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /VSS))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /VDD))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VSSQ))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /VDDQ))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /UB#))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /LB#))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /OE#))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /ZZ#))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /CE#))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /WE#))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_CC-PublicDomain_SilkScreenTop_Big (layer B.Cu) (tedit 5A205720)
    (at 109.85 89.4)
    (descr "Symbol, CC-PublicDomain, SilkScreen Top, Big,")
    (tags "Symbol, CC-PublicDomain, SilkScreen Top, Big,")
    (fp_text reference REF** (at -8.75 -5.85) (layer Cmts.User) hide)
    (fp_text value Symbol_CC-PublicDomain_SilkScreenTop_Big (at 0.59944 -8.001) (layer B.Fab))
  )
  (module Symbols:ESD-Logo_8.9x8mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 108.75 109.2)
    (descr "Electrostatic discharge Logo")
    (tags "Logo ESD")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value ESD-Logo_8.9x8mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (gr_text A0 (at 88.65 83.75 270) (layer F.SilkS))
  (gr_text 1 (at 85.95 83.05 270) (layer F.SilkS))
  (gr_text 2 (at 82.85 86.1) (layer F.SilkS))
  (gr_text 3 (at 82.85 88.7) (layer F.SilkS))
  (gr_text 4 (at 82.85 91.2) (layer F.SilkS))
  (gr_text 5 (at 82.95 93.8) (layer F.SilkS))
  (gr_text 6 (at 83 96.45) (layer F.SilkS))
  (gr_text 7 (at 83.05 99) (layer F.SilkS))
  (gr_text 8 (at 83.05 101.4) (layer F.SilkS))
  (gr_text 9 (at 82.95 103.85) (layer F.SilkS))
  (gr_text 10 (at 83.5 106.65) (layer F.SilkS))
  (gr_text 11 (at 83.6 109.1) (layer F.SilkS))
  (gr_text 12 (at 83.4 111.7) (layer F.SilkS))
  (gr_text 13 (at 83.5 114.3) (layer F.SilkS))
  (gr_text 14 (at 85.95 116.4 270) (layer F.SilkS))
  (gr_text 15 (at 88.75 116.4 270) (layer F.SilkS))
  (gr_text 16 (at 91.2 116.35 270) (layer F.SilkS))
  (gr_text 17 (at 93.65 116.35 270) (layer F.SilkS))
  (gr_text 18 (at 96.45 116.25 270) (layer F.SilkS))
  (gr_text 19 (at 98.85 116.35 270) (layer F.SilkS))
  (gr_text 20 (at 101.25 116.25 270) (layer F.SilkS))
  (gr_text A21 (at 103.7 115.7 270) (layer F.SilkS))
  (gr_text DQ15 (at 106.35 114.65 270) (layer F.SilkS))
  (gr_text 14 (at 108.75 116.1 270) (layer F.SilkS))
  (gr_text 13 (at 111.4 116.2 270) (layer F.SilkS))
  (gr_text 12 (at 114 116.15 270) (layer F.SilkS))
  (gr_text 11 (at 116.7 114.15) (layer F.SilkS))
  (gr_text 10 (at 116.45 111.55) (layer F.SilkS))
  (gr_text 9 (at 116.85 108.9) (layer F.SilkS))
  (gr_text 8 (at 116.9 106.5) (layer F.SilkS))
  (gr_text 7 (at 116.95 103.85) (layer F.SilkS))
  (gr_text 6 (at 117 101.25) (layer F.SilkS))
  (gr_text 5 (at 117.1 98.6) (layer F.SilkS))
  (gr_text 4 (at 116.7 96.25) (layer F.SilkS))
  (gr_text 3 (at 116.8 93.9) (layer F.SilkS))
  (gr_text 2 (at 116.65 91.25) (layer F.SilkS))
  (gr_text 0 (at 116.7 86) (layer F.SilkS))
  (gr_text 1 (at 116.65 88.7) (layer F.SilkS))
  (gr_text "DQ0\n" (at 119.8 82.25) (layer F.SilkS))
  (gr_text WE# (at 113.8 84.65 270) (layer F.SilkS))
  (gr_text CE# (at 111.2 84.5 270) (layer F.SilkS))
  (gr_text ZZ# (at 108.75 84.8 270) (layer F.SilkS))
  (gr_text OE# (at 106.15 84.55 270) (layer F.SilkS))
  (gr_text LB# (at 103.75 84.45 270) (layer F.SilkS))
  (gr_text UB# (at 101.2 84.6 270) (layer F.SilkS))
  (gr_text VDDQ (at 98.55 85.3 270) (layer F.SilkS))
  (gr_text VSSQ (at 96 85.25 270) (layer F.SilkS))
  (gr_text VDD (at 93.45 84.55 270) (layer F.SilkS))
  (gr_text VSS (at 91 84.45 270) (layer F.SilkS))
  (gr_text "PSRAM Test V0" (at 100 90) (layer F.SilkS))
  (gr_line (start 75 125) (end 75 75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125 125) (end 75 125) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125 75) (end 125 125) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75 75) (end 125 75) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.571 96.952) (xy 96.952 96.952) (xy 96.952 95.936) (xy 97.968 95.936) (xy 97.968 95.555)
        (xy 96.571 95.555)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.571 103.048) (xy 96.952 103.048) (xy 96.952 104.064) (xy 97.968 104.064) (xy 97.968 104.445)
        (xy 96.571 104.445)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.032 104.445) (xy 103.429 104.445) (xy 103.429 103.048) (xy 103.048 103.048) (xy 103.048 104.064)
        (xy 102.032 104.064)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.032 95.555) (xy 103.429 95.555) (xy 103.429 96.952) (xy 103.048 96.952) (xy 103.048 95.936)
        (xy 102.032 95.936)
      )
    )
  )
  (zone (net 45) (net_name /VSS) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.125))
    (polygon
      (pts
        (xy 70 70) (xy 130 70) (xy 130 130) (xy 70 130)
      )
    )
  )
  (zone (net 4) (net_name /VSSQ) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.125))
    (polygon
      (pts
        (xy 70 70) (xy 130 70) (xy 130 130) (xy 70 130)
      )
    )
  )
)
