(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 62)
    (no_connects 0)
    (area 156.976 41.592499 229.02031 102.3608)
    (thickness 1.6)
    (drawings 15)
    (tracks 90)
    (zones 0)
    (modules 46)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 3.81)
    (trace_clearance 0.254)
    (zone_clearance 0.25146)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 2.032)
    (pad_drill 1.2954)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 "Net-(K1-Pad1)")
  (net 2 120VAC)
  (net 3 "Net-(K1-Pad3)")
  (net 4 Earth)
  (net 5 "Net-(M1-PadNC)")
  (net 6 "Net-(M1-PadIORE)")
  (net 7 "Net-(M1-PadSCL)")
  (net 8 "Net-(M1-PadSDA)")
  (net 9 "Net-(M1-Pad3V)")
  (net 10 +5V)
  (net 11 "Net-(M1-PadA0)")
  (net 12 "Net-(M1-PadA1)")
  (net 13 "Net-(M1-PadA2)")
  (net 14 "Net-(M1-PadA3)")
  (net 15 "Net-(M1-PadA4)")
  (net 16 "Net-(M1-PadA5)")
  (net 17 "Net-(M1-PadAREF)")
  (net 18 "Net-(M1-PadD0)")
  (net 19 "Net-(M1-PadD1)")
  (net 20 "Net-(M1-PadD2)")
  (net 21 "Net-(M1-PadD3)")
  (net 22 "Net-(M1-PadD4)")
  (net 23 "Net-(M1-PadD5)")
  (net 24 "Net-(M1-PadD6)")
  (net 25 "Net-(M1-PadD7)")
  (net 26 "Net-(M1-PadD8)")
  (net 27 "Net-(M1-PadD9)")
  (net 28 "Net-(M1-PadD10)")
  (net 29 "Net-(M1-PadD11)")
  (net 30 "Net-(M1-PadD12)")
  (net 31 "Net-(M1-PadD13)")
  (net 32 "Net-(M1-PadRESE)")
  (net 33 "Net-(M1-PadVIN)")
  (net 34 "Net-(Q1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net 120VAC)
    (add_net Earth)
    (add_net "Net-(K1-Pad1)")
    (add_net "Net-(K1-Pad3)")
    (add_net "Net-(M1-Pad3V)")
    (add_net "Net-(M1-PadA0)")
    (add_net "Net-(M1-PadA1)")
    (add_net "Net-(M1-PadA2)")
    (add_net "Net-(M1-PadA3)")
    (add_net "Net-(M1-PadA4)")
    (add_net "Net-(M1-PadA5)")
    (add_net "Net-(M1-PadAREF)")
    (add_net "Net-(M1-PadD0)")
    (add_net "Net-(M1-PadD1)")
    (add_net "Net-(M1-PadD10)")
    (add_net "Net-(M1-PadD11)")
    (add_net "Net-(M1-PadD12)")
    (add_net "Net-(M1-PadD13)")
    (add_net "Net-(M1-PadD2)")
    (add_net "Net-(M1-PadD3)")
    (add_net "Net-(M1-PadD4)")
    (add_net "Net-(M1-PadD5)")
    (add_net "Net-(M1-PadD6)")
    (add_net "Net-(M1-PadD7)")
    (add_net "Net-(M1-PadD8)")
    (add_net "Net-(M1-PadD9)")
    (add_net "Net-(M1-PadIORE)")
    (add_net "Net-(M1-PadNC)")
    (add_net "Net-(M1-PadRESE)")
    (add_net "Net-(M1-PadSCL)")
    (add_net "Net-(M1-PadSDA)")
    (add_net "Net-(M1-PadVIN)")
    (add_net "Net-(Q1-Pad2)")
  )
  (module thermostat:transistor (layer F.Cu) (tedit 5ADE7100)
    (at 182.753 54.737 270)
    (fp_text reference Q1 (at 0.254 2.032 270) (layer F.SilkS))
    (fp_text value PN2222A (at 0.1 7.6 270) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 0 -2 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at -2 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(K1-Pad1)"))
    (pad 3 thru_hole circle (at 2 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (model Transistors_OldSowjetAera.3dshapes/OldSowjetaera_Transistor_Type-II_SmallPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module thermostat:R_0.2 (layer F.Cu) (tedit 5ADD26D5)
    (at 211.2645 67.945 270)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr virtual)
    (fp_text reference R1 (at -4.5085 -0.127 360) (layer F.SilkS))
    (fp_text value 100k (at 0.8382 1.81356 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.9304 1.9304) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 "Net-(M1-PadA1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.9304 1.9304) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 +5V))
  )
  (module thermostat:R_0.2 (layer F.Cu) (tedit 5ADD26D5)
    (at 211.328 79.756 90)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr virtual)
    (fp_text reference R2 (at -4.5085 -0.127 180) (layer F.SilkS))
    (fp_text value 100k (at 0.8382 1.81356 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.9304 1.9304) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.9304 1.9304) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 "Net-(M1-PadA2)"))
  )
  (module thermostat:R_0.2 (layer F.Cu) (tedit 5ADD26D5)
    (at 189.357 55.118 90)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr virtual)
    (fp_text reference R4 (at -4.5085 -0.127 180) (layer F.SilkS))
    (fp_text value 1k (at 0.8382 1.81356 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.9304 1.9304) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.9304 1.9304) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "Net-(M1-PadD9)"))
  )
  (module thermostat:Buzzer-6.5mm (layer F.Cu) (tedit 5ADE719D)
    (at 194.437 55.626)
    (fp_text reference U1 (at 0.127 2.159) (layer F.SilkS))
    (fp_text value Buzzer (at 3.556 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(M1-PadD8)"))
    (pad 2 thru_hole circle (at 6.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 Earth))
  )
  (module thermostat:2-pin-0.2 (layer F.Cu) (tedit 5ADE6B83)
    (at 163.3855 90.7415)
    (fp_text reference U6 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value 2-pin-0.2 (at -0.1905 -2.4765) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 2.032 2.032) (drill 1.2954) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.032 2.032) (drill 1.2954) (layers *.Cu *.Mask)
      (net 4 Earth))
  )
  (module thermostat:2-pin-0.2 (layer F.Cu) (tedit 5ADE6256)
    (at 164.211 45.974 180)
    (fp_text reference U5 (at 0 0.5 180) (layer F.SilkS) hide)
    (fp_text value 2-pin-0.2 (at -0.1905 -2.4765 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 2.032 2.032) (drill 1.2954) (layers *.Cu *.Mask)
      (net 2 120VAC))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.032 2.032) (drill 1.2954) (layers *.Cu *.Mask)
      (net 3 "Net-(K1-Pad3)"))
  )
  (module thermostat:2-pin-0.2 (layer F.Cu) (tedit 5ADE6256)
    (at 217.805 79.756 90)
    (fp_text reference U4 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value 2-pin-0.2 (at -0.1905 -2.4765 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2.032 2.032) (drill 1.2954) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.032 2.032) (drill 1.2954) (layers *.Cu *.Mask)
      (net 13 "Net-(M1-PadA2)"))
  )
  (module thermostat:2-pin-0.2 (layer F.Cu) (tedit 5ADE6256)
    (at 217.805 67.945 90)
    (fp_text reference U3 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value 2-pin-0.2 (at -0.1905 -2.4765 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2.032 2.032) (drill 1.2954) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.032 2.032) (drill 1.2954) (layers *.Cu *.Mask)
      (net 12 "Net-(M1-PadA1)"))
  )
  (module thermostat:AC-DC-RAC01-GA (layer F.Cu) (tedit 5ADE7104)
    (at 160.528 79.883)
    (fp_text reference U2 (at 0 -7.62 90) (layer F.SilkS))
    (fp_text value AC-DC-Converter (at 15.367 -7.493) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 120VAC))
    (pad 2 thru_hole circle (at 0 -15.24) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad 3 thru_hole circle (at 27.94 -15.24) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad 4 thru_hole circle (at 27.94 -7.62) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 +5V))
  )
  (module thermostat:Relay-SPST-0.3-0.4 (layer F.Cu) (tedit 5ADE70FB)
    (at 177.038 52.578 180)
    (fp_text reference K1 (at 0 -3.81 270) (layer F.SilkS))
    (fp_text value RELAY_SPST (at 0 -0.5 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(K1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 120VAC))
    (pad 3 thru_hole circle (at 17.78 0 180) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(K1-Pad3)"))
    (pad 5 thru_hole circle (at 0 -7.62 180) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 Earth))
  )
  (module thermostat:ARDUINOR3-JFA locked (layer F.Cu) (tedit 5ADE69A9)
    (at 157.48 95.25)
    (descr "ARDUINO UNO R3 JFA")
    (tags "ARDUINO UNO")
    (attr virtual)
    (fp_text reference M1 (at 2.794 -9.398) (layer Cmts.User) hide)
    (fp_text value ARDUINOUNOR3-JFA (at 41.91 5.715) (layer Eco2.User) hide)
    (fp_text user IOref (at 29.972 -0.762) (layer F.SilkS))
    (fp_text user SDA (at 21.2725 -52.324) (layer F.SilkS))
    (fp_text user SCL (at 18.796 -52.324) (layer F.SilkS))
    (fp_text user Rst (at 33.274 -0.762) (layer F.SilkS))
    (fp_text user 3v3 (at 36.068 -0.762) (layer F.SilkS))
    (fp_text user 5v (at 38.608 -0.762) (layer F.SilkS))
    (fp_text user Gnd (at 41.91 -0.762) (layer F.SilkS))
    (fp_text user Vin (at 45.974 -0.762) (layer F.SilkS))
    (fp_text user A0 (at 50.8 -0.762) (layer F.SilkS))
    (fp_text user A1 (at 53.34 -0.762) (layer F.SilkS))
    (fp_text user A2 (at 55.88 -0.762) (layer F.SilkS))
    (fp_text user A3 (at 58.42 -0.762) (layer F.SilkS))
    (fp_text user A4 (at 60.96 -0.762) (layer F.SilkS))
    (fp_text user A5 (at 63.5 -0.762) (layer F.SilkS))
    (fp_text user ARef (at 24.003 -52.324) (layer F.SilkS))
    (fp_text user Gnd (at 26.543 -52.324) (layer F.SilkS))
    (fp_text user D13 (at 29.083 -52.324) (layer F.SilkS))
    (fp_text user D12 (at 31.623 -52.324) (layer F.SilkS))
    (fp_text user D11 (at 34.163 -52.324) (layer F.SilkS))
    (fp_text user D10 (at 36.703 -52.324) (layer F.SilkS))
    (fp_text user D9 (at 39.243 -52.324) (layer F.SilkS))
    (fp_text user D8 (at 41.783 -52.324) (layer F.SilkS))
    (fp_text user D7 (at 45.847 -52.324) (layer F.SilkS))
    (fp_text user D6 (at 48.387 -52.324) (layer F.SilkS))
    (fp_text user D5 (at 50.927 -52.324) (layer F.SilkS))
    (fp_text user D4 (at 53.467 -52.324) (layer F.SilkS))
    (fp_text user D3 (at 56.007 -52.324) (layer F.SilkS))
    (fp_text user D2 (at 58.547 -52.324) (layer F.SilkS))
    (fp_text user D1 (at 61.08446 -52.324) (layer F.SilkS))
    (fp_text user D0 (at 63.754 -52.324) (layer F.SilkS))
    (fp_text user "Digital I/O" (at 36.211 -61.578) (layer Cmts.User))
    (fp_text user "Digital I/O" (at 55.515 -61.578) (layer Cmts.User))
    (pad NC thru_hole circle (at 27.94 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 5 "Net-(M1-PadNC)"))
    (pad IORE thru_hole circle (at 30.48 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 6 "Net-(M1-PadIORE)"))
    (pad SCL thru_hole circle (at 18.796 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 7 "Net-(M1-PadSCL)"))
    (pad SDA thru_hole circle (at 21.336 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 8 "Net-(M1-PadSDA)"))
    (pad 3V thru_hole circle (at 35.56 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 9 "Net-(M1-Pad3V)"))
    (pad 5V thru_hole circle (at 38.1 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad A0 thru_hole circle (at 50.8 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 11 "Net-(M1-PadA0)"))
    (pad A1 thru_hole circle (at 53.34 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 12 "Net-(M1-PadA1)"))
    (pad A2 thru_hole circle (at 55.88 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 13 "Net-(M1-PadA2)"))
    (pad A3 thru_hole circle (at 58.42 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 14 "Net-(M1-PadA3)"))
    (pad A4 thru_hole circle (at 60.96 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 15 "Net-(M1-PadA4)"))
    (pad A5 thru_hole circle (at 63.5 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 16 "Net-(M1-PadA5)"))
    (pad AREF thru_hole circle (at 23.876 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 17 "Net-(M1-PadAREF)"))
    (pad D0 thru_hole circle (at 63.5 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 18 "Net-(M1-PadD0)"))
    (pad D1 thru_hole circle (at 60.96 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 19 "Net-(M1-PadD1)"))
    (pad D2 thru_hole circle (at 58.42 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 20 "Net-(M1-PadD2)"))
    (pad D3 thru_hole circle (at 55.88 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 21 "Net-(M1-PadD3)"))
    (pad D4 thru_hole circle (at 53.34 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 22 "Net-(M1-PadD4)"))
    (pad D5 thru_hole circle (at 50.8 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 23 "Net-(M1-PadD5)"))
    (pad D6 thru_hole circle (at 48.26 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 24 "Net-(M1-PadD6)"))
    (pad D7 thru_hole circle (at 45.72 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 25 "Net-(M1-PadD7)"))
    (pad D8 thru_hole circle (at 41.656 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 26 "Net-(M1-PadD8)"))
    (pad D9 thru_hole circle (at 39.116 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 27 "Net-(M1-PadD9)"))
    (pad D10 thru_hole circle (at 36.576 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 28 "Net-(M1-PadD10)"))
    (pad D11 thru_hole circle (at 34.036 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 29 "Net-(M1-PadD11)"))
    (pad D12 thru_hole circle (at 31.496 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 30 "Net-(M1-PadD12)"))
    (pad D13 thru_hole circle (at 28.95346 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 31 "Net-(M1-PadD13)"))
    (pad GND thru_hole circle (at 26.416 -50.8) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad GND1 thru_hole circle (at 43.18 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad GND2 thru_hole circle (at 40.64 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad RESE thru_hole circle (at 33.02 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 32 "Net-(M1-PadRESE)"))
    (pad VIN thru_hole circle (at 45.72 -2.54) (size 1.6764 1.6764) (drill 0.99822) (layers *.Cu *.Mask)
      (net 33 "Net-(M1-PadVIN)"))
  )
  (module thermostat:Potentiometer_VishaySpectrol-Econtrim-Type36T (layer F.Cu) (tedit 5ADE6A57)
    (at 214.376 60.325)
    (descr "Potentiometer, Trimmer, Spectrol Type 36T, Econtrim, Rev A, 02 Aug 2010,")
    (tags "Potentiometer, Trimmer, Spectrol Type 36T, Econtrim, Rev A, 02 Aug 2010,")
    (fp_text reference R5 (at 2.667 -8.001) (layer F.SilkS))
    (fp_text value POT (at 2.667 2.794) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.49936 -4.99872) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 4.99872 0) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask)
      (net 10 +5V))
  )
  (module thermostat:Potentiometer_VishaySpectrol-Econtrim-Type36T (layer F.Cu) (tedit 5ADE70D8)
    (at 203.708 76.327 180)
    (descr "Potentiometer, Trimmer, Spectrol Type 36T, Econtrim, Rev A, 02 Aug 2010,")
    (tags "Potentiometer, Trimmer, Spectrol Type 36T, Econtrim, Rev A, 02 Aug 2010,")
    (fp_text reference R3 (at 2.667 -8.001 180) (layer F.SilkS))
    (fp_text value POT (at 2.667 2.794 180) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.49936 -4.99872 180) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask)
      (net 11 "Net-(M1-PadA0)"))
    (pad 3 thru_hole circle (at 4.99872 0 180) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask)
      (net 10 +5V))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 220.98 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD32 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(M1-PadA5)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 218.44 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD31 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(M1-PadA4)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 220.98 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD30 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(M1-PadD0)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 215.9 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD29 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(M1-PadA3)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 218.44 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD28 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(M1-PadD1)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 213.36 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD27 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(M1-PadA2)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 215.9 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD26 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(M1-PadD2)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 210.82 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD25 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(M1-PadA1)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 213.36 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD24 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(M1-PadD3)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 208.28 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD23 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(M1-PadA0)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 210.82 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD22 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(M1-PadD4)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 208.28 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD21 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(M1-PadD5)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 203.2 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD20 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(M1-PadVIN)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 205.74 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD19 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(M1-PadD6)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 200.66 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD18 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 Earth))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 203.2 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD17 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(M1-PadD7)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 198.12 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD16 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 Earth))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 195.58 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD15 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 +5V))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 199.136 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD14 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(M1-PadD8)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 193.04 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD13 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(M1-Pad3V)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 196.596 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD12 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(M1-PadD9)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 190.5 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD11 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(M1-PadRESE)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 194.056 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD10 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(M1-PadD10)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 187.96 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD9 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(M1-PadIORE)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 191.516 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD8 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(M1-PadD11)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 185.42 90.17)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD7 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(M1-PadNC)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 188.976 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD6 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(M1-PadD12)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 186.436 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD5 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(M1-PadD13)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 183.896 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD4 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 Earth))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 181.356 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD3 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(M1-PadAREF)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 178.816 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD2 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(M1-PadSDA)"))
  )
  (module thermostat:2_15_1_0 (layer F.Cu) (tedit 5ADE6B53)
    (at 176.276 46.99)
    (descr "THROUGH-HOLE PAD")
    (tags "THROUGH-HOLE PAD")
    (attr virtual)
    (fp_text reference PAD1 (at 4.699 1.143) (layer B.SilkS) hide)
    (fp_text value WIREPAD2_15_1_0 (at 0.0762 -1.01092) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(M1-PadSCL)"))
  )
  (gr_line (start 223.52 92.71) (end 223.52 54.991) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 223.52 95.25) (end 157.48 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 223.52 92.71) (end 223.52 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 223.52 43.434) (end 223.52 54.864) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 221.996 41.91) (end 223.52 43.434) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 221.488 41.91) (end 221.996 41.91) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.48 41.91) (end 221.615 41.91) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.48 95.25) (end 157.48 41.91) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "LCD\nContrast" (at 210.185 58.42 90) (layer F.SilkS))
  (gr_text Tuning (at 201.422 73.279) (layer F.SilkS))
  (gr_text "Sensor 2" (at 208.8515 79.502 90) (layer F.SilkS))
  (gr_text "Sensor 1" (at 208.8515 67.945 90) (layer F.SilkS))
  (gr_text "AC Neutral\nIn/Out" (at 163.576 84.709) (layer F.SilkS))
  (gr_text "AC Hot Out" (at 158.115 46.609 270) (layer F.SilkS))
  (gr_text "AC Hot In" (at 170.307 45.974 270) (layer F.SilkS))
  (zone (net 10) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25146))
    (min_thickness 0.25146)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 223.012 43.434) (xy 223.012 55.626) (xy 222.504 92.71) (xy 222.504 93.472) (xy 221.488 94.488)
        (xy 176.2125 94.488) (xy 175.26 93.472) (xy 175.26 73.152) (xy 175.26 43.688) (xy 176.53 42.418)
        (xy 221.996 42.418)
      )
    )
  )
  (zone (net 4) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25146))
    (min_thickness 0.25146)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 223.012 43.434) (xy 223.012 55.626) (xy 222.504 92.71) (xy 222.504 93.472) (xy 221.488 94.488)
        (xy 176.2125 94.488) (xy 175.26 93.472) (xy 175.26 73.152) (xy 175.26 43.688) (xy 176.53 42.418)
        (xy 221.996 42.418)
      )
    )
  )
)
