(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 18)
    (zones 0)
    (modules 5)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 109.347 90.17)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /LDCathode)
  (net 2 /LDAnode)
  (net 3 /TEC+Control)
  (net 4 /Therm1)
  (net 5 /Therm2)
  (net 6 "Net-(LDButterflyPins1-Pad4)")
  (net 7 "Net-(LDButterflyPins1-Pad3)")
  (net 8 /TEC-)
  (net 9 GND)
  (net 10 "Net-(LDButterflyPins1-Pad8)")
  (net 11 /TEC+)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /LDAnode)
    (add_net /LDCathode)
    (add_net /TEC+)
    (add_net /TEC+Control)
    (add_net /TEC-)
    (add_net /Therm1)
    (add_net /Therm2)
    (add_net GND)
    (add_net "Net-(LDButterflyPins1-Pad3)")
    (add_net "Net-(LDButterflyPins1-Pad4)")
    (add_net "Net-(LDButterflyPins1-Pad8)")
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 117 81)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference Therm1 (at 1.27 -4.12) (layer F.SilkS))
    (fp_text value Therm1 (at 1.27 4.08) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 /Therm2))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 4 /Therm1))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 113.919 72 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference TEC1 (at 1.27 -4.12) (layer F.SilkS))
    (fp_text value TEC1 (at 1.27 4.08) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 /TEC-))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 11 /TEC+))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 112 82 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 /TEC+))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 /TEC+Control))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyFootprints:InnolumeButterflyGainChipPins (layer F.Cu) (tedit 5D7A6BB6)
    (at 115.826999 76.818999)
    (fp_text reference LDButterflyPins1 (at 0.124001 9.795001) (layer F.SilkS))
    (fp_text value LDButterflyPins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 11.938) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 /TEC+Control))
    (pad 2 thru_hole circle (at -2.54 11.938) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 /Therm1))
    (pad 5 thru_hole circle (at 5.08 11.938) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 /Therm2))
    (pad 4 thru_hole circle (at 2.54 11.938) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(LDButterflyPins1-Pad4)"))
    (pad 3 thru_hole circle (at 0 11.938) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(LDButterflyPins1-Pad3)"))
    (pad 10 thru_hole circle (at -5.08 -11.938) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 /TEC-))
    (pad 9 thru_hole circle (at -2.54 -11.938) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 6 thru_hole circle (at 5.08 -11.938) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 /LDAnode))
    (pad 7 thru_hole circle (at 2.54 -11.938) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 /LDCathode))
    (pad 8 thru_hole circle (at 0 -11.938) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(LDButterflyPins1-Pad8)"))
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 120.142 72 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference LaserDiode1 (at 2.525 4.055) (layer F.SilkS))
    (fp_text value LaserDiode1 (at 1.27 4.08) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 /LDCathode))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 2 /LDAnode))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 10 (at 110.744 67.056) (layer B.SilkS))
  (gr_text 9 (at 113.284 67.056) (layer B.SilkS))
  (gr_text 8 (at 115.824 67.056) (layer B.SilkS))
  (gr_text 7 (at 118.364 67.056) (layer B.SilkS))
  (gr_text 6 (at 120.904 67.056) (layer B.SilkS))
  (gr_text 5 (at 120.904 86.741) (layer B.SilkS))
  (gr_text 4 (at 118.364 86.741) (layer B.SilkS))
  (gr_text 3 (at 115.824 86.741) (layer B.SilkS))
  (gr_text 2 (at 113.284 86.741) (layer B.SilkS))
  (gr_text 1 (at 110.744 86.741) (layer B.SilkS))
  (gr_text TEC+ (at 111.887 78.867) (layer F.SilkS))
  (gr_text TEC- (at 110.871 67.818 90) (layer F.SilkS))
  (gr_text A+ (at 120.142 75.692) (layer F.SilkS))
  (gr_text C- (at 117.221 75.692) (layer F.SilkS))
  (gr_line (start 109.347 63.5) (end 122.301 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109.347 90.17) (end 109.347 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.301 90.17) (end 109.347 90.17) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.301 63.5) (end 122.301 90.17) (layer Edge.Cuts) (width 0.05))
  (zone (net 9) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.347 63.5) (xy 122.301 63.5) (xy 122.301 90.17) (xy 109.347 90.17)
      )
    )
  )
  (zone (net 9) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.347 63.5) (xy 122.301 63.5) (xy 122.301 90.17) (xy 109.347 90.17)
      )
    )
  )
)
