(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A2")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "V_out")
  (net 2 "Earth")
  (net 3 "V_in")
  (net 4 "Net-(C13-Pad2)")
  (net 5 "Net-(C14-Pad2)")
  (net 6 "Net-(C15-Pad2)")
  (net 7 "Net-(C16-Pad2)")
  (net 8 "Net-(C17-Pad2)")
  (net 9 "Net-(C18-Pad2)")
  (net 10 "Net-(C19-Pad2)")
  (net 11 "Net-(C20-Pad2)")
  (net 12 "Net-(C21-Pad2)")
  (net 13 "Net-(C24-Pad2)")
  (net 14 "Net-(C25-Pad2)")
  (net 15 "Net-(C26-Pad2)")
  (net 16 "Net-(C27-Pad2)")
  (net 17 "Net-(C28-Pad2)")
  (net 18 "Net-(C29-Pad2)")
  (net 19 "Net-(C30-Pad2)")
  (net 20 "Net-(C31-Pad2)")
  (net 21 "Net-(C32-Pad2)")
  (net 22 "Net-(C35-Pad2)")
  (net 23 "Net-(C36-Pad2)")
  (net 24 "Net-(C37-Pad2)")
  (net 25 "Net-(C38-Pad2)")
  (net 26 "Net-(C39-Pad2)")
  (net 27 "Net-(C40-Pad2)")
  (net 28 "Net-(C41-Pad2)")
  (net 29 "Net-(C42-Pad2)")
  (net 30 "Net-(C43-Pad2)")
  (net 31 "Net-(C46-Pad2)")
  (net 32 "Net-(C47-Pad2)")
  (net 33 "Net-(C48-Pad2)")
  (net 34 "Net-(C49-Pad2)")
  (net 35 "Net-(C50-Pad2)")
  (net 36 "Net-(C51-Pad2)")
  (net 37 "Net-(C52-Pad2)")
  (net 38 "Net-(C53-Pad2)")
  (net 39 "Net-(C54-Pad2)")
  (net 40 "Net-(C57-Pad2)")
  (net 41 "Net-(C58-Pad2)")
  (net 42 "Net-(C59-Pad2)")
  (net 43 "Net-(C60-Pad2)")
  (net 44 "Net-(C61-Pad2)")
  (net 45 "Net-(C62-Pad2)")
  (net 46 "Net-(C63-Pad2)")
  (net 47 "Net-(C64-Pad2)")
  (net 48 "Net-(C65-Pad2)")
  (net 49 "Net-(C68-Pad2)")
  (net 50 "Net-(C69-Pad2)")
  (net 51 "Net-(C70-Pad2)")
  (net 52 "Net-(C71-Pad2)")
  (net 53 "Net-(C72-Pad2)")
  (net 54 "Net-(C73-Pad2)")
  (net 55 "Net-(C74-Pad2)")
  (net 56 "Net-(C75-Pad2)")
  (net 57 "Net-(C76-Pad2)")
  (net 58 "Net-(C79-Pad2)")
  (net 59 "Net-(C80-Pad2)")
  (net 60 "Net-(C81-Pad2)")
  (net 61 "Net-(C82-Pad2)")
  (net 62 "Net-(C83-Pad2)")
  (net 63 "Net-(C84-Pad2)")
  (net 64 "Net-(C85-Pad2)")
  (net 65 "Net-(C86-Pad2)")
  (net 66 "Net-(C87-Pad2)")
  (net 67 "Net-(C90-Pad2)")
  (net 68 "Net-(C91-Pad2)")
  (net 69 "Net-(C92-Pad2)")
  (net 70 "Net-(C93-Pad2)")
  (net 71 "Net-(C94-Pad2)")
  (net 72 "Net-(C95-Pad2)")
  (net 73 "Net-(C96-Pad2)")
  (net 74 "Net-(C97-Pad2)")
  (net 75 "Net-(C98-Pad2)")
  (net 76 "Net-(C101-Pad2)")
  (net 77 "Net-(C102-Pad2)")
  (net 78 "Net-(C103-Pad2)")
  (net 79 "Net-(C104-Pad2)")
  (net 80 "Net-(C105-Pad2)")
  (net 81 "Net-(C106-Pad2)")
  (net 82 "Net-(C107-Pad2)")
  (net 83 "Net-(C108-Pad2)")
  (net 84 "Net-(C109-Pad2)")
  (net 85 "Net-(C2-Pad2)")
  (net 86 "Net-(C3-Pad2)")
  (net 87 "Net-(C4-Pad2)")
  (net 88 "Net-(C5-Pad2)")
  (net 89 "Net-(C6-Pad2)")
  (net 90 "Net-(C7-Pad2)")
  (net 91 "Net-(C8-Pad2)")
  (net 92 "Net-(C10-Pad1)")
  (net 93 "Net-(C10-Pad2)")
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.753615 62.23)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C18" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 8 "Net-(C17-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 9 "Net-(C18-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.742223 188.773328)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper95" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 79 "Net-(C104-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 80 "Net-(C105-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.197777 139.471664)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper67" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "Net-(C73-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 55 "Net-(C74-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.671115 159.106664)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H12" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.753615 78.663888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C29" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 17 "Net-(C28-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 18 "Net-(C29-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.831115 139.471664)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper61" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 49 "Net-(C68-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 245.11 138.04944 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J7" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.208615 95.097776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C44" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 30 "Net-(C43-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.671115 191.97444)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H14" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.473615 111.531664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C46" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 31 "Net-(C46-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.33 111.531664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C45" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.243615 144.39944)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C72" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 52 "Net-(C71-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 53 "Net-(C72-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.842503 127.965552)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C58" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 40 "Net-(C57-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 41 "Net-(C58-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.653331 73.736112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper29" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(C31-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(C32-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.473615 62.23)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C13" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "Net-(C13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.33 144.39944)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C67" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.671115 142.672776)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H11" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 245.11 55.88 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J2" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.79 90.17)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.197777 123.037776)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper57" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(C62-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(C63-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 76.058892 139.471664)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper62" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 49 "Net-(C68-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 50 "Net-(C69-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.85 46.176664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 92 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 93 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.991115 95.097776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C43" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 29 "Net-(C42-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 30 "Net-(C43-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.211391 95.097776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C37" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 23 "Net-(C36-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 24 "Net-(C37-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.653331 57.302224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper19" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(C20-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(C21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.208615 144.39944)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C77" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 57 "Net-(C76-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.653331 172.33944)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper89" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 74 "Net-(C97-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 75 "Net-(C98-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.286669 106.603888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper43" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(C47-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(C48-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.197777 172.33944)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper87" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 72 "Net-(C95-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 73 "Net-(C96-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.971115 78.663888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C30" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 18 "Net-(C29-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 19 "Net-(C30-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.991115 177.267216)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C98" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 74 "Net-(C97-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 75 "Net-(C98-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.211391 193.701104)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C103" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 77 "Net-(C102-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 78 "Net-(C103-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.671115 175.540552)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H13" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_3.5mm_Pad_Via" (layer "F.Cu")
    (at 255.953845 33.703845)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (property "Sheetfile" "Bias Voltage Divider.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.625 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -2.625) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 2.625) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.625 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.97 188.773328)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper96" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 80 "Net-(C105-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 81 "Net-(C106-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.971115 144.39944)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C74" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 54 "Net-(C73-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 55 "Net-(C74-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.753615 127.965552)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C62" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 44 "Net-(C61-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 45 "Net-(C62-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.971115 127.965552)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C63" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 45 "Net-(C62-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 46 "Net-(C63-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.514446 155.905552)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper74" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(C81-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 61 "Net-(C82-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.34 46.176664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 91 "Net-(C8-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 92 "Net-(C10-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.473615 144.39944)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C68" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 49 "Net-(C68-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.211391 177.267216)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C92" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 68 "Net-(C91-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 69 "Net-(C92-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.211391 127.965552)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C59" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 41 "Net-(C58-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 42 "Net-(C59-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.831115 90.17)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper31" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(C35-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.580279 127.965552)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C60" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 42 "Net-(C59-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 43 "Net-(C60-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.425554 188.773328)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper98" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 82 "Net-(C107-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 83 "Net-(C108-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.49 167.25944 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D9" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.211391 62.23)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C15" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "Net-(C14-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 6 "Net-(C15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.53 44.45)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H5" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.208615 177.267216)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C99" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 75 "Net-(C98-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.881115 123.037776)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper60" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "Net-(C65-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.197777 73.736112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper27" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(C29-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(C30-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.425554 73.736112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper28" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(C30-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(C31-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.243615 111.531664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C50" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 34 "Net-(C49-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 35 "Net-(C50-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.208615 111.531664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C55" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 39 "Net-(C54-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.991115 160.833328)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C87" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 65 "Net-(C86-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 66 "Net-(C87-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.828885 41.248888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper6" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 89 "Net-(C6-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 90 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.0675 46.176664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 93 "Net-(C10-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.97 139.471664)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper66" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 53 "Net-(C72-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "Net-(C73-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.33 193.701104)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C100" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.831115 155.905552)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper71" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(C79-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.971115 193.701104)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C107" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 81 "Net-(C106-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 82 "Net-(C107-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.33 78.663888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C23" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.842503 78.663888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C25" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 13 "Net-(C24-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "Net-(C25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.580279 144.39944)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C71" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 51 "Net-(C70-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 52 "Net-(C71-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 245.11 72.313888 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J3" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.208615 160.833328)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C88" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 66 "Net-(C87-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm_Pad_Via" (layer "F.Cu")
    (at 31.163845 34.973845)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (property "Sheetfile" "Bias Voltage Divider.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.625 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -2.625) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 2.625) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.625 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.425554 155.905552)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper78" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 64 "Net-(C85-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 65 "Net-(C86-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.842503 111.531664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C47" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 31 "Net-(C46-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 32 "Net-(C47-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.425554 106.603888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper48" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(C52-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(C53-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.842503 144.39944)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C69" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 49 "Net-(C68-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 50 "Net-(C69-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.648885 41.248888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.671115 109.805)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H9" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.439164 46.176664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 87 "Net-(C4-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 88 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.514446 123.037776)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper54" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(C59-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "Net-(C60-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.653331 155.905552)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper79" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 65 "Net-(C86-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 66 "Net-(C87-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.881115 90.17)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper40" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(C43-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.286669 188.773328)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper93" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 77 "Net-(C102-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 78 "Net-(C103-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.197777 57.302224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper17" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(C18-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(C19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.653331 106.603888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper49" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(C53-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(C54-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 245.11 154.483328 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J8" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.425554 139.471664)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper68" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 55 "Net-(C74-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(C75-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.481115 160.833328)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C86" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 64 "Net-(C85-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 65 "Net-(C86-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.49 101.523888 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D5" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.97 57.302224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper16" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(C17-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(C18-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.97 172.33944)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper86" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 71 "Net-(C94-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 72 "Net-(C95-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 76.058892 123.037776)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper52" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(C57-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(C58-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.211391 78.663888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C26" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "Net-(C25-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 15 "Net-(C26-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.286669 172.33944)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper83" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 68 "Net-(C91-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 69 "Net-(C92-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.831115 172.33944)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper81" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 67 "Net-(C90-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.671115 76.937224)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H7" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.881115 57.302224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper20" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(C21-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.842503 62.23)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C14" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "Net-(C13-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "Net-(C14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.742223 123.037776)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper55" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "Net-(C60-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "Net-(C61-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.514446 188.773328)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper94" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 78 "Net-(C103-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 79 "Net-(C104-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.971115 95.097776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C41" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 27 "Net-(C40-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 28 "Net-(C41-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.580279 111.531664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C49" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 33 "Net-(C48-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 34 "Net-(C49-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.243615 62.23)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C17" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 7 "Net-(C16-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 8 "Net-(C17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.514446 73.736112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper24" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(C26-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(C27-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.243615 160.833328)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C83" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 61 "Net-(C82-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 62 "Net-(C83-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.49 51.408888 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D2" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.580279 95.097776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C38" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 24 "Net-(C37-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 25 "Net-(C38-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.33 177.267216)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C89" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.286669 155.905552)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper73" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 59 "Net-(C80-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(C81-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.653331 123.037776)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper59" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(C64-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "Net-(C65-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.74 41.248888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper10" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 93 "Net-(C10-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.842503 160.833328)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C80" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 58 "Net-(C79-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 59 "Net-(C80-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.473615 78.663888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C24" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 13 "Net-(C24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 76.058892 90.17)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper32" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(C35-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(C36-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.742223 73.736112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper25" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(C27-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(C28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.991115 193.701104)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C109" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 83 "Net-(C108-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 84 "Net-(C109-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.831115 106.603888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper41" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(C46-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.842503 177.267216)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C91" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 67 "Net-(C90-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 68 "Net-(C91-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.601108 41.248888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper5" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(C5-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 89 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.49 150.825552 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D8" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.1025 46.176664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 88 "Net-(C5-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 89 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.6125 46.176664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 89 "Net-(C6-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 90 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.842503 193.701104)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C102" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 76 "Net-(C101-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 77 "Net-(C102-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.881115 155.905552)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper80" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 66 "Net-(C87-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.481115 78.663888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C31" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 19 "Net-(C30-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 20 "Net-(C31-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.284439 41.248888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper8" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "Net-(C8-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 92 "Net-(C10-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.514446 106.603888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper44" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(C48-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(C49-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.514446 90.17)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper34" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(C37-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(C38-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.425554 90.17)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper38" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(C41-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(C42-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.425554 57.302224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper18" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(C19-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(C20-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.481115 62.23)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C20" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 10 "Net-(C19-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 11 "Net-(C20-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.473615 177.267216)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C90" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 67 "Net-(C90-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.831115 73.736112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper21" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(C24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.97 73.736112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper26" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(C28-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(C29-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 76.058892 106.603888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper42" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(C46-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(C47-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.580279 78.663888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C27" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 15 "Net-(C26-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 16 "Net-(C27-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.473615 193.701104)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C101" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 76 "Net-(C101-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.831115 57.302224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper11" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(C13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.671115 60.503336)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H6" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.243615 177.267216)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C94" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 70 "Net-(C93-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 71 "Net-(C94-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.481115 193.701104)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C108" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 82 "Net-(C107-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 83 "Net-(C108-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.348885 36.168888 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D1" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.208615 78.663888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C33" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 21 "Net-(C32-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.514446 57.302224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper14" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C15-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(C16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 245.11 105.181664 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J5" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 76.058892 172.33944)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper82" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 67 "Net-(C90-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 68 "Net-(C91-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.481115 111.531664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C53" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 37 "Net-(C52-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 38 "Net-(C53-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 245.11 170.917216 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J9" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.188885 46.176664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.991115 127.965552)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C65" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 47 "Net-(C64-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 48 "Net-(C65-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.425554 123.037776)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper58" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(C63-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(C64-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.79 73.736112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.79 57.302224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.69 41.248888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper1" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 85 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.197777 90.17)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper37" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(C40-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(C41-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.49 134.391664 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D7" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.211391 111.531664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C48" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 32 "Net-(C47-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 33 "Net-(C48-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.580279 177.267216)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C93" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 69 "Net-(C92-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 70 "Net-(C93-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.49 183.693328 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D10" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.97 106.603888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper46" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(C50-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(C51-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.373331 41.248888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper4" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 87 "Net-(C4-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.580279 160.833328)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C82" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 60 "Net-(C81-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 61 "Net-(C82-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 245.11 88.747776 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J4" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.753615 144.39944)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C73" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 53 "Net-(C72-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 54 "Net-(C73-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.991115 62.23)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C21" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 11 "Net-(C20-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 12 "Net-(C21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.481115 177.267216)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C97" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 73 "Net-(C96-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 74 "Net-(C97-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.33 127.965552)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C56" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 75.917777 41.248888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper2" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 85 "Net-(C2-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 86 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.881115 172.33944)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper90" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 75 "Net-(C98-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.701388 46.176664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 85 "Net-(C2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 86 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.753615 160.833328)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C84" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 62 "Net-(C83-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 63 "Net-(C84-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.653331 188.773328)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper99" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 83 "Net-(C108-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 84 "Net-(C109-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.473615 127.965552)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C57" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 40 "Net-(C57-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.473615 160.833328)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C79" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 58 "Net-(C79-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 76.058892 57.302224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper12" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(C13-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(C14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.753615 177.267216)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C95" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 71 "Net-(C94-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 72 "Net-(C95-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 82.842503 95.097776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C36" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 22 "Net-(C35-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 23 "Net-(C36-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.97 90.17)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper36" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(C39-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(C40-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.243615 78.663888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C28" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 16 "Net-(C27-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 17 "Net-(C28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.971115 177.267216)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C96" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 72 "Net-(C95-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 73 "Net-(C96-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.49 68.656112 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D3" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.742223 155.905552)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper75" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 61 "Net-(C82-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(C83-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.79 123.037776)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R6" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 76.058892 155.905552)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper72" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(C79-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 59 "Net-(C80-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.512216 41.248888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper9" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 92 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 93 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.286669 123.037776)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper53" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(C58-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(C59-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.33 62.23)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C12" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.580279 193.701104)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C104" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 78 "Net-(C103-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 79 "Net-(C104-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 245.11 187.351104 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J10" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.197777 106.603888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper47" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(C51-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(C52-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.742223 139.471664)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper65" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 52 "Net-(C71-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 53 "Net-(C72-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.286669 90.17)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper33" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(C36-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(C37-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.831115 188.773328)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper91" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 76 "Net-(C101-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.653331 139.471664)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper69" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(C75-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(C76-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.881115 106.603888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper50" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(C54-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.991115 78.663888)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C32" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 20 "Net-(C31-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 21 "Net-(C32-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.79 139.471664)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R7" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.33 95.097776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C34" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.83 46.176664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 90 "Net-(C7-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 91 "Net-(C8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.514446 139.471664)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper64" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "Net-(C70-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 52 "Net-(C71-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.481115 127.965552)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C64" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 46 "Net-(C63-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 47 "Net-(C64-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.742223 57.302224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper15" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(C16-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(C17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.753615 193.701104)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C106" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 80 "Net-(C105-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 81 "Net-(C106-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.286669 57.302224)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper13" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(C14-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.881115 139.471664)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper70" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(C76-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.211391 144.39944)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C70" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 50 "Net-(C69-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 51 "Net-(C70-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.145554 41.248888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper3" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 86 "Net-(C3-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 87 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.243615 193.701104)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C105" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 79 "Net-(C104-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 80 "Net-(C105-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.286669 73.736112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper23" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(C25-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(C26-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.742223 90.17)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper35" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(C38-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(C39-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.243615 95.097776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C39" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 25 "Net-(C38-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 26 "Net-(C39-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.473615 95.097776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C35" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 22 "Net-(C35-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.481115 95.097776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C42" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 28 "Net-(C41-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 29 "Net-(C42-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 180.481115 144.39944)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C75" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 55 "Net-(C74-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 56 "Net-(C75-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-logo:wham-logo-kicad" (layer "F.Cu")
    (at 33.02 180.34 90)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0 90) (layer "F.SilkS") hide)
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 66.3325 46.176664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "V_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 85 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 76.058892 188.773328)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper92" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 76 "Net-(C101-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 77 "Net-(C102-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.208615 193.701104)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C110" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 84 "Net-(C109-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.881115 188.773328)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper100" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 84 "Net-(C109-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.971115 111.531664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C52" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 36 "Net-(C51-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 37 "Net-(C52-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.671115 93.371112)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H8" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.753615 111.531664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C51" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 35 "Net-(C50-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 36 "Net-(C51-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 205.881115 73.736112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper30" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(C32-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.49 85.09 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D4" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.208615 62.23)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C22" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 12 "Net-(C21-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.97 123.037776)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper56" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "Net-(C61-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(C62-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.971115 62.23)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C19" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 9 "Net-(C18-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 10 "Net-(C19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.79 172.33944)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R9" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.211391 160.833328)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C81" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 59 "Net-(C80-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 60 "Net-(C81-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 140.97 155.905552)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper76" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(C83-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 63 "Net-(C84-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 99.070276 46.176664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 86 "Net-(C3-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 87 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.79 106.603888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 108.514446 172.33944)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper84" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 69 "Net-(C92-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 70 "Net-(C93-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.742223 172.33944)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper85" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 70 "Net-(C93-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 71 "Net-(C94-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 163.971115 160.833328)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C85" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 63 "Net-(C84-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 64 "Net-(C85-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 227.33 160.833328)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C78" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "150 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3975 -8.56) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 245.11 121.615552 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J6" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.753615 95.097776)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C40" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 26 "Net-(C39-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 27 "Net-(C40-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 59.831115 123.037776)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper51" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(C57-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm_Pad_Via" (layer "F.Cu")
    (at 254 198.205 180)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (property "Sheetfile" "Bias Voltage Divider.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.625 0 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 -1.856155 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 1.856155 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -2.625 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0 180) (size 7 7) (drill 3.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 2.625 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 -1.856155 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 1.856155 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.625 0 180) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.79 188.773328)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R10" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm_Pad_Via" (layer "F.Cu")
    (at 30.395 199.39)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (property "Sheetfile" "Bias Voltage Divider.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.625 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -2.625) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 2.625) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.625 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 235.49 117.957776 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "400W bidirectional Transient Voltage Suppressor, 10.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "bidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D6" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ10CA" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "V_out") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 189.653331 90.17)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider3")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper39" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(C42-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(C43-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 131.243615 127.965552)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C61" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 43 "Net-(C60-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 44 "Net-(C61-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 173.425554 172.33944)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider6")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper88" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 73 "Net-(C96-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 74 "Net-(C97-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 76.058892 73.736112)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper22" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(C24-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(C25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.197777 188.773328)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider9")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper97" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 81 "Net-(C106-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 82 "Net-(C107-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 92.286669 139.471664)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper63" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 50 "Net-(C69-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "Net-(C70-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 224.79 155.905552)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R8" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "2.7 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 213.208615 127.965552)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C66" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 48 "Net-(C65-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "V_out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 124.742223 106.603888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper45" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(C49-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(C50-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.056662 41.248888)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper7" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 90 "Net-(C7-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "Net-(C8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.991115 144.39944)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider8")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C76" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 56 "Net-(C75-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 57 "Net-(C76-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.197777 155.905552)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider5")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R_upper77" (at 6.35 -2.72) (layer "F.SilkS"))
    (fp_text value "27 kOhm" (at 6.35 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 63 "Net-(C84-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 64 "Net-(C85-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 115.580279 62.23)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C16" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 6 "Net-(C15-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 7 "Net-(C16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 196.991115 111.531664)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider4")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C54" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "100 pF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 38 "Net-(C53-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 39 "Net-(C54-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 244.968885 39.826664 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J1" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "V_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:My_Mount_Pad" (layer "F.Cu")
    (at 49.671115 126.238888)
    (property "Sheetfile" "/Users/tqian/Documents/Fusion/WHAM/Wham-Experiment/Wham-Bias/Bias Voltage Divider/Bias-VD-v2/Bias-VD-v2.kicad_sch")
    (property "Sheetname" "single_divider7")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H10" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.8 7.8) (drill 5.4) (layers "*.Cu" "*.Mask")
      (net 3 "V_in") (pinfunction "1") (pintype "input"))
  )
  (gr_line (start 41.083891 183.693336) (end 138.873891 183.693336)
    (layer "Edge.Cuts"))
  (gr_line (start 261.62 204.47) (end 261.62 24.13)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 167.64) (end 43.18 167.64)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 151.13) (end 43.18 148.59)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 85.09) (end 43.18 85.09)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 53.34) (end 43.18 53.34)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 115.57) (end 139.7 118.11)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 50.8) (end 139.7 50.8)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 101.6) (end 43.18 99.06)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 181.61) (end 139.7 184.15)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 165.1) (end 139.7 167.64)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 50.8) (end 139.7 53.34)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 118.11) (end 43.18 118.11)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 99.06) (end 139.7 99.06)
    (layer "Edge.Cuts"))
  (gr_line (start 261.62 24.13) (end 24.573891 23.673336)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 68.58) (end 43.18 66.04)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 134.62) (end 43.18 132.08)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 82.55) (end 139.7 85.09)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 151.13) (end 43.18 151.13)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 82.55) (end 139.7 82.55)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 85.09) (end 43.18 82.55)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 184.15) (end 43.18 181.61)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 148.59) (end 139.7 148.59)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 132.08) (end 139.7 132.08)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 148.59) (end 139.7 151.13)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 118.11) (end 43.18 115.57)
    (layer "Edge.Cuts"))
  (gr_line (start 24.573891 204.47) (end 261.62 204.47)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 66.04) (end 139.7 66.04)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 167.64) (end 43.18 165.1)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 115.57) (end 139.7 115.57)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 181.61) (end 139.7 181.61)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 68.58) (end 43.18 68.58)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 101.6) (end 43.18 101.6)
    (layer "Edge.Cuts"))
  (gr_line (start 24.573891 23.673336) (end 24.573891 204.47)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 165.1) (end 139.7 165.1)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 66.04) (end 139.7 68.58)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 132.08) (end 139.7 134.62)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 134.62) (end 43.18 134.62)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 99.06) (end 139.7 101.6)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 184.15) (end 43.18 184.15)
    (layer "Edge.Cuts"))
  (gr_line (start 43.18 53.34) (end 43.18 50.8)
    (layer "Edge.Cuts"))
  (gr_text "V Out\n\nGnd" (at 251.46 191.77) (layer "F.SilkS"))
  (gr_text "Bias Ring Voltage Divider\nT. Qian 5 Dec 2023" (at 36.915 165.868845 90) (layer "F.SilkS"))
  (gr_text "V Out\n\nGnd" (at 251.46 93.98) (layer "F.SilkS"))
  (gr_text "V Out\n\nGnd" (at 251.46 62.23) (layer "F.SilkS"))
  (gr_text "V Out\n\nGnd" (at 251.46 143.51) (layer "F.SilkS"))
  (gr_text "V Out\n\nGnd" (at 251.46 110.49) (layer "F.SilkS"))
  (gr_text "V Out\n\nGnd" (at 251.46 46.99) (layer "F.SilkS"))
  (gr_text "V Out\n\nGnd" (at 251.46 175.26) (layer "F.SilkS"))
  (gr_text "V Out\n\nGnd" (at 251.46 78.74) (layer "F.SilkS"))
  (gr_text "V Out\n\nGnd" (at 251.46 128.27) (layer "F.SilkS"))
  (gr_text "V Out\n\nGnd" (at 251.46 160.02) (layer "F.SilkS"))
)
