(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 120)
    (no_connects 0)
    (area 76.124999 69.774999 190.575001 101.675001)
    (thickness 1.6)
    (drawings 13)
    (tracks 399)
    (zones 0)
    (modules 67)
    (nets 49)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 76.2635 101.5365)
    (grid_origin 76.2635 101.5365)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 inputoffset)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C4-Pad2)")
  (net 6 bela_ain0)
  (net 7 "Net-(C5-Pad2)")
  (net 8 bela_ain1)
  (net 9 "Net-(C6-Pad2)")
  (net 10 bela_ain2)
  (net 11 "Net-(C7-Pad2)")
  (net 12 bela_ain3)
  (net 13 "Net-(C8-Pad2)")
  (net 14 VCC)
  (net 15 GND)
  (net 16 VSS)
  (net 17 "Net-(Cci1-Pad1)")
  (net 18 modular_ain0)
  (net 19 "Net-(Cci2-Pad1)")
  (net 20 modular_ain1)
  (net 21 "Net-(Cci3-Pad1)")
  (net 22 modular_ain2)
  (net 23 "Net-(Cci4-Pad1)")
  (net 24 modular_ain3)
  (net 25 "Net-(P1-Pad1)")
  (net 26 "Net-(P1-Pad4)")
  (net 27 "Net-(R1-Pad1)")
  (net 28 "Net-(R2-Pad1)")
  (net 29 "Net-(R3-Pad1)")
  (net 30 "Net-(R4-Pad1)")
  (net 31 "Net-(R5-Pad1)")
  (net 32 "Net-(R10-Pad1)")
  (net 33 "Net-(R11-Pad1)")
  (net 34 "Net-(R12-Pad1)")
  (net 35 "Net-(R13-Pad2)")
  (net 36 "Net-(R10-Pad2)")
  (net 37 "Net-(R11-Pad2)")
  (net 38 "Net-(R12-Pad2)")
  (net 39 "Net-(R13-Pad1)")
  (net 40 "Net-(R14-Pad1)")
  (net 41 "Net-(R15-Pad1)")
  (net 42 "Net-(R16-Pad1)")
  (net 43 "Net-(R25-Pad2)")
  (net 44 "Net-(R26-Pad2)")
  (net 45 "Net-(R27-Pad2)")
  (net 46 "Net-(R28-Pad2)")
  (net 47 "Net-(R33-Pad1)")
  (net 48 "Net-(RinF1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(Cci1-Pad1)")
    (add_net "Net-(Cci2-Pad1)")
    (add_net "Net-(Cci3-Pad1)")
    (add_net "Net-(Cci4-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R28-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R33-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(RinF1-Pad1)")
    (add_net VCC)
    (add_net VSS)
    (add_net bela_ain0)
    (add_net bela_ain1)
    (add_net bela_ain2)
    (add_net bela_ain3)
    (add_net inputoffset)
    (add_net modular_ain0)
    (add_net modular_ain1)
    (add_net modular_ain2)
    (add_net modular_ain3)
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA6F9)
    (at 102.489 74.8665)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at -1.7145 0.635 90) (layer F.SilkS))
    (fp_text value 330p (at 2.286 -3.429 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 inputoffset))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA6E9)
    (at 107.506 68.6435)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at -1.7145 -1.143 90) (layer F.SilkS))
    (fp_text value 330p (at 4.2545 -0.1905 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 inputoffset))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA4A4)
    (at 143.891 69.4055 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 4.191 0.0635 270) (layer F.SilkS))
    (fp_text value 330pF (at 1.27 2.0955 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 inputoffset))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA622)
    (at 186.563 75.819 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C4 (at 2.667 2.159 360) (layer F.SilkS))
    (fp_text value 330pF (at -1.9685 0.5715 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 inputoffset))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA5F3)
    (at 87.122 75.692)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C5 (at 4.5085 -1.397 180) (layer F.SilkS))
    (fp_text value 330pF (at -1.905 -0.1905 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 bela_ain0))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA47E)
    (at 114.046 74.803)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C6 (at 4.5085 -1.143 180) (layer F.SilkS))
    (fp_text value 330p (at -1.8415 -0.254 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 bela_ain1))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(C6-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA641)
    (at 141.986 72.644 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 4.1275 0.0635 360) (layer F.SilkS))
    (fp_text value 330pF (at 1.3335 2.3495 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 bela_ain2))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(C7-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA3AD)
    (at 171.831 74.9935)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at -1.7145 0 90) (layer F.SilkS))
    (fp_text value 330pF (at 1.397 -2.4765) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 bela_ain3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(C8-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 584DA433)
    (at 88.9635 71.0565 180)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C9 (at 3.937 2.2225 270) (layer F.SilkS))
    (fp_text value 10uF (at 1.143 3.4925 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 584DA43B)
    (at 88.646 98.298 180)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C10 (at 4.3815 -2.4765 360) (layer F.SilkS))
    (fp_text value 10uF (at 4.445 1.3335 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 VSS))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA413)
    (at 107.506 88.646)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C11 (at 1.27 -0.0635 90) (layer F.SilkS))
    (fp_text value 10n (at -1.778 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA465)
    (at 110.046 74.9935 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C12 (at -0.0635 3.048 270) (layer F.SilkS))
    (fp_text value 10n (at 2.0955 2.2225 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 VSS))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA400)
    (at 165.227 88.646)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C13 (at 1.2065 -0.127 90) (layer F.SilkS))
    (fp_text value 10n (at -1.778 -0.0635 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA3B2)
    (at 167.64 75.057 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C14 (at 4.318 0.0635 270) (layer F.SilkS))
    (fp_text value 10n (at 1.25 2.5 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 VSS))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA492)
    (at 132.778 74.93)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C15 (at 4.191 0 90) (layer F.SilkS))
    (fp_text value 10n (at -1.9055 -0.1905 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA4C1)
    (at 141.986 83.1215 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C16 (at 4.191 0 360) (layer F.SilkS))
    (fp_text value 10n (at -1.7145 0.127 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 VSS))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA421)
    (at 107.506 91.821)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference Cci1 (at 1.2065 0.0635 90) (layer F.SilkS))
    (fp_text value 1uF (at -1.651 3.3655 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "Net-(Cci1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 modular_ain0))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA41A)
    (at 110.046 95.123 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference Cci2 (at 1.27 0 270) (layer F.SilkS))
    (fp_text value 1uF (at 4.2545 3.302 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 "Net-(Cci2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 modular_ain1))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA3EC)
    (at 165.227 91.821)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference Cci3 (at 1.3335 0.0635 90) (layer F.SilkS))
    (fp_text value 1uF (at -1.778 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Net-(Cci3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 22 modular_ain2))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 584DA3F4)
    (at 167.704 95.0595 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference Cci4 (at 1.2705 -0.1905 270) (layer F.SilkS))
    (fp_text value 1uF (at 4.2545 0.254 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 23 "Net-(Cci4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 24 modular_ain3))
  )
  (module mta-156:MTA-156-4 (layer F.Cu) (tedit 5846D0B3)
    (at 81.153 77.5335)
    (descr MTA-156-4)
    (tags MTA-156-4)
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value MTA-156-4 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 5 2.5) (drill 1.68) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 3.96) (size 5 2.5) (drill 1.68) (layers *.Cu *.Mask F.SilkS)
      (net 15 GND))
    (pad 3 thru_hole oval (at 0 7.92) (size 5 2.5) (drill 1.68) (layers *.Cu *.Mask F.SilkS)
      (net 15 GND))
    (pad 4 thru_hole oval (at 0 11.88) (size 5 2.5) (drill 1.68) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P1-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm_LongPads (layer F.Cu) (tedit 58463B9D)
    (at 99.8855 85.598 90)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 4.826 -1.4605 90) (layer F.SilkS))
    (fp_text value TL074 (at 3.8735 7.874 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(R13-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R13-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R2-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R10-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(R14-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 bela_ain1))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(R26-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 VSS))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(R25-Pad2)"))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 bela_ain0))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm_LongPads (layer F.Cu) (tedit 58463DC7)
    (at 157.607 85.6615 90)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 3.4925 -1.4605 90) (layer F.SilkS))
    (fp_text value TL074 (at 3.8735 7.874 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(R15-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R11-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R3-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R4-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R12-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(R16-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 bela_ain3))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(R28-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 VSS))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(R27-Pad2)"))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 bela_ain2))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 584DA49B)
    (at 130.175 85.6615 90)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U3 (at 6.1595 9.271 90) (layer F.SilkS))
    (fp_text value TL071 (at 4.064 3.9375 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 inputoffset))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(R33-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 VSS))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 inputoffset))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 584DA116)
    (at 131.572 99.1235 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -1.2065 10.287 90) (layer F.SilkS) hide)
    (fp_text value in_modular (at 5.0165 2.286 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 modular_ain0))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 modular_ain1))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 modular_ain2))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 modular_ain3))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 584DA64A)
    (at 127.826 71.1835 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 2.7305 -2.413 90) (layer F.SilkS) hide)
    (fp_text value out_bela (at 1.651 9.9695 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 bela_ain0))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 bela_ain1))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 bela_ain2))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 bela_ain3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5844C766)
    (at 186.69 69.85)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF4 (at 0 -4.2) (layer F.Fab) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5844C75E)
    (at 186.69 97.79)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF3 (at 0 -4.2) (layer F.Fab) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5844C755)
    (at 80.01 69.85)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF2 (at 0 -4.2) (layer F.Fab) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5844C748)
    (at 80.01 97.79)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF1 (at 0 -4.2) (layer F.Fab) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module trim:trimmer (layer F.Cu) (tedit 584DA813)
    (at 134.226 93.1037)
    (fp_text reference TR1 (at -3.493 -4.318) (layer F.SilkS))
    (fp_text value 10k (at 0.2 -4.1) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 VSS))
    (pad 2 thru_hole circle (at 0 -2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 48 "Net-(RinF1-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 -2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 48 "Net-(RinF1-Pad1)"))
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 101.79 99.314 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 6.8 0 180) (layer F.SilkS))
    (fp_text value 100k (at 4.2 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 27 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 17 "Net-(Cci1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 114.173 89.0905 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 100k (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 28 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 19 "Net-(Cci2-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 160.655 99.314 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 6.8 0 180) (layer F.SilkS))
    (fp_text value 100k (at 4.2 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 29 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 21 "Net-(Cci3-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 172.022 89.154 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R4 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 100k (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 30 "Net-(R4-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 23 "Net-(Cci4-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 98.6155 89.154 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R5 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 20k (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 31 "Net-(R5-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 27 "Net-(R1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 117.348 99.314 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R6 (at 6.8 0 180) (layer F.SilkS))
    (fp_text value 20k (at 4.2 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 36 "Net-(R10-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 28 "Net-(R2-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 153.924 89.0905 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R7 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 20k (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 37 "Net-(R11-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 29 "Net-(R3-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 175.196 99.2505 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R8 (at 6.8 0 180) (layer F.SilkS))
    (fp_text value 20k (at 4.2 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 38 "Net-(R12-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 30 "Net-(R4-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 95.504 99.2505 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R9 (at 6.8 0 180) (layer F.SilkS))
    (fp_text value 20k (at 4.2 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 35 "Net-(R13-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 31 "Net-(R5-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 120.65 89.154 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R10 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 20k (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 32 "Net-(R10-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 36 "Net-(R10-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 153.098 75.5015 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R11 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 20k (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 33 "Net-(R11-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 37 "Net-(R11-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 178.372 89.0905 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R12 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 20k (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 34 "Net-(R12-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 38 "Net-(R12-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 92.329 89.0905 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R13 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 10k (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 39 "Net-(R13-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 35 "Net-(R13-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 123.762 99.314 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R14 (at 6.8 0 180) (layer F.SilkS))
    (fp_text value 10k (at 4.2 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 40 "Net-(R14-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 32 "Net-(R10-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 157.353 89.0905 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R15 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 10k (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 41 "Net-(R15-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 33 "Net-(R11-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 181.483 89.027 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R16 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 10k (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 42 "Net-(R16-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 34 "Net-(R12-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 92.329 76.327 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R17 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 27k4 (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 39 "Net-(R13-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 122.618 75.5015 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R18 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 27k4 (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(C6-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 40 "Net-(R14-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 146.685 85.6615 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R19 (at 6.8 0 180) (layer F.SilkS))
    (fp_text value 27k4 (at 4.2 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 41 "Net-(R15-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 181.038 75.565 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R20 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 27k4 (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(C8-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 42 "Net-(R16-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 95.4405 86.487 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R21 (at 6.8 0 180) (layer F.SilkS))
    (fp_text value 27k4 (at 4.2 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 119.316 85.6615 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R22 (at 6.8 0 180) (layer F.SilkS))
    (fp_text value 27k4 (at 4.2 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(C6-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 149.924 75.565 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R23 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 27k4 (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(C7-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 177.864 85.725 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R24 (at 6.8 0 180) (layer F.SilkS))
    (fp_text value 27k4 (at 4.2 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(C8-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 102.298 68.707 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R25 (at 6.8 0 270) (layer F.SilkS))
    (fp_text value 27k4 (at 4.2 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 inputoffset))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 43 "Net-(R25-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 125.794 85.6615 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R26 (at 6.8 0 180) (layer F.SilkS))
    (fp_text value 27k4 (at 4.2 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 inputoffset))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 44 "Net-(R26-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 146.558 69.342)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R27 (at 6.8 0 90) (layer F.SilkS))
    (fp_text value 27k4 (at 4.2 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 inputoffset))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 45 "Net-(R27-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 187.706 78.9305 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R28 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 27k4 (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 inputoffset))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 46 "Net-(R28-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 102.298 71.8185 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R29 (at 6.8 0 270) (layer F.SilkS))
    (fp_text value 16k2 (at 4.2 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 43 "Net-(R25-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 bela_ain0))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 124.333 71.374 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R30 (at 6.8 0 270) (layer F.SilkS))
    (fp_text value 16k2 (at 4.2 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 44 "Net-(R26-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 bela_ain1))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 156.654 72.517 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R31 (at 6.8 0 270) (layer F.SilkS))
    (fp_text value 16k2 (at 4.2 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 45 "Net-(R27-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 bela_ain2))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 184.658 89.154 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R32 (at 6.8 0 180) (layer F.SilkS))
    (fp_text value 16k2 (at 4.2 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 46 "Net-(R28-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 bela_ain3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 147.32 89.154 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R33 (at 6.8 0 360) (layer F.SilkS))
    (fp_text value 10k (at 4.2 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 47 "Net-(R33-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module xnorman:Resistor_Vertical_RM5mm-xnor (layer F.Cu) (tedit 584D982A)
    (at 87.376 82.423 270)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R34 (at -2.2 1.6 270) (layer F.SilkS))
    (fp_text value bead (at 1.4 -1.8 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.49936 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5019 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 25 "Net-(P1-Pad1)"))
  )
  (module xnorman:Resistor_Vertical_RM5mm-xnor (layer F.Cu) (tedit 584D982A)
    (at 87.3125 91.5035 270)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R35 (at -2.2 1.6 270) (layer F.SilkS))
    (fp_text value bead (at 1.4 -1.8 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.49936 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 26 "Net-(P1-Pad4)"))
    (pad 2 thru_hole circle (at 2.5019 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 16 VSS))
  )
  (module xnorman:Resistor_Horizontal_RM10mm-xnorman (layer F.Cu) (tedit 584D9799)
    (at 144.208 99.314 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference RinF1 (at 6.8 0 180) (layer F.SilkS))
    (fp_text value 30k1 (at 4.2 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 48 "Net-(RinF1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 47 "Net-(R33-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 0 (at 129.2225 100.584) (layer F.SilkS))
  (gr_text gnd (at 141.5415 96.139 90) (layer F.SilkS))
  (gr_text 0 (at 125.476 67.691) (layer F.SilkS))
  (gr_text gnd (at 128.524 73.533) (layer F.SilkS))
  (gr_text - (at 83.5025 91.8845) (layer F.SilkS))
  (gr_text + (at 83.2485 74.676) (layer F.SilkS))
  (gr_text http://x37v.info (at 164.9095 72.4535 180) (layer B.SilkS))
  (gr_text "xnor 12/2016" (at 164.2999 70.4469 180) (layer B.SilkS))
  (gr_text "modular to bela\nanalog" (at 182.4355 69.3293) (layer B.SilkS))
  (gr_line (start 76.2 66.04) (end 190.5 66.04) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190.5 66.04) (end 190.5 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190.5 101.6) (end 76.2 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.2 66.04) (end 76.2 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 15) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 190.3603 66.1797) (xy 76.3143 66.1797) (xy 76.3143 101.3333) (xy 190.1063 101.3333) (xy 190.3603 66.2813)
      )
    )
  )
  (zone (net 15) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 190.2587 66.2813) (xy 76.5683 66.4337) (xy 76.4667 101.3333) (xy 190.1063 101.2317) (xy 190.1063 66.4337)
      )
    )
  )
)
