(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 61)
    (tracks 170)
    (zones 0)
    (modules 4)
    (nets 22)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.635 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.3 1.35)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad20)")
  (net 3 "Net-(J1-Pad16)")
  (net 4 "Net-(J1-Pad12)")
  (net 5 "Net-(J1-Pad8)")
  (net 6 "Net-(J1-Pad4)")
  (net 7 "Net-(J1-Pad28)")
  (net 8 "Net-(J1-Pad32)")
  (net 9 "Net-(J1-Pad40)")
  (net 10 "Net-(J1-Pad24)")
  (net 11 "Net-(J1-Pad36)")
  (net 12 "Net-(J2-Pad20)")
  (net 13 "Net-(J2-Pad16)")
  (net 14 "Net-(J2-Pad12)")
  (net 15 "Net-(J2-Pad8)")
  (net 16 "Net-(J2-Pad4)")
  (net 17 "Net-(J2-Pad28)")
  (net 18 "Net-(J2-Pad32)")
  (net 19 "Net-(J2-Pad40)")
  (net 20 "Net-(J2-Pad24)")
  (net 21 "Net-(J2-Pad36)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad28)")
    (add_net "Net-(J1-Pad32)")
    (add_net "Net-(J1-Pad36)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad40)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad36)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad40)")
    (add_net "Net-(J2-Pad8)")
  )
  (module Igloo12:TEST_PAD (layer F.Cu) (tedit 5CC8D95F)
    (at 115.87 57.855 180)
    (fp_text reference U1 (at 0 -3.429) (layer F.Fab) hide)
    (fp_text value TEST_PAD (at 0 -1.7145) (layer F.Fab) hide)
    (pad 1 smd rect (at -5.1435 0 180) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad40)"))
    (pad 2 smd rect (at -4.0005 0 180) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad36)"))
    (pad 3 smd rect (at -2.8575 0 180) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad32)"))
    (pad 4 smd rect (at -1.7145 0 180) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad28)"))
    (pad 5 smd rect (at -0.5715 0 180) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad24)"))
    (pad 6 smd rect (at 0.5715 0 180) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad20)"))
    (pad 7 smd rect (at 1.7145 0 180) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad16)"))
    (pad 8 smd rect (at 2.8575 0 180) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad12)"))
    (pad 9 smd rect (at 4.0005 0 180) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 10 smd rect (at 5.1435 0 180) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad4)"))
  )
  (module Igloo12:TEST_PAD (layer F.Cu) (tedit 5CC8D95F)
    (at 115.87 73.085)
    (fp_text reference U2 (at 0 -3.429) (layer F.Fab) hide)
    (fp_text value TEST_PAD (at 0 -1.7145) (layer F.Fab) hide)
    (pad 1 smd rect (at -5.1435 0) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-Pad40)"))
    (pad 2 smd rect (at -4.0005 0) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J2-Pad36)"))
    (pad 3 smd rect (at -2.8575 0) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J2-Pad32)"))
    (pad 4 smd rect (at -1.7145 0) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad28)"))
    (pad 5 smd rect (at -0.5715 0) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J2-Pad24)"))
    (pad 6 smd rect (at 0.5715 0) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad20)"))
    (pad 7 smd rect (at 1.7145 0) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad16)"))
    (pad 8 smd rect (at 2.8575 0) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad12)"))
    (pad 9 smd rect (at 4.0005 0) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad8)"))
    (pad 10 smd rect (at 5.1435 0) (size 0.381 1.27) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad4)"))
  )
  (module Igloo12:LSHM-120-01-L-RH-A-S-TR (layer B.Cu) (tedit 5E6035CD)
    (at 115.87 42.5)
    (fp_text reference J1 (at -0.2105 10.413) (layer B.Fab) hide)
    (fp_text value LSHM-120-01-L-RH-A-S-TR (at -0.2105 11.413) (layer B.Fab) hide)
    (pad 39 smd rect (at 4.75 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 37 smd rect (at 4.25 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 26 smd rect (at 1.25 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 25 smd rect (at 1.25 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 31 smd rect (at 2.75 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 0.25 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 21 smd rect (at 0.25 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 3.75 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J1-Pad36)"))
    (pad 24 smd rect (at 0.75 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J1-Pad24)"))
    (pad 34 smd rect (at 3.25 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 33 smd rect (at 3.25 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 40 smd rect (at 4.75 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad40)"))
    (pad 35 smd rect (at 3.75 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 38 smd rect (at 4.25 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 32 smd rect (at 2.75 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J1-Pad32)"))
    (pad 29 smd rect (at 2.25 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 28 smd rect (at 1.75 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad28)"))
    (pad 27 smd rect (at 1.75 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 23 smd rect (at 0.75 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 30 smd rect (at 2.25 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at 6.75 7.85) (size 1.9 1.9) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at -6.75 7.85) (size 1.9 1.9) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at 8.3 7.3) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at 8.3 5.05) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at -8.3 7.3) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole circle (at -8.3 5.05) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at 6.325 6.175) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at -6.325 6.175) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.75 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.75 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -4.25 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -4.25 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -3.75 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.75 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -3.25 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -3.25 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 9 smd rect (at -2.75 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -2.75 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -2.25 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -2.25 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad12)"))
    (pad 13 smd rect (at -1.75 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -1.75 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd rect (at -1.25 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -1.25 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad16)"))
    (pad 17 smd rect (at -0.75 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 18 smd rect (at -0.75 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 19 smd rect (at -0.25 5.6) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 20 smd rect (at -0.25 8.675) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad20)"))
    (model ${KIPRJMOD}/Igloo12.3dshapes/LSHM-120-01-L-RH-A-S-TR.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Igloo12:LSHM-120-01-L-RH-A-S-TR (layer B.Cu) (tedit 5E6035CD)
    (at 115.87 88.47 180)
    (fp_text reference J2 (at -0.2105 10.413) (layer B.Fab) hide)
    (fp_text value LSHM-120-01-L-RH-A-S-TR (at -0.2105 11.413) (layer B.Fab) hide)
    (pad 39 smd rect (at 4.75 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 37 smd rect (at 4.25 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 26 smd rect (at 1.25 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 25 smd rect (at 1.25 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 31 smd rect (at 2.75 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 0.25 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 21 smd rect (at 0.25 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 3.75 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J2-Pad36)"))
    (pad 24 smd rect (at 0.75 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J2-Pad24)"))
    (pad 34 smd rect (at 3.25 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 33 smd rect (at 3.25 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 40 smd rect (at 4.75 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J2-Pad40)"))
    (pad 35 smd rect (at 3.75 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 38 smd rect (at 4.25 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 32 smd rect (at 2.75 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J2-Pad32)"))
    (pad 29 smd rect (at 2.25 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 28 smd rect (at 1.75 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J2-Pad28)"))
    (pad 27 smd rect (at 1.75 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 23 smd rect (at 0.75 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 30 smd rect (at 2.25 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at 6.75 7.85 180) (size 1.9 1.9) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at -6.75 7.85 180) (size 1.9 1.9) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at 8.3 7.3 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at 8.3 5.05 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at -8.3 7.3 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole circle (at -8.3 5.05 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at 6.325 6.175 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 41 thru_hole circle (at -6.325 6.175 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.75 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.75 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -4.25 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -4.25 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(J2-Pad4)"))
    (pad 5 smd rect (at -3.75 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.75 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -3.25 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -3.25 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J2-Pad8)"))
    (pad 9 smd rect (at -2.75 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -2.75 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -2.25 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -2.25 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J2-Pad12)"))
    (pad 13 smd rect (at -1.75 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -1.75 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd rect (at -1.25 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -1.25 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J2-Pad16)"))
    (pad 17 smd rect (at -0.75 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 18 smd rect (at -0.75 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 19 smd rect (at -0.25 5.6 180) (size 0.3 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 20 smd rect (at -0.25 8.675 180) (size 0.3 1.35) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J2-Pad20)"))
    (model ${KIPRJMOD}/Igloo12.3dshapes/LSHM-120-01-L-RH-A-S-TR.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 5 (at 115.12 79.57 180) (layer F.SilkS))
  (gr_text 3 (at 113.12 79.57 180) (layer F.SilkS))
  (gr_text 9 (at 119.12 79.57 180) (layer F.SilkS))
  (gr_text 7 (at 117.12 79.57 180) (layer F.SilkS))
  (gr_text 1 (at 111.12 79.57 180) (layer F.SilkS))
  (gr_text 9 (at 112.62 51.4) (layer F.SilkS))
  (gr_text 7 (at 114.62 51.4) (layer F.SilkS))
  (gr_text 5 (at 116.62 51.4) (layer F.SilkS))
  (gr_text 3 (at 118.62 51.4) (layer F.SilkS))
  (gr_text 1 (at 120.62 51.4) (layer F.SilkS))
  (gr_text 7 (at 114.1555 56.064) (layer F.SilkS))
  (gr_text 3 (at 118.7275 56.064) (layer F.SilkS))
  (gr_text 5 (at 116.4415 56.064) (layer F.SilkS))
  (gr_text "Dylan Oh\nMar 2020" (at 101.162 84.973 90) (layer F.Mask))
  (gr_text 9 (at 119.8705 74.86 180) (layer F.SilkS))
  (gr_text 3 (at 113.0125 74.86 180) (layer F.SilkS))
  (gr_text 7 (at 117.5845 74.86 180) (layer F.SilkS))
  (gr_text NORTH (at 115.87 49.46) (layer F.Mask))
  (gr_text N (at 105.87 55.47) (layer F.Mask))
  (gr_text SOUTH (at 115.87 81.6 180) (layer F.Mask))
  (gr_text 5 (at 115.2985 74.86 180) (layer F.SilkS))
  (gr_text N (at 125.87 55.47) (layer F.Mask))
  (gr_text 1 (at 121.0135 56.064) (layer F.SilkS))
  (gr_text S (at 125.87 75.47 180) (layer F.Mask))
  (gr_text 9 (at 111.8695 56.064) (layer F.SilkS))
  (gr_text S (at 105.87 75.47 180) (layer F.Mask))
  (gr_text 1 (at 110.7265 74.86 180) (layer F.SilkS))
  (gr_text Igloo12 (at 97.755 79.288 90) (layer F.Mask))
  (gr_line (start 121.585 59.755) (end 121.585 71.185) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.87 45.47) (end 135.87 85.47) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.155 59.755) (end 121.585 59.755) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.155 71.185) (end 110.155 59.755) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.87 85.47) (end 95.87 85.47) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 95.87 85.47) (end 95.87 45.47) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.585 71.185) (end 110.155 71.185) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 95.87 45.47) (end 135.87 45.47) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.87 45.47) (xy 135.87 45.47) (xy 135.87 85.47) (xy 95.87 85.47)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.87 45.47) (xy 135.87 45.47) (xy 135.87 85.47) (xy 95.87 85.47)
      )
    )
  )
)
