(kicad_pcb (version 4) (host pcbnew 4.0.3-rc1-stable)
  (general
    (links 144)
    (no_connects 0)
    (area 111.266999 69.774999 196.417001 119.925001)
    (thickness 1.6)
    (drawings 11)
    (tracks 1366)
    (zones 0)
    (modules 22)
    (nets 70)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 4)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 6)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 111.356 69.875)
    (grid_origin 111.356 69.875)
    (visible_elements FFFFE77F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber 2.1b/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 A11)
  (net 6 A9)
  (net 7 BUSACK)
  (net 8 ROMCS48K)
  (net 9 A4)
  (net 10 A5)
  (net 11 A6)
  (net 12 A7)
  (net 13 RESET)
  (net 14 BUSREQ)
  (net 15 TOP28)
  (net 16 A10)
  (net 17 A8)
  (net 18 RFSH)
  (net 19 M1)
  (net 20 -12V)
  (net 21 +12V)
  (net 22 WAIT)
  (net 23 -5V)
  (net 24 WR)
  (net 25 U)
  (net 26 V)
  (net 27 Y)
  (net 28 VIDEO/OE2_128K)
  (net 29 IOREQGE)
  (net 30 A3)
  (net 31 A2)
  (net 32 A1)
  (net 33 A0)
  (net 34 CLOCK)
  (net 35 +9V)
  (net 36 A12)
  (net 37 A14)
  (net 38 RD)
  (net 39 IOREQ)
  (net 40 MREQ)
  (net 41 HALT)
  (net 42 NMI)
  (net 43 INT)
  (net 44 D4)
  (net 45 D3)
  (net 46 D5)
  (net 47 D6)
  (net 48 D2)
  (net 49 D1)
  (net 50 D0)
  (net 51 OE1_128K)
  (net 52 D7)
  (net 53 A13)
  (net 54 A15)
  (net 55 EP_CE)
  (net 56 PA16)
  (net 57 PA17)
  (net 58 PA18)
  (net 59 PA14)
  (net 60 PA15)
  (net 61 PT_ROMCS)
  (net 62 J1-Up)
  (net 63 J2-Down)
  (net 64 J3-Left)
  (net 65 J4-Right)
  (net 66 J6-Fire)
  (net 67 Rom_WR)
  (net 68 Rom_RD)
  (net 69 "Net-(JP1-Pad2)")
  (net_class Default "Esta es la clase de red por defecto."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net +9V)
    (add_net -12V)
    (add_net -5V)
    (add_net A0)
    (add_net A1)
    (add_net A10)
    (add_net A11)
    (add_net A12)
    (add_net A13)
    (add_net A14)
    (add_net A15)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net A8)
    (add_net A9)
    (add_net BUSACK)
    (add_net BUSREQ)
    (add_net CLOCK)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net EP_CE)
    (add_net GND)
    (add_net HALT)
    (add_net INT)
    (add_net IOREQ)
    (add_net IOREQGE)
    (add_net J1-Up)
    (add_net J2-Down)
    (add_net J3-Left)
    (add_net J4-Right)
    (add_net J6-Fire)
    (add_net M1)
    (add_net MREQ)
    (add_net NMI)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(JP1-Pad2)")
    (add_net OE1_128K)
    (add_net PA14)
    (add_net PA15)
    (add_net PA16)
    (add_net PA17)
    (add_net PA18)
    (add_net PT_ROMCS)
    (add_net RD)
    (add_net RESET)
    (add_net RFSH)
    (add_net ROMCS48K)
    (add_net Rom_RD)
    (add_net Rom_WR)
    (add_net TOP28)
    (add_net U)
    (add_net V)
    (add_net VIDEO/OE2_128K)
    (add_net WAIT)
    (add_net WR)
    (add_net Y)
  )
  (module Housings_DIP:DIP-24_W7.62mm_LongPads (layer F.Cu) (tedit 58811003)
    (at 137.391 82.829)
    (descr "24-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 4 -3.5) (layer F.SilkS))
    (fp_text value GAL22V10 (at 4.014 13.949999 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(JP1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 A14))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 54 A15))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 MREQ))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 IOREQ))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 RD))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 WR))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 64 J3-Left))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 65 J4-Right))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 62 J1-Up))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 63 J2-Down))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 13 thru_hole oval (at 7.62 27.94) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 66 J6-Fire))
    (pad 14 thru_hole oval (at 7.62 25.4) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 68 Rom_RD))
    (pad 15 thru_hole oval (at 7.62 22.86) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 67 Rom_WR))
    (pad 16 thru_hole oval (at 7.62 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 52 D7))
    (pad 17 thru_hole oval (at 7.62 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 47 D6))
    (pad 18 thru_hole oval (at 7.62 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 D5))
    (pad 19 thru_hole oval (at 7.62 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 D4))
    (pad 20 thru_hole oval (at 7.62 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 D3))
    (pad 21 thru_hole oval (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 D2))
    (pad 22 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 D1))
    (pad 23 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 50 D0))
    (pad 24 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Housings_DIP.3dshapes/DIP-24_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module p_w_pth_plcc:plcc32_pth-skt (layer F.Cu) (tedit 585AA429)
    (at 159.356 98.375 180)
    (fp_text reference U3 (at 10.408 10.847 180) (layer F.SilkS))
    (fp_text value "SST 39SF040" (at -0.514 -11.632 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 1.27 7.62 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 56 PA16))
    (pad 1 thru_hole circle (at -1.27 5.08 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 58 PA18))
    (pad 3 thru_hole circle (at 1.27 5.08 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 60 PA15))
    (pad 4 thru_hole circle (at 3.81 7.62 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 36 A12))
    (pad 5 thru_hole circle (at 6.35 5.08 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 A7))
    (pad 6 thru_hole circle (at 3.81 5.08 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 A6))
    (pad 7 thru_hole circle (at 6.35 2.54 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 10 A5))
    (pad 8 thru_hole circle (at 3.81 2.54 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 9 A4))
    (pad 9 thru_hole circle (at 6.35 0 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 30 A3))
    (pad 10 thru_hole circle (at 3.81 0 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 31 A2))
    (pad 11 thru_hole circle (at 6.35 -2.54 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 32 A1))
    (pad 12 thru_hole circle (at 3.81 -2.54 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 33 A0))
    (pad 13 thru_hole circle (at 6.35 -5.08 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 50 D0))
    (pad 14 thru_hole circle (at 3.81 -7.62 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 49 D1))
    (pad 15 thru_hole circle (at 3.81 -5.08 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 48 D2))
    (pad 16 thru_hole circle (at 1.27 -7.62 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 17 thru_hole circle (at 1.27 -5.08 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 45 D3))
    (pad 18 thru_hole circle (at -1.27 -7.62 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 44 D4))
    (pad 19 thru_hole circle (at -1.27 -5.08 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 46 D5))
    (pad 20 thru_hole circle (at -3.81 -7.62 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 47 D6))
    (pad 21 thru_hole circle (at -6.35 -5.08 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 52 D7))
    (pad 22 thru_hole circle (at -3.81 -5.08 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 55 EP_CE))
    (pad 23 thru_hole circle (at -6.35 -2.54 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 16 A10))
    (pad 24 thru_hole circle (at -3.81 -2.54 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 68 Rom_RD))
    (pad 25 thru_hole circle (at -6.35 0 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 A11))
    (pad 26 thru_hole circle (at -3.81 0 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 A9))
    (pad 27 thru_hole circle (at -6.35 2.54 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 17 A8))
    (pad 32 thru_hole circle (at -1.27 7.62 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 28 thru_hole circle (at -3.81 2.54 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 53 A13))
    (pad 29 thru_hole circle (at -6.35 5.08 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 59 PA14))
    (pad 30 thru_hole circle (at -3.81 7.62 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 57 PA17))
    (pad 31 thru_hole circle (at -3.81 5.08 180) (size 1.69926 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 67 Rom_WR))
    (model "${KIPRJMOD}/pcb libs/packages3d/pth_plcc/plcc32_pth-skt.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ZX_Spectrum:ZX_BUS (layer F.Cu) (tedit 585AA440)
    (at 147.876 74.041)
    (descr "ZX Bus")
    (tags "CONN BUS  ZX")
    (fp_text reference J2 (at 46.157 -0.991) (layer F.SilkS))
    (fp_text value ZX_48K_EDGE (at 2.54 -6.35) (layer F.SilkS) hide)
    (pad A28 connect rect (at 43.18 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 5 A11))
    (pad A27 connect rect (at 40.64 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 6 A9))
    (pad A26 connect rect (at 38.1 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 7 BUSACK))
    (pad A25 connect rect (at 35.56 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 61 PT_ROMCS))
    (pad A24 connect rect (at 33.02 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 9 A4))
    (pad A23 connect rect (at 30.48 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 10 A5))
    (pad A22 connect rect (at 27.94 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 11 A6))
    (pad A21 connect rect (at 25.4 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 12 A7))
    (pad A20 connect rect (at 22.86 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 13 RESET))
    (pad A19 connect rect (at 20.32 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 14 BUSREQ))
    (pad B28 connect rect (at 43.18 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 15 TOP28))
    (pad B27 connect rect (at 40.64 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 16 A10))
    (pad B26 connect rect (at 38.1 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 17 A8))
    (pad B25 connect rect (at 35.56 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 18 RFSH))
    (pad B24 connect rect (at 33.02 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 19 M1))
    (pad B23 connect rect (at 30.48 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 20 -12V))
    (pad B22 connect rect (at 27.94 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 21 +12V))
    (pad B21 connect rect (at 25.4 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 22 WAIT))
    (pad B20 connect rect (at 22.86 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 23 -5V))
    (pad B19 connect rect (at 20.32 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 24 WR))
    (pad A18 connect rect (at 17.78 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 25 U))
    (pad A17 connect rect (at 15.24 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 26 V))
    (pad A16 connect rect (at 12.7 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 27 Y))
    (pad A15 connect rect (at 10.16 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 28 VIDEO/OE2_128K))
    (pad A14 connect rect (at 7.62 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad A13 connect rect (at 5.08 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 29 IOREQGE))
    (pad A12 connect rect (at 2.54 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 30 A3))
    (pad A11 connect rect (at 0 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 31 A2))
    (pad A10 connect rect (at -2.54 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 32 A1))
    (pad A9 connect rect (at -5.08 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 33 A0))
    (pad A8 connect rect (at -7.62 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 34 CLOCK))
    (pad A7 connect rect (at -10.16 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad A6 connect rect (at -12.7 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad A4 connect rect (at -17.78 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 35 +9V))
    (pad A3 connect rect (at -20.32 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad A2 connect rect (at -22.86 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 36 A12))
    (pad A1 connect rect (at -25.4 0) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 37 A14))
    (pad B18 connect rect (at 17.78 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 38 RD))
    (pad B17 connect rect (at 15.24 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 39 IOREQ))
    (pad B16 connect rect (at 12.7 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 40 MREQ))
    (pad B15 connect rect (at 10.16 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 41 HALT))
    (pad B14 connect rect (at 7.62 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 42 NMI))
    (pad B13 connect rect (at 5.08 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 43 INT))
    (pad B12 connect rect (at 2.54 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 44 D4))
    (pad B11 connect rect (at 0 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 45 D3))
    (pad B10 connect rect (at -2.54 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 46 D5))
    (pad B9 connect rect (at -5.08 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 47 D6))
    (pad B8 connect rect (at -7.62 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 48 D2))
    (pad B7 connect rect (at -10.16 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 49 D1))
    (pad B6 connect rect (at -12.7 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 50 D0))
    (pad B4 connect rect (at -17.78 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 51 OE1_128K))
    (pad B3 connect rect (at -20.32 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 52 D7))
    (pad B2 connect rect (at -22.86 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 53 A13))
    (pad B1 connect rect (at -25.4 0) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 54 A15))
  )
  (module Mounting_Holes:MountingHole_5mm (layer F.Cu) (tedit 57E2C539)
    (at 191.342 96.35)
    (descr "Mounting hole, Befestigungsbohrung, 5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 5mm, No Annular, Kein Restring,")
    (fp_text reference "PP6 Box Hole" (at 0 -5) (layer F.SilkS) hide)
    (fp_text value "5mm - 0.5mm allowance" (at 0 7.00024) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -0.65) (size 6 6) (drill 6) (layers *.Cu))
  )
  (module w_details:hole_2mm (layer F.Cu) (tedit 57E26DCB)
    (at 194.356 113.875)
    (descr "Hole 2mm")
    (fp_text reference "hole_2mm_(3)" (at 0 -2.794) (layer F.SilkS) hide)
    (fp_text value VAL** (at 4.826 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.99898) (layers *.Cu F.SilkS))
    (model walter/details/hole.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57E165B0)
    (at 176.356 109.375 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at -2 0 360) (layer F.SilkS))
    (fp_text value 100nf (at 1.5 -2 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57E26370)
    (at 130.025 90.957)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 5 0) (layer F.SilkS))
    (fp_text value 100nf (at 1.5 -5) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57E26D4D)
    (at 193.356 84.875 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C3 (at -2 -1 540) (layer F.SilkS))
    (fp_text value 100nf (at -1.905 0 360) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57E16CBC)
    (at 166.856 85.375 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C4 (at 1 2.5 360) (layer F.SilkS))
    (fp_text value 100nf (at 1 -2.5 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57E16BF4)
    (at 132.356 108.875 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C5 (at 4.5 0 360) (layer F.SilkS))
    (fp_text value 100nf (at -1.905 0 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-18_W7.62mm_LongPads (layer F.Cu) (tedit 57E16170)
    (at 173.856 84.375)
    (descr "18-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 4 -3.5) (layer F.SilkS))
    (fp_text value PIC16F1826 (at 3.81 9.779 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 56 PA16))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 57 PA17))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 58 PA18))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 TOP28))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 67 Rom_WR))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 ROMCS48K))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 OE1_128K))
    (pad 11 thru_hole oval (at 7.62 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 VIDEO/OE2_128K))
    (pad 12 thru_hole oval (at 7.62 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 RESET))
    (pad 13 thru_hole oval (at 7.62 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 NMI))
    (pad 14 thru_hole oval (at 7.62 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 61 PT_ROMCS))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 55 EP_CE))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 59 PA14))
    (pad 18 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 60 PA15))
    (model Housings_DIP.3dshapes/DIP-18_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_details:hole_2mm (layer F.Cu) (tedit 575A8F71)
    (at 116.356 116.875)
    (descr "Hole 2mm")
    (fp_text reference hole_2mm (at 0 -2.794) (layer F.SilkS) hide)
    (fp_text value VAL** (at 4.826 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.99898) (layers *.Cu F.SilkS))
    (model walter/details/hole.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_details:hole_2mm (layer F.Cu) (tedit 575A9053)
    (at 116.356 72.875)
    (descr "Hole 2mm")
    (fp_text reference "hole_2mm_(2)" (at 0 -2.794) (layer F.SilkS) hide)
    (fp_text value VAL** (at 4.826 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.99898) (layers *.Cu F.SilkS))
    (model walter/details/hole.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module p_w_switch:PCB_PUSH (layer F.Cu) (tedit 57E16C59)
    (at 187.356 83.875)
    (descr "PCB pushbutton, Tyco FSM6x6 series")
    (tags pushbutton)
    (fp_text reference SW2 (at -4.88 -4.348 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 5.588) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.25044 -3.2512) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.25044 3.2512) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole circle (at 2.25044 -3.2512) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -2.25044 3.2512) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (model "${KIPRJMOD}/pcb libs/packages3d/switch/pcb_push.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module p_w_pth_resistors:RC03 (layer F.Cu) (tedit 57E16197)
    (at 190.356 108.875)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R2 (at -0.006 -1.789) (layer F.SilkS))
    (fp_text value 10k (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 61 PT_ROMCS))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model "${KIPRJMOD}/pcb libs/packages3d/pth_resistors/rc03.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module p_w_conn_d-sub:DB_9M (layer F.Cu) (tedit 585B0C1F)
    (at 115.856 95.875 270)
    (descr "D-SUB 9 pin plug, Tyco P/N 4-338168-2")
    (fp_text reference DB9 (at -0.092 -11.883 450) (layer F.SilkS))
    (fp_text value Kempston (at 0 0 270) (layer F.SilkS))
    (pad "" thru_hole circle (at 12.49426 -7.112 270) (size 5.00126 5.00126) (drill 3.2004) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -8.382 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 -0.24892)) (layers *.Cu *.Mask)
      (net 64 J3-Left))
    (pad 4 thru_hole oval (at 2.77114 -8.382 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 -0.24892)) (layers *.Cu *.Mask)
      (net 65 J4-Right))
    (pad 5 thru_hole oval (at 5.53974 -8.382 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 -0.24892)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -2.77114 -8.382 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 -0.24892)) (layers *.Cu *.Mask)
      (net 63 J2-Down))
    (pad 1 thru_hole oval (at -5.53974 -8.382 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 -0.24892)) (layers *.Cu *.Mask)
      (net 62 J1-Up))
    (pad 6 thru_hole oval (at -4.15544 -5.842 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 0.24892)) (layers *.Cu *.Mask)
      (net 66 J6-Fire))
    (pad 7 thru_hole oval (at -1.3843 -5.842 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 0.24892)) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 8 thru_hole oval (at 1.3843 -5.842 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 0.24892)) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 4.15544 -5.842 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 0.24892)) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -12.49426 -7.112 270) (size 5.00126 5.00126) (drill 3.2004) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/pcb libs/packages3d/conn_d-sub/db_9m.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ZX_Spectrum:ZX_CONN (layer F.Cu) (tedit 585AA497)
    (at 147.749 117.284)
    (descr "ZX CON")
    (tags "CONN ZX")
    (fp_text reference J1 (at -15.311 0.089) (layer F.SilkS))
    (fp_text value ZX_48K_EDGE (at 2.54 -6.35) (layer F.SilkS) hide)
    (pad A28 connect oval (at 43.18 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 5 A11))
    (pad A27 connect oval (at 40.64 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 6 A9))
    (pad A26 connect oval (at 38.1 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 7 BUSACK))
    (pad A25 connect oval (at 35.56 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 8 ROMCS48K))
    (pad A24 connect oval (at 33.02 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 9 A4))
    (pad A23 connect oval (at 30.48 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 10 A5))
    (pad A22 connect oval (at 27.94 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 11 A6))
    (pad A21 connect oval (at 25.4 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 12 A7))
    (pad A20 connect oval (at 22.86 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 13 RESET))
    (pad A19 connect oval (at 20.32 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 14 BUSREQ))
    (pad B28 connect oval (at 43.18 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 15 TOP28))
    (pad B27 connect oval (at 40.64 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 16 A10))
    (pad B26 connect oval (at 38.1 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 A8))
    (pad B25 connect oval (at 35.56 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 18 RFSH))
    (pad B24 connect oval (at 33.02 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 19 M1))
    (pad B23 connect oval (at 30.48 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 20 -12V))
    (pad B22 connect oval (at 27.94 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 21 +12V))
    (pad B21 connect oval (at 25.4 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 22 WAIT))
    (pad B20 connect oval (at 22.86 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 23 -5V))
    (pad B19 connect oval (at 20.32 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 24 WR))
    (pad A18 connect oval (at 17.78 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 25 U))
    (pad A17 connect oval (at 15.24 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 26 V))
    (pad A16 connect oval (at 12.7 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 27 Y))
    (pad A15 connect oval (at 10.16 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 28 VIDEO/OE2_128K))
    (pad A14 connect oval (at 7.62 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad A13 connect oval (at 5.08 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 29 IOREQGE))
    (pad A12 connect oval (at 2.54 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 30 A3))
    (pad A11 connect oval (at 0 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 31 A2))
    (pad A10 connect oval (at -2.54 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 32 A1))
    (pad A9 connect oval (at -5.08 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 33 A0))
    (pad A8 connect oval (at -7.62 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 34 CLOCK))
    (pad A7 connect oval (at -10.16 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad A6 connect oval (at -12.7 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad A4 connect oval (at -17.78 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 35 +9V))
    (pad A3 connect oval (at -20.32 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad A2 connect oval (at -22.86 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 36 A12))
    (pad A1 connect oval (at -25.4 0) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 37 A14))
    (pad B18 connect oval (at 17.78 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 38 RD))
    (pad B17 connect oval (at 15.24 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 39 IOREQ))
    (pad B16 connect oval (at 12.7 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 40 MREQ))
    (pad B15 connect oval (at 10.16 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 41 HALT))
    (pad B14 connect oval (at 7.62 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 42 NMI))
    (pad B13 connect oval (at 5.08 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 43 INT))
    (pad B12 connect oval (at 2.54 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 44 D4))
    (pad B11 connect oval (at 0 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 45 D3))
    (pad B10 connect oval (at -2.54 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 46 D5))
    (pad B9 connect oval (at -5.08 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 47 D6))
    (pad B8 connect oval (at -7.62 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 48 D2))
    (pad B7 connect oval (at -10.16 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 49 D1))
    (pad B6 connect oval (at -12.7 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 50 D0))
    (pad B4 connect oval (at -17.78 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 51 OE1_128K))
    (pad B3 connect oval (at -20.32 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 52 D7))
    (pad B2 connect oval (at -22.86 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 53 A13))
    (pad B1 connect oval (at -25.4 0) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 54 A15))
  )
  (module p_w_pin_strip:pin_socket_2 (layer F.Cu) (tedit 585B0B95)
    (at 132.311 101.879 90)
    (descr "Pin socket 2pin")
    (tags "CONN DEV")
    (fp_text reference JP1 (at 0 -2.5 90) (layer F.SilkS) hide)
    (fp_text value Joystick (at -0.254 -3.175 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 10 A5))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(JP1-Pad2)"))
    (model "${KIPRJMOD}/pcb libs/packages3d/pin_strip/pin_socket_2.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module p_w_pin_strip:pin_socket_2 (layer F.Cu) (tedit 585AA4BE)
    (at 116.69 76.733)
    (descr "Pin socket 2pin")
    (tags "CONN DEV")
    (fp_text reference P1 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value "Serial Pins" (at 0.381 2.286) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 65 J4-Right))
    (model "${KIPRJMOD}/pcb libs/packages3d/pin_strip/pin_socket_2.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module p_w_pth_resistors:RC03 (layer F.Cu) (tedit 57E16197)
    (at 155.856 85.375)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 10k (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 55 EP_CE))
    (model "${KIPRJMOD}/pcb libs/packages3d/pth_resistors/rc03.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module p_w_switch:PCB_PUSH (layer F.Cu) (tedit 57E16C59)
    (at 130.856 83.875)
    (descr "PCB pushbutton, Tyco FSM6x6 series")
    (tags pushbutton)
    (fp_text reference SW1 (at 5 -5 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 5.588) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.25044 -3.2512) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.25044 3.2512) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole circle (at 2.25044 -3.2512) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -2.25044 3.2512) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (model "${KIPRJMOD}/pcb libs/packages3d/switch/pcb_push.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module p_w_pth_diodes:diode_do35 (layer F.Cu) (tedit 582EF6F4)
    (at 190.356 104.375)
    (descr "Diode, DO-35 package")
    (fp_text reference D1 (at -0.133 -1.861) (layer F.SilkS))
    (fp_text value 1n4148 (at 0 -2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 8 ROMCS48K))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 61 PT_ROMCS))
    (model "${KIPRJMOD}/pcb libs/packages3d/pth_diodes/diode_do35.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text "December 2016" (at 119.356 113.375) (layer F.SilkS))
  (gr_line (start 133.525 69.85) (end 196.342 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "ZX Dandanator! Mini 2.1\n" (at 177.696 112.545) (layer F.SilkS))
  (gr_line (start 111.342 119.85) (end 111.342 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 196.342 119.85) (end 111.342 119.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 196.342 69.85) (end 196.342 119.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.342 69.85) (end 131.747 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.525 78.74) (end 133.525 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.747 78.74) (end 133.525 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.747 69.85) (end 131.747 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.356 115.875) (xy 192.356 115.875) (xy 192.356 111.875) (xy 196.356 111.875) (xy 196.356 115.875)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.356 70.875) (xy 118.356 70.875) (xy 118.356 74.875) (xy 114.356 74.875)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.356 114.875) (xy 118.356 114.875) (xy 118.356 118.875) (xy 114.356 118.875)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.356 114.875) (xy 118.356 114.875) (xy 118.356 118.875) (xy 114.356 118.875)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.356 70.875) (xy 118.356 70.875) (xy 118.356 74.875) (xy 114.356 74.875)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.356 115.875) (xy 192.356 115.875) (xy 192.356 111.875) (xy 196.356 111.875) (xy 196.356 115.875)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.356 77.875) (xy 194.356 77.875) (xy 194.356 70.875) (xy 195.356 70.875) (xy 195.356 118.875)
        (xy 193.356 118.875) (xy 193.356 114.875) (xy 120.356 114.875) (xy 120.356 118.875) (xy 112.356 118.875)
        (xy 112.356 70.875) (xy 119.356 70.875) (xy 119.356 77.875)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.356 77.875) (xy 194.356 77.875) (xy 194.356 70.875) (xy 195.356 70.875) (xy 195.356 118.875)
        (xy 193.356 118.875) (xy 193.356 114.875) (xy 120.356 114.875) (xy 120.356 118.875) (xy 112.356 118.875)
        (xy 112.356 70.875) (xy 119.356 70.875) (xy 119.356 77.875)
      )
    )
  )
)
