(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 0)
    (no_connects 0)
    (area 167.031599 59.767399 221.537601 145.007401)
    (thickness 1.6)
    (drawings 7)
    (tracks 327)
    (zones 0)
    (modules 16)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 1.05)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 203.4286 115.7224)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 ElmoTX)
  (net 2 ElmoRX)
  (net 3 GND)
  (net 4 HallA)
  (net 5 5V)
  (net 6 HallC)
  (net 7 I+)
  (net 8 I-)
  (net 9 HallB)
  (net 10 B-)
  (net 11 B+)
  (net 12 A-)
  (net 13 A+)
  (net 14 CMD-)
  (net 15 CMD+)
  (net 16 ENABLE)
  (net 17 IN3)
  (net 18 OUT1)
  (net 19 OUT3)
  (net 20 PortC_I-)
  (net 21 PortC_I+)
  (net 22 PortC_B-)
  (net 23 PortC_B+)
  (net 24 PortC_A-)
  (net 25 PortC_A+)
  (net 26 "Net-(J4-Pad1)")
  (net 27 "Net-(J4-Pad2)")
  (net 28 "Net-(J4-Pad3)")
  (net 29 VCC)
  (net 30 CANH)
  (net 31 CANL)
  (net 32 "Net-(1400ohms1-Pad2)")
  (net 33 LED2)
  (net 34 LED1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5V)
    (add_net A+)
    (add_net A-)
    (add_net B+)
    (add_net B-)
    (add_net CANH)
    (add_net CANL)
    (add_net CMD+)
    (add_net CMD-)
    (add_net ENABLE)
    (add_net ElmoRX)
    (add_net ElmoTX)
    (add_net GND)
    (add_net HallA)
    (add_net HallB)
    (add_net HallC)
    (add_net I+)
    (add_net I-)
    (add_net IN3)
    (add_net LED1)
    (add_net LED2)
    (add_net "Net-(1400ohms1-Pad2)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net OUT1)
    (add_net OUT3)
    (add_net PortC_A+)
    (add_net PortC_A-)
    (add_net PortC_B+)
    (add_net PortC_B-)
    (add_net PortC_I+)
    (add_net PortC_I-)
    (add_net VCC)
  )
  (net_class Small ""
    (clearance 0.2)
    (trace_width 0.1397)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module w_conn_pc:D-Sub_HD_26_F (layer F.Cu) (tedit 59B83A68)
    (at 193.9666 139.5984 180)
    (descr http://www.farnell.com/datasheets/1802103.pdf)
    (tags "D-Sub D Sub HD High Density")
    (fp_text reference J3 (at 0 6.35 180) (layer F.SilkS))
    (fp_text value "Amphenol FCI ICD26S13E4GX00LF" (at 0 -6.35 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 8.65 -2.54 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 6.36 -2.54 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 14 CMD-))
    (pad 3 thru_hole circle (at 4.07 -2.54 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 15 CMD+))
    (pad 4 thru_hole circle (at 1.78 -2.54 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 16 ENABLE))
    (pad 5 thru_hole circle (at -0.51 -2.54 180) (size 1.35 1.35) (drill 1.05) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -2.8 -2.54 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 17 IN3))
    (pad 7 thru_hole circle (at -5.09 -2.54 180) (size 1.35 1.35) (drill 1.05) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -7.38 -2.54 180) (size 1.35 1.35) (drill 1.05) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -9.67 -2.54 180) (size 1.35 1.35) (drill 1.05) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 9.8 0 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 7.51 0 180) (size 1.35 1.35) (drill 1.05) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 5.22 0 180) (size 1.35 1.35) (drill 1.05) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 2.93 0 180) (size 1.35 1.35) (drill 1.05) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 0.64 0 180) (size 1.35 1.35) (drill 1.05) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at -1.65 0 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 16 thru_hole circle (at -3.94 0 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 18 OUT1))
    (pad 17 thru_hole circle (at -6.23 0 180) (size 1.35 1.35) (drill 1.05) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at -8.52 0 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 19 OUT3))
    (pad 19 thru_hole circle (at 8.65 2.54 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 20 thru_hole circle (at 6.36 2.54 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 4.07 2.54 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 20 PortC_I-))
    (pad 22 thru_hole circle (at 1.78 2.54 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 21 PortC_I+))
    (pad 23 thru_hole circle (at -0.51 2.54 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 22 PortC_B-))
    (pad 24 thru_hole circle (at -2.8 2.54 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 23 PortC_B+))
    (pad 25 thru_hole circle (at -5.09 2.54 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 24 PortC_A-))
    (pad 26 thru_hole circle (at -7.38 2.54 180) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
      (net 25 PortC_A+))
    (pad 0 thru_hole circle (at 16.7 0 180) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask))
    (pad 0 thru_hole circle (at -16.7 0 180) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask))
    (model Connectors.3dshapes/DB15MC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ElmoGoldTwitter (layer B.Cu) (tedit 59B83F95)
    (at 193.8401 115.8494 90)
    (fp_text reference U1 (at 0.127 -0.3984 90) (layer B.SilkS) hide)
    (fp_text value ElmoGoldTwitter (at 0.127 0.6016 90) (layer F.SilkS) hide)
    (pad F1 thru_hole circle (at 14.224 12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask))
    (pad F2 thru_hole circle (at 14.224 11.684 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 13 A+))
    (pad F3 thru_hole circle (at 12.954 12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask))
    (pad F4 thru_hole circle (at 12.954 11.684 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 12 A-))
    (pad F5 thru_hole circle (at 11.684 12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask))
    (pad F6 thru_hole circle (at 11.684 11.684 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 11 B+))
    (pad F7 thru_hole circle (at 10.414 12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask))
    (pad F8 thru_hole circle (at 10.414 11.684 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 10 B-))
    (pad F9 thru_hole circle (at 9.144 12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask))
    (pad F10 thru_hole circle (at 9.144 11.684 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 7 I+))
    (pad F11 thru_hole circle (at 7.874 12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask))
    (pad F12 thru_hole circle (at 7.874 11.684 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Mask B.Cu)
      (net 8 I-))
    (pad F13 thru_hole circle (at 6.604 12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 4 HallA))
    (pad F14 thru_hole circle (at 6.604 11.684 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Mask B.Cu)
      (net 24 PortC_A-))
    (pad F15 thru_hole circle (at 5.334 12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 9 HallB))
    (pad F16 thru_hole circle (at 5.334 11.684 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Mask B.Cu)
      (net 25 PortC_A+))
    (pad F17 thru_hole circle (at 4.064 12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 6 HallC))
    (pad F18 thru_hole circle (at 4.064 11.684 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Mask B.Cu)
      (net 22 PortC_B-))
    (pad F19 thru_hole circle (at 2.794 12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 5 5V))
    (pad F20 thru_hole circle (at 2.794 11.684 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Mask B.Cu)
      (net 23 PortC_B+) (clearance 0.127))
    (pad F21 thru_hole circle (at 1.524 12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad F22 thru_hole circle (at 1.524 11.684 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 20 PortC_I-) (clearance 0.127))
    (pad F23 thru_hole circle (at 0.254 12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad F24 thru_hole circle (at 0.254 11.684 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 21 PortC_I+))
    (pad 1 thru_hole circle (at 8.382 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 30 CANH))
    (pad 2 thru_hole circle (at 8.382 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 31 CANL))
    (pad 3 thru_hole circle (at 7.112 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 ElmoTX))
    (pad 4 thru_hole circle (at 7.112 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 2 ElmoRX))
    (pad 5 thru_hole circle (at 5.842 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 5.842 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 4.572 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 8 thru_hole circle (at 4.572 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 9 thru_hole circle (at 3.302 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 15 CMD+))
    (pad 10 thru_hole circle (at 3.302 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 14 CMD-))
    (pad 12 thru_hole circle (at 2.032 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 5 5V))
    (pad 13 thru_hole circle (at 0.762 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Mask B.Cu)
      (net 3 GND))
    (pad 14 thru_hole circle (at 0.762 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 5 5V))
    (pad 15 thru_hole circle (at -0.508 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 34 LED1))
    (pad 16 thru_hole circle (at -0.508 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Mask B.Cu)
      (net 33 LED2))
    (pad 17 thru_hole circle (at -1.778 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at -1.778 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Mask B.Cu))
    (pad 19 thru_hole circle (at -3.048 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 19 OUT3))
    (pad 20 thru_hole circle (at -3.048 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 18 OUT1))
    (pad 21 thru_hole circle (at -4.318 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 22 thru_hole circle (at -4.318 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 23 thru_hole circle (at -5.588 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at -5.588 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at -6.858 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at -6.858 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 17 IN3))
    (pad 27 thru_hole circle (at -8.128 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at -8.128 -14.224 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 16 ENABLE))
    (pad 11 thru_hole circle (at 2.032 -12.954 90) (size 1.0668 1.0668) (drill 0.7112) (layers *.Mask B.Cu))
    (pad L1 thru_hole circle (at 14.097 3.9624 90) (size 1.75 1.75) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 VCC))
    (pad L2 thru_hole circle (at 14.097 1.9685 90) (size 1.75 1.75) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad M3 thru_hole circle (at 9.2456 15.24 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 "Net-(J4-Pad3)"))
    (pad M2 thru_hole circle (at 5.588 15.24 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(J4-Pad2)"))
    (pad M1 thru_hole circle (at 1.9558 15.24 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(J4-Pad1)"))
    (pad P1 thru_hole circle (at -1.6764 15.24 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND) (zone_connect 2))
    (pad P2 thru_hole circle (at -5.334 15.24 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 VCC) (zone_connect 2))
    (pad P3 thru_hole circle (at -9.017 15.24 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND) (zone_connect 2))
    (model Diodes_SMD.3dshapes/D_SMC_Standard.wrl
      (at (xyz 0 0.005 -0.005))
      (scale (xyz 1.95 1.95 2))
      (rotate (xyz 180 0 90))
    )
  )
  (module Connectors:DB9MC (layer F.Cu) (tedit 587FE23B)
    (at 198.4746 71.2724)
    (descr "Connecteur DB9 male couche")
    (tags "CONN DB9")
    (fp_text reference J1 (at -4.32 -11.43) (layer F.SilkS))
    (fp_text value DB9_MALE_MountingHoles (at -4.32 -5.08) (layer F.Fab))
    (pad "" thru_hole circle (at 7.24 -2.54) (size 3.81 3.81) (drill 3.05) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -18.16 -2.54) (size 3.81 3.81) (drill 3.05) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.79 0) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 ElmoTX))
    (pad 3 thru_hole circle (at -5.59 0) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 ElmoRX))
    (pad 4 thru_hole circle (at -8.25 0) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 30 CANH))
    (pad 5 thru_hole circle (at -11.05 0) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 9 thru_hole circle (at -9.65 -2.54) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -6.86 -2.54) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -4.19 -2.54) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -1.4 -2.54) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 31 CANL))
    (model ${KISYS3DMOD}/Connectors.3dshapes/DB9MC.wrl
      (at (xyz -0.22 0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pc:DB_15F-VGA (layer F.Cu) (tedit 59B8309B)
    (at 219.64142 76.40574 90)
    (descr "D-SUB 15 pin VGA socket, Tyco P/N 440467-1")
    (fp_text reference J2 (at 0 4.699 90) (layer F.SilkS))
    (fp_text value "Amphenol FCI ICD15S13E6GV00LF" (at 0 -8.509 90) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 12.49426 -2.47142 90) (size 5.00126 5.00126) (drill 3.2004) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -0.2667 -4.4704 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 HallA))
    (pad 2 thru_hole circle (at 2.0193 -4.4704 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 5V))
    (pad 1 thru_hole circle (at 4.31038 -4.4704 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole circle (at -2.56032 -4.4704 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 5V))
    (pad 5 thru_hole circle (at -4.84886 -4.4704 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 9 thru_hole circle (at -1.41478 -2.9718 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 HallC))
    (pad 8 thru_hole circle (at 0.87376 -2.9718 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 I+))
    (pad 7 thru_hole circle (at 3.16484 -2.9718 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 I-))
    (pad 6 thru_hole circle (at 5.45592 -2.9718 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 HallB))
    (pad "" thru_hole circle (at -12.49426 -2.47142 90) (size 5.00126 5.00126) (drill 3.2004) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -3.70586 -2.9718 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 4.31038 -1.47066 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 B-))
    (pad 12 thru_hole circle (at 2.0193 -1.47066 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 B+))
    (pad 13 thru_hole circle (at -0.26924 -1.4732 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 A-))
    (pad 14 thru_hole circle (at -2.56032 -1.47066 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 A+))
    (pad 15 thru_hole circle (at -4.84886 -1.47066 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Connectors.3dshapes/DB9MC.wrl
      (at (xyz 0 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_3pol (layer F.Cu) (tedit 56301605)
    (at 216.8906 113.6904 90)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J4 (at 3.5 -4.3 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 3.5 6 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(J4-Pad2)"))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 "Net-(J4-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(J4-Pad1)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_3pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer F.Cu) (tedit 59B70AF2)
    (at 216.8906 124.6834 90)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J5 (at 1.75 -4.3 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.75 6 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 VCC) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND) (zone_connect 2))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 59B81213)
    (at 198.8566 86.1244 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C1 (at 12.326 -8.89 270) (layer F.SilkS))
    (fp_text value "Nichicon UPW1J152MHD" (at 3.75 10.31 270) (layer F.Fab))
    (fp_text user %R (at 3.75 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 VCC) (zone_connect 2))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 59B81220)
    (at 179.2986 86.1244 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C2 (at 12.072 -8.89 270) (layer F.SilkS))
    (fp_text value "Nichicon UPW1J152MHD" (at 3.75 10.31 270) (layer F.Fab))
    (fp_text user %R (at 3.75 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 VCC) (zone_connect 2))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 203.3016 76.3524 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at 1 -3.81 180) (layer F.SilkS))
    (fp_text value "Nichicon UVK1V470MDD1TD" (at 1 3.81 180) (layer F.Fab))
    (fp_text user %R (at 1 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 5V))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 59B8081D)
    (at 171.6786 127.2794)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference J6 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 3.8) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 59B80823)
    (at 215.4286 97.9424)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference J7 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 3.8) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 59B8081F)
    (at 173.4286 76.7224)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference J8 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 3.8) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 59B80821)
    (at 217.6526 138.9634)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference J9 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 3.8) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 171.2976 105.6894 270)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference 1400ohms1 (at 0.09906 -3.0988 270) (layer F.SilkS))
    (fp_text value R (at -0.39878 4.20116 270) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 29 VCC))
    (pad 2 smd trapezoid (at 2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(1400ohms1-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 29 VCC))
    (pad 2 thru_hole rect (at 5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 32 "Net-(1400ohms1-Pad2)"))
  )
  (module LEDs:LED_RGB_1210 (layer F.Cu) (tedit 5979AE99)
    (at 172.0596 115.9764 270)
    (descr "RGB LED 3.2x2.7mm http://www.avagotech.com/docs/AV02-0610EN")
    (tags "LED 3227")
    (attr smd)
    (fp_text reference D1 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value LED_Dual_AACC (at 0 2.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -1.75 -0.7 90) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(1400ohms1-Pad2)"))
    (pad 2 smd rect (at -1.75 0.7 90) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(1400ohms1-Pad2)"))
    (pad 4 smd rect (at 1.75 -0.7 90) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 33 LED2))
    (pad 3 smd rect (at 1.75 0.7 90) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 34 LED1))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pc:LOGO (layer B.Cu) (tedit 0)
    (at 192.2526 125.8824 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (gr_text "If the drive is \ninstalled correctly,\nyou cannot \nread this text.\n" (at 194.5386 122.3264) (layer F.SilkS))
  (gr_text "Leg 1 Elmo Twitter PCB\nRevision 1\nJack Doan 9/12/2017" (at 189.4586 83.9724 90) (layer B.SilkS))
  (gr_line (start 221.4626 59.8424) (end 221.2086 59.8424) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 221.4626 144.9324) (end 221.4626 59.8424) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.1066 144.9324) (end 221.4626 144.9324) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.1066 59.8424) (end 167.1066 144.9324) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 221.2086 59.8424) (end 167.1066 59.8424) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 226.0346 58.8264) (xy 167.1066 59.8424) (xy 167.1066 144.9324) (xy 225.2726 144.9324)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 222.1484 104.1908) (xy 207.8228 104.1146) (xy 207.5942 115.4684) (xy 208.407 115.8748) (xy 222.2246 115.951)
      )
    )
  )
  (zone (net 29) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 226.0346 58.8264) (xy 166.5478 59.1312) (xy 165.3286 146.6342) (xy 225.7044 146.3294)
      )
    )
  )
)
