<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<wire x1="-81.788" y1="-50.8" x2="81.788" y2="-50.8" width="0" layer="20"/>
<wire x1="-81.788" y1="50.8" x2="-81.788" y2="-50.8" width="0" layer="20"/>
<wire x1="81.788" y1="50.8" x2="-81.788" y2="50.8" width="0" layer="20"/>
<wire x1="81.788" y1="-50.8" x2="81.788" y2="50.8" width="0" layer="20"/>
<text>NMR SADDLE COIL 
100 Degrees Aperture
2.049" Diameter Roll
PARALLEL Configuration</text>
</plain>
<libraries>
<library name="CONRADS">
<packages>
<package name="SOLDERPADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="CONRADS" package="SOLDERPADS" value="SOLDERPADS"/>
</elements>
<signals>
<signal name="COIL">
<contactref element="U$1" pad="P$1"/>
<contactref element="U$1" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
