(kicad_pcb (version 20171130) (host pcbnew 5.1.2-f72e74a~84~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 70)
    (tracks 378)
    (zones 0)
    (modules 24)
    (nets 52)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.2032)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VBUS)
  (net 3 +3V3)
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 /PIO0_14)
  (net 7 /PIO0_15)
  (net 8 /PIO0_16)
  (net 9 /PIO0_17)
  (net 10 /PIO0_18)
  (net 11 /PIO0_19)
  (net 12 /PIO0_20)
  (net 13 /PIO0_21)
  (net 14 /PIO0_22)
  (net 15 /~RESET~)
  (net 16 /PIO0_23)
  (net 17 /PIO0_24)
  (net 18 /PIO0_25)
  (net 19 /PIO0_26)
  (net 20 /PIO0_29)
  (net 21 /PIO0_30)
  (net 22 /PIO0_31)
  (net 23 /PIO1_0)
  (net 24 /PIO1_1)
  (net 25 /PIO1_2)
  (net 26 /PIO1_3)
  (net 27 /PIO1_4)
  (net 28 /PIO1_5)
  (net 29 /PIO1_6)
  (net 30 /PIO1_7)
  (net 31 /PIO1_8)
  (net 32 /PIO0_0)
  (net 33 /PIO0_1)
  (net 34 /PIO0_4)
  (net 35 /PIO0_5)
  (net 36 /PIO0_6)
  (net 37 /PIO0_7)
  (net 38 /PIO0_8)
  (net 39 /PIO0_9)
  (net 40 /PIO0_10)
  (net 41 /PIO0_11)
  (net 42 /PIO0_12)
  (net 43 /PIO0_13)
  (net 44 "Net-(J4-Pad3)")
  (net 45 "Net-(J4-Pad4)")
  (net 46 "Net-(J4-Pad2)")
  (net 47 /USB_DM)
  (net 48 /USB_DP)
  (net 49 "Net-(U1-Pad26)")
  (net 50 "Net-(S1-Pad4)")
  (net 51 "Net-(S2-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /PIO0_0)
    (add_net /PIO0_1)
    (add_net /PIO0_10)
    (add_net /PIO0_11)
    (add_net /PIO0_12)
    (add_net /PIO0_13)
    (add_net /PIO0_14)
    (add_net /PIO0_15)
    (add_net /PIO0_16)
    (add_net /PIO0_17)
    (add_net /PIO0_18)
    (add_net /PIO0_19)
    (add_net /PIO0_20)
    (add_net /PIO0_21)
    (add_net /PIO0_22)
    (add_net /PIO0_23)
    (add_net /PIO0_24)
    (add_net /PIO0_25)
    (add_net /PIO0_26)
    (add_net /PIO0_29)
    (add_net /PIO0_30)
    (add_net /PIO0_31)
    (add_net /PIO0_4)
    (add_net /PIO0_5)
    (add_net /PIO0_6)
    (add_net /PIO0_7)
    (add_net /PIO0_8)
    (add_net /PIO0_9)
    (add_net /PIO1_0)
    (add_net /PIO1_1)
    (add_net /PIO1_2)
    (add_net /PIO1_3)
    (add_net /PIO1_4)
    (add_net /PIO1_5)
    (add_net /PIO1_6)
    (add_net /PIO1_7)
    (add_net /PIO1_8)
    (add_net /USB_DM)
    (add_net /USB_DP)
    (add_net /VBUS)
    (add_net /~RESET~)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(S1-Pad4)")
    (add_net "Net-(S2-Pad4)")
    (add_net "Net-(U1-Pad26)")
  )
  (module Symbol:OSHW-Logo_5.7x6mm_SilkScreen locked (layer F.Cu) (tedit 5CFE7B3B)
    (at 175.895 100.33)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 144.5768 96.8756 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at -0.1016 1.4478 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 /VBUS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 144.5768 93.1164 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at -0.1016 -1.4478 270) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 171.3992 94.3216 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value .1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 165.9128 96.0374 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value .1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 155.321 92.964 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 1.397 90) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 156.7688 97.282 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 2.413 -0.0762 90) (layer F.SilkS))
    (fp_text value LED_ALT (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 176.149 94.742 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D2 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value LED_ALT (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical locked (layer B.Cu) (tedit 59FED5CC)
    (at 134.62 88.9 270)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (fp_text reference J1 (at 2.286 0) (layer B.SilkS))
    (fp_text value Conn_01x24 (at 0 -60.75 270) (layer B.Fab))
    (fp_text user %R (at 0 -29.21) (layer B.Fab))
    (pad 24 thru_hole oval (at 0 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /PIO0_14))
    (pad 23 thru_hole oval (at 0 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /PIO0_15))
    (pad 22 thru_hole oval (at 0 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /PIO0_16))
    (pad 21 thru_hole oval (at 0 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /PIO0_17))
    (pad 20 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /PIO0_18))
    (pad 19 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /PIO0_19))
    (pad 18 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /PIO0_20))
    (pad 17 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /PIO0_21))
    (pad 16 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /PIO0_22))
    (pad 15 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /~RESET~))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /PIO0_23))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /PIO0_24))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /PIO0_25))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /PIO0_26))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /PIO0_29))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /PIO0_30))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /PIO0_31))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /PIO1_0))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /PIO1_1))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /PIO1_2))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VBUS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical locked (layer B.Cu) (tedit 59FED5CC)
    (at 134.62 104.14 270)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (fp_text reference J2 (at -2.032 0) (layer B.SilkS))
    (fp_text value Conn_01x24 (at 0 -60.75 270) (layer B.Fab))
    (fp_text user %R (at 0 -29.21) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VBUS))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /PIO1_3))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /PIO1_4))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /PIO1_5))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /PIO1_6))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /PIO1_7))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /PIO1_8))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /PIO0_0))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /PIO0_1))
    (pad 15 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /PIO0_4))
    (pad 16 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /PIO0_5))
    (pad 17 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /PIO0_6))
    (pad 18 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /PIO0_7))
    (pad 19 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /PIO0_8))
    (pad 20 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /PIO0_9))
    (pad 21 thru_hole oval (at 0 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /PIO0_10))
    (pad 22 thru_hole oval (at 0 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /PIO0_11))
    (pad 23 thru_hole oval (at 0 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /PIO0_12))
    (pad 24 thru_hole oval (at 0 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /PIO0_13))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:USB_Micro_B_Female_10118194-0001LF (layer F.Cu) (tedit 5B07215D)
    (at 137.16 96.52 270)
    (descr http://portal.fciconnect.com/Comergent//fci/drawing/10118194.pdf)
    (fp_text reference J4 (at -3.937 0.381 180) (layer F.SilkS))
    (fp_text value 10118194-0001LF (at 0 7 90) (layer F.Fab))
    (fp_text user %R (at 0 2.84 90) (layer F.Fab))
    (pad 3 smd rect (at 0 0 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J4-Pad3)"))
    (pad 4 smd rect (at 0.65 0 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J4-Pad4)"))
    (pad 5 smd rect (at 1.3 0 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.65 0 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J4-Pad2)"))
    (pad 1 smd rect (at -1.3 0 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 /VBUS))
    (pad SH thru_hole oval (at 2.5 0 270) (size 1.25 0.95) (drill oval 0.85 0.55) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole oval (at -2.5 0 270) (size 1.25 0.95) (drill oval 0.85 0.55) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole oval (at -3.5 2.7 270) (size 1 1.55) (drill oval 0.5 1.15) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole oval (at 3.5 2.7 270) (size 1 1.55) (drill oval 0.5 1.15) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 162.179 100.838 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.43 45) (layer F.SilkS))
    (fp_text value 3K3 (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 45) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.875 0 45) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /PIO1_6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 141.605 99.06 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -2.413 0.254 90) (layer F.SilkS))
    (fp_text value 33 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /USB_DM))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 140.081 99.06 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -2.413 0 90) (layer F.SilkS))
    (fp_text value 33 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(J4-Pad3)"))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /USB_DP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 178.6128 92.6338)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at -2.5908 -0.4318) (layer F.SilkS))
    (fp_text value 3K3 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /~RESET~))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 178.6128 94.1578)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 2.4892 0.8382) (layer F.SilkS))
    (fp_text value 3K3 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /PIO0_31))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 167.513 98.679 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 3K3 (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 /PIO0_4))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 155.2448 97.282 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -2.54 0.0762 90) (layer F.SilkS))
    (fp_text value 330 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 178.6128 95.6818 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 330 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /PIO0_31))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Tactile_THT_6x6mm locked (layer F.Cu) (tedit 5AF34E1F)
    (at 193.421 93.1418 270)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1825910&DocType=Customer+Drawing&DocLang=English)
    (fp_text reference S1 (at -0.5334 2.2606 180) (layer F.SilkS))
    (fp_text value 1825910-6 (at 3.6322 7.0866 90) (layer F.Fab))
    (fp_text user %R (at 3.3782 2.286 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 4.5 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 /~RESET~))
    (pad 4 thru_hole circle (at 6.5 4.5 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 50 "Net-(S1-Pad4)"))
    (pad 2 thru_hole circle (at 6.5 0 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module digikey-footprints:Switch_Tactile_THT_6x6mm locked (layer F.Cu) (tedit 5AF34E1F)
    (at 186.182 93.1418 270)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1825910&DocType=Customer+Drawing&DocLang=English)
    (fp_text reference S2 (at -0.4318 2.2606 180) (layer F.SilkS))
    (fp_text value 1825910-6 (at 3.6322 7.0866 90) (layer F.Fab))
    (fp_text user %R (at 3.3782 2.286 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 6.5 0 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 6.5 4.5 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 51 "Net-(S2-Pad4)"))
    (pad 3 thru_hole circle (at 0 4.5 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 /PIO0_31))
  )
  (module Package_QFP:LQFP-48_7x7mm_P0.5mm locked (layer F.Cu) (tedit 5C18330E)
    (at 167.64 96.52 315)
    (descr "LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (attr smd)
    (fp_text reference U1 (at 0 -5.85 135) (layer F.SilkS))
    (fp_text value LPC51U68JBD48 (at 0 5.85 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -4.1625 -2.75 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /PIO0_23))
    (pad 2 smd roundrect (at -4.1625 -2.25 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /PIO0_24))
    (pad 3 smd roundrect (at -4.1625 -1.75 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /PIO0_25))
    (pad 4 smd roundrect (at -4.1625 -1.25 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /PIO0_26))
    (pad 5 smd roundrect (at -4.1625 -0.75 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /USB_DP))
    (pad 6 smd roundrect (at -4.1625 -0.25 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /USB_DM))
    (pad 7 smd roundrect (at -4.1625 0.25 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /PIO0_29))
    (pad 8 smd roundrect (at -4.1625 0.75 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /PIO0_30))
    (pad 9 smd roundrect (at -4.1625 1.25 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /PIO0_31))
    (pad 10 smd roundrect (at -4.1625 1.75 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /PIO1_0))
    (pad 11 smd roundrect (at -4.1625 2.25 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /PIO1_1))
    (pad 12 smd roundrect (at -4.1625 2.75 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /PIO1_2))
    (pad 13 smd roundrect (at -2.75 4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /PIO1_3))
    (pad 14 smd roundrect (at -2.25 4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /PIO1_4))
    (pad 15 smd roundrect (at -1.75 4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /PIO1_5))
    (pad 16 smd roundrect (at -1.25 4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 17 smd roundrect (at -0.75 4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 18 smd roundrect (at -0.25 4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 19 smd roundrect (at 0.25 4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 20 smd roundrect (at 0.75 4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /PIO1_6))
    (pad 21 smd roundrect (at 1.25 4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /PIO1_7))
    (pad 22 smd roundrect (at 1.75 4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /PIO1_8))
    (pad 23 smd roundrect (at 2.25 4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /PIO0_0))
    (pad 24 smd roundrect (at 2.75 4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /PIO0_1))
    (pad 25 smd roundrect (at 4.1625 2.75 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 26 smd roundrect (at 4.1625 2.25 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(U1-Pad26)"))
    (pad 27 smd roundrect (at 4.1625 1.75 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /PIO0_4))
    (pad 28 smd roundrect (at 4.1625 1.25 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /PIO0_5))
    (pad 29 smd roundrect (at 4.1625 0.75 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /PIO0_6))
    (pad 30 smd roundrect (at 4.1625 0.25 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /PIO0_7))
    (pad 31 smd roundrect (at 4.1625 -0.25 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /PIO0_8))
    (pad 32 smd roundrect (at 4.1625 -0.75 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /PIO0_9))
    (pad 33 smd roundrect (at 4.1625 -1.25 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /PIO0_10))
    (pad 34 smd roundrect (at 4.1625 -1.75 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /PIO0_11))
    (pad 35 smd roundrect (at 4.1625 -2.25 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /PIO0_12))
    (pad 36 smd roundrect (at 4.1625 -2.75 315) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /PIO0_13))
    (pad 37 smd roundrect (at 2.75 -4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /PIO0_14))
    (pad 38 smd roundrect (at 2.25 -4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /PIO0_15))
    (pad 39 smd roundrect (at 1.75 -4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /PIO0_16))
    (pad 40 smd roundrect (at 1.25 -4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /PIO0_17))
    (pad 41 smd roundrect (at 0.75 -4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 42 smd roundrect (at 0.25 -4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 43 smd roundrect (at -0.25 -4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /PIO0_18))
    (pad 44 smd roundrect (at -0.75 -4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /PIO0_19))
    (pad 45 smd roundrect (at -1.25 -4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /PIO0_20))
    (pad 46 smd roundrect (at -1.75 -4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /PIO0_21))
    (pad 47 smd roundrect (at -2.25 -4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /PIO0_22))
    (pad 48 smd roundrect (at -2.75 -4.1625 315) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /~RESET~))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-48_7x7mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5A02FF57)
    (at 149.987 95.123)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 3.0226 -2.8448) (layer F.SilkS))
    (fp_text value " AZ1117CH-3.3TRG1" (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 /VBUS))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Symbol_6.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 142.875 93.98 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference LOGO1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value Logo_Open_Hardware_Small (at 0.75 0) (layer B.Fab) hide)
  )
  (gr_text ISP (at 183.896 101.346) (layer F.SilkS))
  (gr_text RESET (at 191.262 101.346) (layer F.SilkS))
  (gr_text SDA4 (at 160.02 87.503) (layer F.SilkS))
  (gr_text SCL4 (at 162.56 87.503) (layer F.SilkS))
  (gr_text SDA1 (at 165.1 87.503) (layer F.SilkS))
  (gr_text SCL1 (at 167.64 87.503) (layer F.SilkS))
  (gr_text TX (at 167.767 105.6005) (layer F.SilkS))
  (gr_text RX (at 165.1 105.6005) (layer F.SilkS))
  (gr_text 2054-LPC51U68JBD48-breakout (at 142.6464 101.3206) (layer F.SilkS))
  (gr_arc (start 194.31 87.63) (end 194.945 87.63) (angle -90) (layer Edge.Cuts) (width 0.3556))
  (gr_arc (start 194.31 105.41) (end 194.31 106.045) (angle -90) (layer Edge.Cuts) (width 0.3556))
  (gr_arc (start 133.35 105.41) (end 132.715 105.41) (angle -90) (layer Edge.Cuts) (width 0.3556))
  (gr_arc (start 133.35 87.63) (end 133.35 86.995) (angle -90) (layer Edge.Cuts) (width 0.3556))
  (gr_text https://github.com/johnwinans/2054-LPC51U68JBD48-breakout (at 162.56 101.6) (layer B.SilkS))
  (gr_text "Copyright © 2018 John Winans" (at 150.368 99.187) (layer B.SilkS))
  (gr_text 0.14 (at 193.04 90.551) (layer F.SilkS))
  (gr_text 0.15 (at 190.5 90.551) (layer F.SilkS))
  (gr_text 0.16 (at 187.96 90.551) (layer F.SilkS))
  (gr_text 0.17 (at 185.42 90.551) (layer F.SilkS))
  (gr_text 0.18 (at 182.88 90.551) (layer F.SilkS))
  (gr_text 0.19 (at 180.34 90.551) (layer F.SilkS))
  (gr_text 0.20 (at 177.8 90.551) (layer F.SilkS))
  (gr_text 0.21 (at 175.26 90.551) (layer F.SilkS))
  (gr_text 0.22 (at 172.72 90.551) (layer F.SilkS))
  (gr_text ~RST~ (at 170.18 90.805) (layer F.SilkS))
  (gr_text 0.23 (at 167.64 90.551) (layer F.SilkS))
  (gr_text 0.24 (at 165.1 90.551) (layer F.SilkS))
  (gr_text 0.25 (at 162.56 90.551) (layer F.SilkS))
  (gr_text 0.26 (at 160.02 90.551) (layer F.SilkS))
  (gr_text 0.29 (at 157.48 90.551) (layer F.SilkS))
  (gr_text 0.30 (at 154.94 90.551) (layer F.SilkS))
  (gr_text 0.31 (at 152.4 90.551) (layer F.SilkS))
  (gr_text 1.0 (at 149.86 90.551) (layer F.SilkS))
  (gr_text 1.1 (at 147.32 90.551) (layer F.SilkS))
  (gr_text 1.2 (at 144.78 90.551) (layer F.SilkS))
  (gr_text GND (at 142.24 90.551) (layer F.SilkS))
  (gr_text +3V3 (at 139.7 90.551) (layer F.SilkS))
  (gr_text GND (at 137.16 90.551) (layer F.SilkS))
  (gr_text VBUS (at 134.62 90.551) (layer F.SilkS))
  (gr_text 0.13 (at 193.04 102.616) (layer F.SilkS))
  (gr_text 0.12 (at 190.5 102.616) (layer F.SilkS))
  (gr_text 0.11 (at 187.96 102.616) (layer F.SilkS))
  (gr_text 0.10 (at 185.42 102.616) (layer F.SilkS))
  (gr_text 0.9 (at 182.88 102.616) (layer F.SilkS))
  (gr_text 0.8 (at 180.34 102.616) (layer F.SilkS))
  (gr_text 0.7 (at 177.8 102.616) (layer F.SilkS))
  (gr_text 0.6 (at 175.26 102.616) (layer F.SilkS))
  (gr_text 0.5 (at 172.72 102.616) (layer F.SilkS))
  (gr_text 0.4 (at 170.18 102.616) (layer F.SilkS))
  (gr_text 0.1 (at 167.64 102.616) (layer F.SilkS))
  (gr_text 0.0 (at 165.1 102.616) (layer F.SilkS))
  (gr_text 1.8 (at 162.56 102.616) (layer F.SilkS))
  (gr_text 1.7 (at 160.02 102.616) (layer F.SilkS))
  (gr_text 1.6 (at 157.48 102.616) (layer F.SilkS))
  (gr_text 1.5 (at 154.94 102.616) (layer F.SilkS))
  (gr_text 1.4 (at 152.4 102.616) (layer F.SilkS))
  (gr_text 1.3 (at 149.86 102.616) (layer F.SilkS))
  (gr_text GND (at 147.32 102.616) (layer F.SilkS))
  (gr_text GND (at 144.78 102.616) (layer F.SilkS))
  (gr_text GND (at 142.24 102.616) (layer F.SilkS))
  (gr_text +3V3 (at 139.7 102.616) (layer F.SilkS))
  (gr_text GND (at 137.16 102.616) (layer F.SilkS))
  (gr_text VBUS (at 134.62 102.616) (layer F.SilkS))
  (dimension 19.05 (width 0.15) (layer Dwgs.User)
    (gr_text "0.7500 in" (at 202.595 96.52 270) (layer Dwgs.User))
    (feature1 (pts (xy 194.945 106.045) (xy 201.881421 106.045)))
    (feature2 (pts (xy 194.945 86.995) (xy 201.881421 86.995)))
    (crossbar (pts (xy 201.295 86.995) (xy 201.295 106.045)))
    (arrow1a (pts (xy 201.295 106.045) (xy 200.708579 104.918496)))
    (arrow1b (pts (xy 201.295 106.045) (xy 201.881421 104.918496)))
    (arrow2a (pts (xy 201.295 86.995) (xy 200.708579 88.121504)))
    (arrow2b (pts (xy 201.295 86.995) (xy 201.881421 88.121504)))
  )
  (dimension 62.23 (width 0.15) (layer Dwgs.User)
    (gr_text "2.4500 in" (at 163.83 110.52) (layer Dwgs.User))
    (feature1 (pts (xy 194.945 106.045) (xy 194.945 109.806421)))
    (feature2 (pts (xy 132.715 106.045) (xy 132.715 109.806421)))
    (crossbar (pts (xy 132.715 109.22) (xy 194.945 109.22)))
    (arrow1a (pts (xy 194.945 109.22) (xy 193.818496 109.806421)))
    (arrow1b (pts (xy 194.945 109.22) (xy 193.818496 108.633579)))
    (arrow2a (pts (xy 132.715 109.22) (xy 133.841504 109.806421)))
    (arrow2b (pts (xy 132.715 109.22) (xy 133.841504 108.633579)))
  )
  (gr_line (start 132.715 105.41) (end 132.715 87.63) (layer Edge.Cuts) (width 0.3556))
  (gr_line (start 194.31 106.045) (end 133.35 106.045) (layer Edge.Cuts) (width 0.3556))
  (gr_line (start 194.945 87.63) (end 194.945 105.41) (layer Edge.Cuts) (width 0.3556))
  (gr_line (start 133.35 86.995) (end 194.31 86.995) (layer Edge.Cuts) (width 0.3556))
  (dimension 15.24 (width 0.15) (layer Dwgs.User)
    (gr_text "0.6000 in" (at 125.7 96.52 270) (layer Dwgs.User))
    (feature1 (pts (xy 132.08 104.14) (xy 126.413579 104.14)))
    (feature2 (pts (xy 132.08 88.9) (xy 126.413579 88.9)))
    (crossbar (pts (xy 127 88.9) (xy 127 104.14)))
    (arrow1a (pts (xy 127 104.14) (xy 126.413579 103.013496)))
    (arrow1b (pts (xy 127 104.14) (xy 127.586421 103.013496)))
    (arrow2a (pts (xy 127 88.9) (xy 126.413579 90.026504)))
    (arrow2b (pts (xy 127 88.9) (xy 127.586421 90.026504)))
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.715 86.995) (xy 194.945 86.995) (xy 194.945 106.045) (xy 132.715 106.045)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.715 86.995) (xy 194.945 86.995) (xy 194.945 106.045) (xy 132.715 106.045)
      )
    )
  )
)
