(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 123)
    (zones 0)
    (modules 13)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.254)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.4 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.25 1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VIN)
  (net 2 GND)
  (net 3 /VOUT)
  (net 4 /EN_UV)
  (net 5 /PG)
  (net 6 "Net-(C3-Pad2)")
  (net 7 /SET)
  (net 8 /OUTS)
  (net 9 /ILIM)
  (net 10 /PGFB)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /EN_UV)
    (add_net /ILIM)
    (add_net /OUTS)
    (add_net /PG)
    (add_net /PGFB)
    (add_net /SET)
    (add_net /VIN)
    (add_net /VOUT)
    (add_net GND)
    (add_net "Net-(C3-Pad2)")
  )
  (module Straightener01:C_1206_Split (layer F.Cu) (tedit 5E50749A)
    (at 134 100.99)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.59) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 4 smd roundrect (at 1.4875 0.5) (size 1.425 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175)
      (net 8 /OUTS))
    (pad 3 smd roundrect (at 1.4875 -0.5) (size 1.425 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175)
      (net 3 /VOUT))
    (pad 2 smd roundrect (at -1.4875 0.5) (size 1.425 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 -0.5) (size 1.425 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175)
      (net 6 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_5x5.3 (layer B.Cu) (tedit 5BCA39CF)
    (at 107.6 100.8)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C1 (at 0 4.35) (layer B.SilkS))
    (fp_text value 22uF (at 0 -4.35) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 2.2 0) (size 3 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.15625)
      (net 2 GND))
    (pad 1 smd roundrect (at -2.2 0) (size 3 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.15625)
      (net 1 /VIN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 125.5 104.9 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 1.5) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.82) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 /VIN))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5E336D88)
    (at 137.6 103 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 2.9 0) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175)
      (net 6 "Net-(C3-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 /SET))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Straightener01:DFN-10 (layer F.Cu) (tedit 5E445622)
    (at 133 104 270)
    (fp_text reference IC1 (at 0 -2.925 90) (layer F.SilkS) hide)
    (fp_text value LT3045EDD (at 0 -3.925 90) (layer F.Fab))
    (pad 1 smd rect (at -1 1.525 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /VIN))
    (pad 2 smd rect (at -0.5 1.525 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /VIN))
    (pad 3 smd rect (at 0 1.525 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /EN_UV))
    (pad 4 smd rect (at 0.5 1.525 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /PG))
    (pad 5 smd rect (at 1 1.525 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 9 /ILIM))
    (pad 6 smd rect (at 1 -1.525 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /PGFB))
    (pad 7 smd rect (at 0.5 -1.525 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /SET))
    (pad 8 smd rect (at 0 -1.525 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -0.5 -1.525 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /OUTS))
    (pad 10 smd rect (at -1 -1.525 270) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /VOUT))
    (pad 11 smd rect (at 0 0 270) (size 2.38 1.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/Straightener01.3dshapes/DFN-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Straightener01:C112640 (layer F.Cu) (tedit 5E222216)
    (at 104.9 100.8 270)
    (fp_text reference J1 (at 0 -4.1 90) (layer F.SilkS) hide)
    (fp_text value C112640 (at 0 -5.1 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 4.475 0 270) (size 1.67 4.72) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.5) (clearance 0.5))
    (pad 2 smd rect (at -4.475 0 270) (size 1.67 4.72) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.5) (clearance 0.5))
    (pad 1 smd rect (at 0 0 270) (size 0.86 4.72) (layers F.Cu F.Paste F.Mask)
      (net 1 /VIN) (solder_mask_margin 0.5) (clearance 0.5))
    (pad 2 smd rect (at 4.925 0 270) (size 1.35 4.72) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.5) (clearance 0.5))
    (pad 2 smd rect (at -4.925 0 270) (size 1.35 4.72) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.5) (clearance 0.5))
    (model ${KIPRJMOD}/Straightener01.3dshapes/C112640.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Straightener01:C112640 (layer F.Cu) (tedit 5E222216)
    (at 150.1 100.8 90)
    (fp_text reference J2 (at 0 -4.1 90) (layer F.SilkS) hide)
    (fp_text value C112640 (at 0 -5.1 90) (layer F.Fab) hide)
    (pad 2 smd rect (at -4.925 0 90) (size 1.35 4.72) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.5) (clearance 0.5))
    (pad 2 smd rect (at 4.925 0 90) (size 1.35 4.72) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.5) (clearance 0.5))
    (pad 1 smd rect (at 0 0 90) (size 0.86 4.72) (layers F.Cu F.Paste F.Mask)
      (net 3 /VOUT) (solder_mask_margin 0.5) (clearance 0.5))
    (pad 2 smd rect (at -4.475 0 90) (size 1.67 4.72) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.5) (clearance 0.5))
    (pad 2 smd rect (at 4.475 0 90) (size 1.67 4.72) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.5) (clearance 0.5))
    (model ${KIPRJMOD}/Straightener01.3dshapes/C112640.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 111.7 108.8)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.1) (layer F.SilkS))
    (fp_text value SET (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /EN_UV))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /VIN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 129.8 104 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -2.1 0 180) (layer F.SilkS))
    (fp_text value 200k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /VIN))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /PG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5E34BF9A)
    (at 132.06 106.8)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -2.36 0) (layer F.SilkS))
    (fp_text value 249 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /ILIM))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 139.5 103 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 2.1 0.02 180) (layer F.SilkS))
    (fp_text value SET (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /SET))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 135.5 106.8 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 1.1) (layer F.SilkS))
    (fp_text value 453k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /PGFB))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /VOUT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5E34BF9D)
    (at 133.81 108.4 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 2.31 0.3) (layer F.SilkS))
    (fp_text value 49.9k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /PGFB))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Feb 2020" (at 150.3 94) (layer F.SilkS))
  (gr_text "Dylan Oh" (at 145.2 98.5) (layer F.Mask))
  (gr_text Straightener01 (at 122 94.9) (layer F.Mask))
  (gr_line (start 103 110) (end 102 109) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102 94) (end 103 93) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152 93) (end 153 94) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152 110) (end 153 109) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.9 113) (end 146.9 110) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.3 113) (end 122.3 110) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.9 113) (end 125.3 113) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.3 110) (end 103 110) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152 110) (end 146.9 110) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153 94) (end 153 109) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103 93) (end 152 93) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102 109) (end 102 94) (layer Edge.Cuts) (width 0.05))
  (zone (net 10) (net_name /PGFB) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 135.03 105.12) (xy 135.4 105.49) (xy 135.4 109.1) (xy 134.1 109.1) (xy 134.1 104.88)
        (xy 135.03 104.88)
      )
    )
  )
  (zone (net 7) (net_name /SET) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 140.2 105.31) (xy 135.67 105.26) (xy 135.03 104.62) (xy 135.03 104.34) (xy 136.12 103.25)
        (xy 140.2 103.25)
      )
    )
  )
  (zone (net 6) (net_name "Net-(C3-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 140.2 103) (xy 136.4 103) (xy 136.4 99.7) (xy 133.4 99.7) (xy 133.4 100.85)
        (xy 131.1 100.85) (xy 131.1 98.6) (xy 140.2 98.6)
      )
    )
  )
  (zone (net 3) (net_name /VOUT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 136.2 101) (xy 134.7 101) (xy 134.7 102.1) (xy 135.57 102.1) (xy 135.57 102.79)
        (xy 135.22 103.14) (xy 134.01 103.14) (xy 134.01 102.7) (xy 133.7 102.39) (xy 133.7 100)
        (xy 136.2 100)
      )
    )
  )
  (zone (net 3) (net_name /VOUT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 137.7 107.5) (xy 135.7 107.5) (xy 135.7 105.6) (xy 137.7 105.6)
      )
    )
  )
  (zone (net 9) (net_name /ILIM) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 131.98 107.505) (xy 130.57 107.51) (xy 130.57 105.28) (xy 130.98 104.87) (xy 131.98 104.87)
      )
    )
  )
  (zone (net 5) (net_name /PG) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 130.5 104.38) (xy 131.98 104.38) (xy 131.98 104.62) (xy 130.77 104.62) (xy 130.27 105.12)
        (xy 130.27 105.5) (xy 128.81 105.5) (xy 128.81 104.2) (xy 130.32 104.2)
      )
    )
  )
  (zone (net 1) (net_name /VIN) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.98 103.62) (xy 130.51 103.62) (xy 130.21 103.92) (xy 127 103.92) (xy 127 99.8)
        (xy 128.81 99.8) (xy 128.81 102.37) (xy 131.98 102.37)
      )
    )
  )
  (zone (net 1) (net_name /VIN) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.4 105.8) (xy 102 105.8) (xy 102 95.8) (xy 128.4 95.8)
      )
    )
  )
  (zone (net 3) (net_name /VOUT) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153 102.8) (xy 134.4 102.8) (xy 133.5 101.9) (xy 133.5 99.9) (xy 153 99.9)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103 93) (xy 152 93) (xy 153 94) (xy 153 109) (xy 152 110)
        (xy 146.9 110) (xy 143.9 113) (xy 125.3 113) (xy 122.3 110) (xy 103 110)
        (xy 102 109) (xy 102 106.1) (xy 128.7 106.1) (xy 128.7 95.5) (xy 102 95.5)
        (xy 102 94)
      )
    )
  )
  (zone (net 1) (net_name /VIN) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.4 105.8) (xy 125.6 105.8) (xy 125.6 95.8) (xy 128.4 95.8)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.3 95.8) (xy 125.3 105.8) (xy 102 105.8) (xy 102 102.7) (xy 107.2 102.7)
        (xy 107.2 98.9) (xy 102 98.9) (xy 102 95.8)
      )
    )
  )
  (zone (net 1) (net_name /VIN) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.9 102.4) (xy 102 102.4) (xy 102 99.2) (xy 106.9 99.2)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153 94) (xy 153 109) (xy 152 110) (xy 146.9 110) (xy 143.9 113)
        (xy 125.3 113) (xy 122.3 110) (xy 103 110) (xy 102 109) (xy 102 94)
        (xy 103 93) (xy 152 93)
      )
    )
  )
  (zone (net 1) (net_name /VIN) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.710161 102.5) (xy 102 102.5) (xy 102 99) (xy 107.710161 99)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153 94) (xy 153 99.6) (xy 133.2 99.6) (xy 133.2 102.1) (xy 134.2 103.1)
        (xy 153 103.1) (xy 153 109) (xy 152 110) (xy 146.9 110) (xy 143.9 113)
        (xy 125.3 113) (xy 122.3 110) (xy 103 110) (xy 102 109) (xy 102 106.1)
        (xy 128.7 106.1) (xy 128.7 95.5) (xy 102 95.5) (xy 102 94) (xy 103 93)
        (xy 127 93) (xy 152 93)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 103 93) (xy 152 93) (xy 153 94) (xy 153 109) (xy 152 110)
        (xy 146.9 110) (xy 143.9 113) (xy 125.3 113) (xy 122.3 110) (xy 103 110)
        (xy 102 109) (xy 102 102.8) (xy 108 102.8) (xy 108 98.7) (xy 102 98.7)
        (xy 102 94)
      )
    )
    (polygon
      (pts
        (xy 130.8 98.3) (xy 130.8 101.15) (xy 133.4 101.15) (xy 133.4 102.51) (xy 133.8 102.91)
        (xy 133.8 109.4) (xy 135.7 109.4) (xy 135.699688 107.8) (xy 138.000157 107.8) (xy 138 105.6)
        (xy 140.5 105.6) (xy 140.5 98.3)
      )
    )
    (polygon
      (pts
        (xy 126.7 99.49) (xy 126.7 104.2) (xy 128.5 104.2) (xy 128.5 105.8) (xy 130.3 105.8)
        (xy 130.3 107.8) (xy 132.25 107.8) (xy 132.25 102.07) (xy 129.1 102.07) (xy 129.1 99.49)
      )
    )
  )
)
