(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1)
  (general
    (links 141)
    (no_connects 0)
    (area 74.244762 54 147.835239 133.380001)
    (thickness 1.6)
    (drawings 59)
    (tracks 810)
    (zones 0)
    (modules 105)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.1)
    (zone_45_only yes)
    (trace_min 0.15)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.4)
    (via_drill 0.2)
    (via_min_size 0.4)
    (via_min_drill 0.2)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.7 1.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 89.632 85.7434)
    (visible_elements 7FFEFE7F)
    (pcbplotparams
      (layerselection 0x010f8_80000007)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory prod))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /ID_SD_EEPROM)
  (net 3 /ID_SC_EEPROM)
  (net 4 /P3V3_HAT)
  (net 5 /P5V_HAT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.15)
    (via_dia 0.4)
    (via_drill 0.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ID_SC_EEPROM)
    (add_net /ID_SD_EEPROM)
    (add_net /P3V3_HAT)
    (add_net /P5V_HAT)
    (add_net GND)
  )
  (module SMD_Packages:SSOP-20 (layer F.Cu) (tedit 5A9F4E5E)
    (at 92.299 87.369 270)
    (descr "SSOP 20 pins")
    (tags "CMS SSOP SMD")
    (attr smd)
    (fp_text reference ADC1 (at 4.383 -0.209 360) (layer F.SilkS))
    (fp_text value SSOP-20 (at 0 0.635 270) (layer F.Fab))
    (pad 1 smd rect (at -3.571 2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at -3.571 -2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 3.571 -2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 3.571 2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.921 2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.286 2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -1.6256 2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -0.9652 2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -0.3302 2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 0.3302 2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 0.9906 2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 1.6256 2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 2.286 2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 2.921 2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 2.921 -2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 2.286 -2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 1.6256 -2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 0.9906 -2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 18 smd rect (at 0.3302 -2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 /P3V3_HAT))
    (pad 19 smd rect (at -0.3302 -2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at -0.9652 -2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at -1.6256 -2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at -2.286 -2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at -2.921 -2.667 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model SMD_Packages.3dshapes/SSOP-20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.255 0.33 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AA1E7D6)
    (at 141.022 71.686 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R23 10k" (at 0 1.27 90) (layer F.SilkS))
    (fp_text value R_0805 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5AA1E7DC)
    (at 141.022 76.258 270)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED10 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value LED_1206 (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5AA1F845)
    (at 139.745 84.913 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R22 10M" (at 1.8054 0.2255 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5AA1E7CD)
    (at 141.784 85.656 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at -2.1125 0 180) (layer B.SilkS))
    (fp_text value C_0805 (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 /P5V_HAT))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5AA1E817)
    (at 140.768 81.338 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T20 2301" (at -0.254 -2.032 90) (layer B.SilkS))
    (fp_text value SOT-23 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 360) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 5 /P5V_HAT))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5AA1E811)
    (at 140.768 84.64)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T19 2302" (at -0.254 2.032) (layer F.SilkS))
    (fp_text value SOT-23 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module hole (layer F.Cu) (tedit 5AA01D04)
    (at 85.5695 82.6559)
    (fp_text reference GND (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value hole (at 0 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module hole (layer F.Cu) (tedit 5AA1E912)
    (at 85.5695 85.0934)
    (fp_text reference VREF (at 0 1.651 90) (layer F.SilkS))
    (fp_text value hole (at 0 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AA01C5E)
    (at 93.524 111.056 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R22 10k" (at -3.048 0 180) (layer F.SilkS))
    (fp_text value R_0805 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AA01C64)
    (at 104.7 68.13)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R21 10k" (at 0 1.27) (layer F.SilkS))
    (fp_text value R_0805 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5A9F0211)
    (at 87.1945 73.2309)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference "C1 100u" (at 1.2 -3) (layer F.SilkS))
    (fp_text value CP_Radial_D5.0mm_P2.50mm (at 1.25 3.81) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /P3V3_HAT))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5A9F4CE4)
    (at 105.97 108.262 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference "C2 100u" (at 1.2 -3 180) (layer F.SilkS))
    (fp_text value CP_Radial_D5.0mm_P2.50mm (at 1.25 3.81 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /P5V_HAT))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AA194BC)
    (at 100.455 69.898 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R19 500k" (at 0 -1.397 270) (layer F.SilkS))
    (fp_text value R_0805 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMA_EndLaunch (layer F.Cu) (tedit 5AA1EE61)
    (at 111.074 116.866)
    (fp_text reference "GPIO 18" (at -0.024 -5.302) (layer F.SilkS))
    (fp_text value SMA_EndLaunch (at 0 -6.35) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.77 -3.25) (size 1.7 1.7) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.77 -3.25) (size 1.7 1.7) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -2) (size 1 3) (layers F.Cu F.Paste F.Mask))
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 5A9F4E4D)
    (at 121.464 111.31 180)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference "U9 7366" (at -5.5 0 270) (layer F.SilkS))
    (fp_text value SOIC-14_N (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 12 smd rect (at -1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 10 smd rect (at 1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AA1F7DD)
    (at 96.71 68.057 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R18 10k" (at 0.065 -1.206 180) (layer F.SilkS))
    (fp_text value R_0805 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module generic_pad (layer F.Cu) (tedit 5AA1E954)
    (at 93.27 77.274)
    (fp_text reference OSC (at -1.524 0) (layer F.SilkS))
    (fp_text value generic_pad (at 0 -6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask))
  )
  (module generic_pad (layer F.Cu) (tedit 5AA1E950)
    (at 93.27 78.798)
    (fp_text reference CLK (at -1.524 0) (layer F.SilkS))
    (fp_text value generic_pad (at 0 -6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask))
  )
  (module SMA_EndLaunch (layer F.Cu) (tedit 5AA1EE74)
    (at 78.538 87.053 270)
    (fp_text reference INPUT (at 0 -5.25 270) (layer F.SilkS))
    (fp_text value SMA_EndLaunch (at 0 -6.35 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.77 -3.25 270) (size 1.7 1.7) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.77 -3.25 270) (size 1.7 1.7) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -2 270) (size 1 3) (layers F.Cu F.Paste F.Mask))
  )
  (module smolpot (layer F.Cu) (tedit 5A9F4AF6)
    (at 95.79 75.82 180)
    (fp_text reference POT1 (at 0 -1.778 180) (layer F.SilkS))
    (fp_text value smolpot (at 0 -2.54 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 2.54 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module SMA_EndLaunch (layer F.Cu) (tedit 5AA1F773)
    (at 90.246 116.866)
    (fp_text reference CLOCK (at 6.536 -3.1726) (layer F.SilkS))
    (fp_text value SMA_EndLaunch (at 0 -6.35) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.77 -3.25) (size 1.7 1.7) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.77 -3.25) (size 1.7 1.7) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -2) (size 1 3) (layers F.Cu F.Paste F.Mask))
  )
  (module SMA_EndLaunch (layer F.Cu) (tedit 5AA1EE6A)
    (at 131.394 116.866)
    (fp_text reference ENABLE (at 0.053 -5.256) (layer F.SilkS))
    (fp_text value SMA_EndLaunch (at 0 -6.35) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.77 -3.25) (size 1.7 1.7) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.77 -3.25) (size 1.7 1.7) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -2) (size 1 3) (layers F.Cu F.Paste F.Mask))
  )
  (module "ASTMK Osc 2012" (layer F.Cu) (tedit 5A9EFB9F)
    (at 89.206 78.798)
    (fp_text reference OSC1 (at 0 -1.524) (layer F.SilkS))
    (fp_text value "ASTMK Osc 2012" (at 0 -6.35) (layer F.Fab))
    (pad 4 smd rect (at 0.1 -0.45) (size 0.2 0.7) (drill (offset 0 -0.1)) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.1 0.45) (size 0.2 0.7) (drill (offset 0 0.1)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.8 0) (size 0.6 1.4) (drill (offset 0.1 0)) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -0.8 0) (size 0.6 1.4) (drill (offset -0.1 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B97)
    (at 91.324 107.519 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R15 10M" (at 1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B89)
    (at 87.099 107.519 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R13 10M" (at 1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B7C)
    (at 82.874 107.519 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R11 10M" (at 1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B9D)
    (at 93.4365 107.519 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R16 10M" (at -1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B8F)
    (at 89.2115 107.519 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R14 10M" (at -1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B84)
    (at 84.9865 107.519 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R12 10M" (at -1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B79)
    (at 80.7615 107.519 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R10 10M" (at -1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A9F4D78)
    (at 80.7615 107.519 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -2.1125 0 180) (layer F.SilkS))
    (fp_text value C_0805 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4BA1)
    (at 95.549 107.519 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R17 10M" (at 1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A9F4D8C)
    (at 95.549 107.519 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at -2.1125 0 180) (layer F.SilkS))
    (fp_text value C_0805 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A9F4D89)
    (at 93.4365 107.519 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at -2.1125 0 180) (layer F.SilkS))
    (fp_text value C_0805 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A9F4D86)
    (at 91.324 107.519 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at -2.1125 0 180) (layer F.SilkS))
    (fp_text value C_0805 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A9F4D83)
    (at 89.2115 107.519 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at -2.1125 0 180) (layer F.SilkS))
    (fp_text value C_0805 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A9F4D7F)
    (at 87.099 107.519 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at -2.1125 0 180) (layer F.SilkS))
    (fp_text value C_0805 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A9F4D7D)
    (at 84.9865 107.519 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at -2.1125 0 180) (layer F.SilkS))
    (fp_text value C_0805 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A9F4D7A)
    (at 82.874 107.519 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at -2.1125 0 180) (layer F.SilkS))
    (fp_text value C_0805 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5AA1F5F3)
    (at 87.682 84.4434 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference "C8 100n" (at 0.65 0.8125 180) (layer F.SilkS))
    (fp_text value C_0402 (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B6F)
    (at 95.549 95.494 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R9 10k" (at 1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B64)
    (at 91.324 95.494 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R7 10k" (at 1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9EEED0)
    (at 87.099 95.494 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R5 10k" (at 1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B53)
    (at 82.874 95.494 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R3 10k" (at 1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B68)
    (at 93.4365 95.494 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R8 10k" (at -1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B5E)
    (at 89.2115 95.494 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R6 10k" (at -1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B57)
    (at 84.9865 95.494 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R4 10k" (at -1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A9F4DDC)
    (at 93.599 68.844 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T1 2302" (at -0.325 1.95 270) (layer F.SilkS))
    (fp_text value SOT-23 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A9F4E32)
    (at 95.549 103.944 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T18 2301" (at -0.325 1.95 90) (layer F.SilkS))
    (fp_text value SOT-23 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A9F4E2E)
    (at 93.4365 100.5315 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T17 2301" (at -0.325 1.95 90) (layer F.SilkS))
    (fp_text value SOT-23 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A9F4E29)
    (at 91.324 103.944 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T16 2301" (at -0.325 1.95 90) (layer F.SilkS))
    (fp_text value SOT-23 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A9F4E24)
    (at 89.2115 100.5315 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T15 2301" (at -0.325 1.95 90) (layer F.SilkS))
    (fp_text value SOT-23 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A9F4E21)
    (at 87.099 103.944 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T14 2301" (at -0.325 1.95 90) (layer F.SilkS))
    (fp_text value SOT-23 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A9F4E1D)
    (at 84.9865 100.5315 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T13 2301" (at -0.325 1.95 90) (layer F.SilkS))
    (fp_text value SOT-23 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A9F4E15)
    (at 82.874 103.944 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T12 2301" (at -0.325 1.95 90) (layer F.SilkS))
    (fp_text value SOT-23 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A9F4E0D)
    (at 80.7615 100.5315 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T11 2301" (at -0.325 1.95 90) (layer F.SilkS))
    (fp_text value SOT-23 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5A9EED0F)
    (at 95.549 95.494 270)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED2 (at 3.014 -0.0065 360) (layer F.SilkS))
    (fp_text value LED_1206 (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5A9EED0F)
    (at 93.4365 95.494 270)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED2 (at 3.014 -0.0065 360) (layer F.SilkS))
    (fp_text value LED_1206 (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5A9EED0F)
    (at 91.324 95.494 270)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED2 (at 3.014 -0.0065 360) (layer F.SilkS))
    (fp_text value LED_1206 (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5A9EED0F)
    (at 89.2115 95.494 270)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED2 (at 3.014 -0.0065 360) (layer F.SilkS))
    (fp_text value LED_1206 (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5A9EED0F)
    (at 87.099 95.494 270)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED2 (at 3.014 -0.0065 360) (layer F.SilkS))
    (fp_text value LED_1206 (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5A9EED0F)
    (at 84.9865 95.494 270)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED2 (at 3.014 -0.0065 360) (layer F.SilkS))
    (fp_text value LED_1206 (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5A9EED0F)
    (at 82.874 95.494 270)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED2 (at 3.014 -0.0065 360) (layer F.SilkS))
    (fp_text value LED_1206 (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5A9EED0F)
    (at 80.7615 95.494 270)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED2 (at 3.014 -0.0065 360) (layer F.SilkS))
    (fp_text value LED_1206 (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A9F4E04)
    (at 110.174 106.3815 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T10 2302" (at -0.325 -1.95 180) (layer B.SilkS))
    (fp_text value SOT-23 (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A9F4DE1)
    (at 110.174 75.344 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T3 2302" (at -0.325 -1.95 180) (layer B.SilkS))
    (fp_text value SOT-23 (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A9F4DE3)
    (at 110.174 79.7315 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T4 2302" (at -0.325 -1.95 180) (layer B.SilkS))
    (fp_text value SOT-23 (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A9F4DE9)
    (at 110.174 84.2815 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T5 2302" (at -0.325 -1.95 180) (layer B.SilkS))
    (fp_text value SOT-23 (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A9F4DF3)
    (at 110.174 88.669 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T6 2302" (at -0.325 -1.95 180) (layer B.SilkS))
    (fp_text value SOT-23 (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A9F4DF6)
    (at 110.174 93.219 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T7 2302" (at -0.325 -1.95 180) (layer B.SilkS))
    (fp_text value SOT-23 (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A9F4DFC)
    (at 110.174 97.6065 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T8 2302" (at -0.325 -1.95 180) (layer B.SilkS))
    (fp_text value SOT-23 (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A9F4DFF)
    (at 110.174 102.1565 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T9 2302" (at -0.325 -1.95 180) (layer B.SilkS))
    (fp_text value SOT-23 (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5AA1F266)
    (at 87.682 88.9934 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference "C9 100n" (at 0.325 0.975 180) (layer F.SilkS))
    (fp_text value C_0402 (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5AA1F268)
    (at 87.682 90.9434 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference "C7 100n" (at 0.325 -0.975 180) (layer F.SilkS))
    (fp_text value C_0402 (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5AA1F2D2)
    (at 88.982 82.9809 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference "C4 100n" (at -2.275 0 180) (layer F.SilkS))
    (fp_text value C_0402 (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 5AA1F43A)
    (at 92.882 89.1559 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference "C6 10u" (at -0.0006 -1.3955 270) (layer B.SilkS))
    (fp_text value C_1206 (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /P3V3_HAT))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A9F4DBE)
    (at 88.074 81.519 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R20 27" (at 0 1.3 180) (layer F.SilkS))
    (fp_text value R_0805 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5A9F4D46)
    (at 92.299 81.519)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference "C3 10u" (at 0 -1.4625) (layer F.SilkS))
    (fp_text value C_1206 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5AA1E871)
    (at 112.574 104.452)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference "LG8 97" (at 0 2.032) (layer F.SilkS))
    (fp_text value SOT-23-6 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5AA1E879)
    (at 112.574 100.134)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference "LG7 97" (at 0 2.032) (layer F.SilkS))
    (fp_text value SOT-23-6 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5AA1E888)
    (at 112.574 95.562)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference "LG6 97" (at 0 2.032) (layer F.SilkS))
    (fp_text value SOT-23-6 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5A9DF7AD)
    (at 112.574 91.244)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference "LG5 97" (at 0 2.032) (layer F.SilkS))
    (fp_text value SOT-23-6 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5AA1E88E)
    (at 112.574 86.672)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference "LG4 97" (at 0 2.032) (layer F.SilkS))
    (fp_text value SOT-23-6 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5AA1E894)
    (at 112.574 82.354)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference "LG3 97" (at 0 2.032) (layer F.SilkS))
    (fp_text value SOT-23-6 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5AA1E89D)
    (at 112.574 77.782)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference "LG2 97" (at 0 2.032) (layer F.SilkS))
    (fp_text value SOT-23-6 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 5A9DE9B2)
    (at 132.894 102.42 180)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference "U5 7366" (at -5.5 0 270) (layer F.SilkS))
    (fp_text value SOIC-14_N (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 12 smd rect (at -1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 10 smd rect (at 1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 5A9DE9AF)
    (at 121.464 102.42 180)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference "U4 7366" (at -5.5 0 270) (layer F.SilkS))
    (fp_text value SOIC-14_N (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 12 smd rect (at -1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 10 smd rect (at 1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 5A9DE9B5)
    (at 132.894 93.53 180)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference "U6 7366" (at -5.5 0 270) (layer F.SilkS))
    (fp_text value SOIC-14_N (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 12 smd rect (at -1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 10 smd rect (at 1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 5A9DE9A9)
    (at 121.464 93.53 180)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference "U3 7366" (at -5.5 0 270) (layer F.SilkS))
    (fp_text value SOIC-14_N (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 12 smd rect (at -1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 10 smd rect (at 1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 5A9DE9B8)
    (at 132.894 84.64 180)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference "U7 7366" (at -5.5 0 270) (layer F.SilkS))
    (fp_text value SOIC-14_N (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 12 smd rect (at -1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 10 smd rect (at 1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 5A9DE9A6)
    (at 121.464 84.64 180)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference "U2 7366" (at -5.5 0 270) (layer F.SilkS))
    (fp_text value SOIC-14_N (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 12 smd rect (at -1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 10 smd rect (at 1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 5A9DE9BC)
    (at 132.894 75.75 180)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference "U8 7366" (at -5.5 0 270) (layer F.SilkS))
    (fp_text value SOIC-14_N (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 12 smd rect (at -1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 10 smd rect (at 1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 5A9DB816)
    (at 121.464 75.75 180)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference "U1 7366" (at -5.5 0 270) (layer F.SilkS))
    (fp_text value SOIC-14_N (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 12 smd rect (at -1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 10 smd rect (at 1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x20 locked (layer B.Cu) (tedit 5A9DFA09)
    (at 86.92 65.59)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference J3 (at 0 1.905) (layer B.SilkS))
    (fp_text value 40HAT (at 0 3.1) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 /P3V3_HAT))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 /P5V_HAT))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 /P5V_HAT))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 6 thru_hole oval (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 8 thru_hole oval (at 7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 10 thru_hole oval (at 10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 11 thru_hole oval (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 12 thru_hole oval (at 12.7 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 13 thru_hole oval (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 14 thru_hole oval (at 15.24 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 15 thru_hole oval (at 17.78 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 16 thru_hole oval (at 17.78 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 17 thru_hole oval (at 20.32 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 18 thru_hole oval (at 20.32 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 19 thru_hole oval (at 22.86 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 20 thru_hole oval (at 22.86 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 21 thru_hole oval (at 25.4 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 22 thru_hole oval (at 25.4 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 23 thru_hole oval (at 27.94 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 24 thru_hole oval (at 27.94 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 25 thru_hole oval (at 30.48 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 26 thru_hole oval (at 30.48 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 27 thru_hole oval (at 33.02 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 /ID_SD_EEPROM))
    (pad 28 thru_hole oval (at 33.02 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 /ID_SC_EEPROM))
    (pad 29 thru_hole oval (at 35.56 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 30 thru_hole oval (at 35.56 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 31 thru_hole oval (at 38.1 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 32 thru_hole oval (at 38.1 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 33 thru_hole oval (at 40.64 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 34 thru_hole oval (at 40.64 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 35 thru_hole oval (at 43.18 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 36 thru_hole oval (at 43.18 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 37 thru_hole oval (at 45.72 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 38 thru_hole oval (at 45.72 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 39 thru_hole oval (at 48.26 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 40 thru_hole oval (at 48.26 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x20.wrl
      (at (xyz 0.95 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module project_footprints:NPTH_3mm_ID locked (layer F.Cu) (tedit 58E34364)
    (at 82.04 64.31)
    (fp_text reference H1 (at 0.06 0.09) (layer F.SilkS))
    (fp_text value 3mm_Mounting_Hole (at 0 -2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 1.6))
  )
  (module project_footprints:NPTH_3mm_ID locked (layer F.Cu) (tedit 58E34364)
    (at 140.04 64.33)
    (fp_text reference H2 (at 0.06 0.09) (layer F.SilkS))
    (fp_text value 3mm_Mounting_Hole (at 0 -2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 1.6))
  )
  (module project_footprints:NPTH_3mm_ID locked (layer F.Cu) (tedit 58E34364)
    (at 82.04 113.32)
    (fp_text reference H3 (at 0.06 0.09) (layer F.SilkS))
    (fp_text value 3mm_Mounting_Hole (at 0 -2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 1.6))
  )
  (module project_footprints:NPTH_3mm_ID locked (layer F.Cu) (tedit 58E34364)
    (at 140.03 113.31)
    (fp_text reference H4 (at 0.06 0.09) (layer F.SilkS))
    (fp_text value 3mm_Mounting_Hole (at 0 -2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 1.6))
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5AA1E8A4)
    (at 112.574 73.464)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference "LG1 97" (at 0 2.032) (layer F.SilkS))
    (fp_text value SOT-23-6 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5AA1934B)
    (at 141.022 96.832 270)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED1 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value LED_1206 (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A9DF96E)
    (at 141.476 101.14 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R1 10k" (at 0 1.27 90) (layer F.SilkS))
    (fp_text value R_0805 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /P5V_HAT))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A9F4DD7)
    (at 141.476 92.377 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "T2 2302" (at -3.302 0 270) (layer F.SilkS))
    (fp_text value SOT-23 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5AA1F28E)
    (at 87.682 85.7434 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference "C5 100n" (at 0.325 -0.8125 180) (layer F.SilkS))
    (fp_text value C_0402 (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A9F4B4E)
    (at 80.7615 95.494 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "R2 10k" (at -1.7875 0 360) (layer B.SilkS))
    (fp_text value R_0805 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "SPI ACT" (at 142.8 76.258 90) (layer F.Mask))
  (gr_text "REFERENCE \nVOLTAGE\nADJUST" (at 103.376 74.724) (layer F.SilkS))
  (gr_text ENABLE (at 142.8 96.832 90) (layer F.Mask))
  (gr_text LSB (at 97.715 95.689) (layer F.Mask))
  (gr_text "Email: sporillium@gmail.com" (at 83.6195 75.1809 90) (layer F.Mask))
  (gr_text "Ellie D. Martin-Eberhardt" (at 82.3195 75.3434 90) (layer F.Mask))
  (gr_text "Raspberry Pi Integrator \nModule v0.1\n" (at 80.207 75.1809 90) (layer F.Mask))
  (gr_line (start 78.546356 63.817611) (end 78.546356 113.817611) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 81.546356 63.817611) (end 81.546356 60.817611) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.546356 60.817611) (end 81.546356 60.817611) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 140.546356 63.817611) (end 143.546356 63.817611) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.546356 113.817611) (end 143.546356 63.817611) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 81.546356 113.817611) (end 78.546356 113.817611) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 81.546356 116.817611) (end 140.546356 116.817611) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 140.546356 113.817611) (end 140.546356 116.817611) (angle -89.9) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0.1) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 144.1 133.38) (xy 77.6 133.38) (xy 77.6 59.08) (xy 144.1 59.08)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.1 128.3) (xy 77.6 128.3) (xy 77.6 54) (xy 144.1 54)
      )
    )
  )
  (zone (net 5) (net_name /P5V_HAT) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0.1) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 147.193 129.54) (xy 75.057 129.54) (xy 75.057 54.61) (xy 147.193 54.61)
      )
    )
  )
)
