<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="-2.54" x2="46.97" y2="-2.54" width="0" layer="20"/>
<wire x1="46.97" y1="-2.54" x2="46.97" y2="54.28" width="0" layer="20"/>
<wire x1="46.97" y1="54.28" x2="0" y2="54.28" width="0" layer="20"/>
<wire x1="0" y1="54.28" x2="0" y2="-2.54" width="0" layer="20"/>
<text>Rev A</text>
<text>Tom Hobson
RGB Controller</text>
<text>DC 12v</text>
<text>+V</text>
<text>+V</text>
<text>Solder all
connections on
underside</text>
</plain>
<libraries>
<library name="transistor-fet">
<description>&lt;b&gt;Field Effect Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
Symbols changed according to IEC617&lt;p&gt; 
All types, packages and assignment to symbols and pins checked&lt;p&gt;
Package outlines partly checked&lt;p&gt;
&lt;p&gt;
JFET = junction FET&lt;p&gt;
IGBT-x = insulated gate bipolar transistor&lt;p&gt;
x=N: NPN; x=P: PNP&lt;p&gt;
IGFET-mc-nnn; (IGFET=insulated gate field effect transistor)&lt;P&gt;
m=D: depletion mode (Verdr&amp;auml;ngungstyp)&lt;p&gt;
m=E: enhancement mode (Anreicherungstyp)&lt;p&gt;
c: N=N-channel; P=P-Channel&lt;p&gt;
GDSB: gate, drain, source, bulk&lt;p&gt;
&lt;p&gt;
by R. Vogg  15.March.2002</description>
<packages>
<package name="TO220">
<description>&lt;b&gt;TO 220 horizontal&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
<package name="PNA460XM">
</package>
</packages>
</library>
<library name="Arduino-clone">
<description>Arduino Clone pinheaders
By cl@xganon.com
http://www.xganon.com</description>
<packages>
<package name="NANO">
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2041">
<description>.100" (2.54mm) Center Header - 4 Pin</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="transistor-fet" package="TO220" value="IRF540">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistor-fet" package="TO220" value="IRF540">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="transistor-fet" package="TO220" value="IRF540">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="CN1" library="adafruit" package="DCJACK_2MM_PTH" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Arduino-clone" package="NANO" value="NANO">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="U$3" library="adafruit" package="PNA460XM" value="PNA460XM"/>
<element name="X3" library="con-molex" package="22-23-2041" value="22-23-2041">
<attribute name="OC_NEWARK" value="38C0355"/>
<attribute name="MPN" value="22-23-2041"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462920"/>
</element>
<element name="X4" library="con-molex" package="22-23-2041" value="22-23-2041">
<attribute name="OC_NEWARK" value="38C0355"/>
<attribute name="MPN" value="22-23-2041"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462920"/>
</element>
</elements>
<signals>
<signal name="GNDBREAK">
<contactref element="CN1" pad="GNDBREAK"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="1"/>
<contactref element="U$1" pad="D3"/>
</signal>
<signal name="N$2">
<contactref element="Q2" pad="1"/>
<contactref element="U$1" pad="D5"/>
</signal>
<signal name="N$3">
<contactref element="Q3" pad="1"/>
<contactref element="U$1" pad="D6"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="3"/>
<contactref element="CN1" pad="GND"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="BLUE">
<contactref element="Q1" pad="2"/>
<contactref element="X3" pad="3"/>
<contactref element="X4" pad="3"/>
</signal>
<signal name="GREEN">
<contactref element="Q2" pad="2"/>
<contactref element="X3" pad="2"/>
<contactref element="X4" pad="2"/>
</signal>
<signal name="RED">
<contactref element="Q3" pad="2"/>
<contactref element="X3" pad="1"/>
<contactref element="X4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="CN1" pad="PWR"/>
<contactref element="X3" pad="4"/>
<contactref element="X4" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="5V"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="U$3" pad="1"/>
<contactref element="U$1" pad="D11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
