(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 16)
    (no_connects 0)
    (area 158.924999 96.924999 170.075001 117.075001)
    (thickness 1.6)
    (drawings 6)
    (tracks 64)
    (zones 0)
    (modules 10)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.65 2.65)
    (pad_drill 2.65)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 164 106)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 /OUT)
  (net 4 "Net-(JP1-Pad1)")
  (net 5 "Net-(JP1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.381)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /OUT)
    (add_net GND)
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP1-Pad3)")
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 164.1 110)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -0.2 1.3) (layer F.SilkS))
    (fp_text value .01u (at 0 -1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 59FE3AC3)
    (at 167 114)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (fp_text reference J2 (at 0 -3.5) (layer Cmts.User))
    (fp_text value Conn_01x01 (at 0 3.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.65 2.65) (drill 2.65) (layers *.Cu))
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 59FE3ABE)
    (at 167 100)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (fp_text reference J3 (at 0 -3.5) (layer Cmts.User))
    (fp_text value Conn_01x01 (at 0 3.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.65 2.65) (drill 2.65) (layers *.Cu))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 165.2 103.9)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.3 -1.4) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /OUT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23W (layer F.Cu) (tedit 5997FF17)
    (at 161.5 107 180)
    (descr "SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3")
    (tags SOT-23W)
    (attr smd)
    (fp_text reference U1 (at -0.3 -2.4 360) (layer F.SilkS))
    (fp_text value DRV5023BIQDBZR (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 2.45 270) (layer F.Fab))
    (pad 1 smd rect (at -1.2 -0.95 180) (size 1 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -1.2 0.95 180) (size 1 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /OUT))
    (pad 3 smd rect (at 1.2 0 180) (size 1 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23W.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S3B-PH-K_03x2.00mm_Angled (layer B.Cu) (tedit 58D3FE32)
    (at 168 105 270)
    (descr "JST PH series connector, S3B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J1 (at -1.5 2.3 270) (layer B.SilkS))
    (fp_text value Conn_01x03 (at 2 -7.25 270) (layer B.Fab))
    (fp_text user %R (at 2 -2.5 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 /OUT))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S3B-PH-K_03x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 162.55 103.9 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0.35 1.4 180) (layer F.SilkS))
    (fp_text value C (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /OUT))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module hlib:jumper_0603 (layer B.Cu) (tedit 5A0BC7DC)
    (at 163 106.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference JP1 (at 4.55 0 270) (layer B.SilkS))
    (fp_text value Jumper_NC_Dual (at 0.45 -1.2 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Mask)
      (net 3 /OUT))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Mask)
      (net 4 "Net-(JP1-Pad1)"))
    (pad 3 smd rect (at 2.25 0 270) (size 0.8 0.75) (layers B.Cu B.Mask)
      (net 5 "Net-(JP1-Pad3)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module hlib:jumper_0603 (layer B.Cu) (tedit 5A0BC7DC)
    (at 161.3 107.75 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference JP2 (at -3.05 0 90) (layer B.SilkS))
    (fp_text value Jumper_NC_Dual (at 0.45 -1.2 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Mask)
      (net 5 "Net-(JP1-Pad3)"))
    (pad 3 smd rect (at 2.25 0 90) (size 0.8 0.75) (layers B.Cu B.Mask)
      (net 4 "Net-(JP1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Horizontal2_Inline_Narrow_Oval (layer F.Cu) (tedit 58CE52AF)
    (at 165.5 108.27 90)
    (descr "TO-92 horizontal, leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U2 (at -1.63 0.8 90) (layer F.SilkS))
    (fp_text value DRV5023BIQLPGM (at 1.27 -10.03 90) (layer F.Fab))
    (fp_text user %R (at 1.27 1.78 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(JP1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 5 "Net-(JP1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Horizontal2_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "S\n+\n-" (at 166.6 106.9) (layer B.SilkS))
  (gr_text "Mag \nLimit \nSwitch\nv1" (at 162 100.5) (layer B.SilkS))
  (gr_line (start 170 117) (end 170 97) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159 117) (end 170 117) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159 97) (end 159 117) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170 97) (end 159 97) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159 97) (xy 170 97) (xy 170 117) (xy 159 117)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159 97) (xy 170 97) (xy 170 117) (xy 159 117)
      )
    )
  )
)
