<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="20.32" y2="0" width="0" layer="20"/>
<wire x1="20.32" y1="0" x2="20.42" y2="28.23" width="0" layer="20"/>
<wire x1="20.42" y1="28.23" x2="0.1" y2="28.23" width="0" layer="20"/>
<wire x1="0.1" y1="28.23" x2="0" y2="0" width="0" layer="20"/>
<hole x="17.78" y="2.54" drill="3"/>
<text>ATTiny Proto Board</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>7</text>
<text>6</text>
<text>5</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>7</text>
<text>6</text>
<text>5</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>Top Plane=VCC</text>
<text>Bottom Plane=GND</text>
</plain>
<libraries>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01NS_KIT">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline Kit Version&lt;/h3&gt;
&lt;p&gt; Mask on only one side to make soldering in kits easier.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X07_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -7 Pin  No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="oshw_revA">
<description>&lt;p&gt;&lt;strong&gt;Open Source Hardware PCB Logos&lt;/strong&gt;
&lt;p&gt;A simple polygon based version of the OSHWA logos for use on Eagle PCB's
&lt;p&gt;For use please refer to the OSHWA definition at &lt;a href="http://www.oshwa.org/definition/"&gt;http://www.oshwa.org/definition/&lt;/a&gt;
&lt;p&gt;Based on the NBitWonder version (&lt;a href="http://nbitwonder.com"&gt;http://nbitwonder.com&lt;/a&gt;)
&lt;p&gt;&lt;strong&gt;Andrew Cooper&lt;/strong&gt;&lt;br&gt;28Nov2016&lt;br&gt;&lt;a href="http://www.darkerview.com"&gt;www.DarkerView.com&lt;/a&gt;</description>
<packages>
<package name="OSHW_5MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="atmel" package="DIL08" value="TINY12P">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X01NS_KIT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X01NS_KIT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X01NS_KIT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="1X01NS_KIT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J11" library="SparkFun-Connectors" package="1X01NS_KIT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J12" library="SparkFun-Connectors" package="1X07_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J13" library="SparkFun-Connectors" package="1X07_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="oshw_revA" package="OSHW_5MM" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="J6" pad="1"/>
<contactref element="J6" pad="4"/>
<contactref element="J6" pad="3"/>
<contactref element="J6" pad="2"/>
<contactref element="J10" pad="1"/>
<contactref element="J9" pad="1"/>
<contactref element="J11" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="J5" pad="1"/>
<contactref element="J5" pad="4"/>
<contactref element="J5" pad="3"/>
<contactref element="J5" pad="2"/>
<contactref element="J7" pad="1"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="7"/>
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="4"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="5"/>
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="J4" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="J3" pad="3"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="J4" pad="4"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="J3" pad="5"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="J12" pad="1"/>
<contactref element="J13" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="J13" pad="2"/>
<contactref element="J12" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="J12" pad="3"/>
<contactref element="J13" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="J13" pad="4"/>
<contactref element="J12" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="J12" pad="5"/>
<contactref element="J13" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
