(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 24)
    (no_connects 0)
    (area 194.031799 51.944199 251.027001 100.151001)
    (thickness 1.6)
    (drawings 8)
    (tracks 108)
    (zones 0)
    (modules 11)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.6)
    (trace_clearance 0.6)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.2)
    (via_min_size 0.4)
    (via_min_drill 0.2)
    (uvia_size 0.03)
    (uvia_drill 0.02)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 3)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x01000_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 CIR-RX)
  (net 2 MIC1N)
  (net 3 MIC1P)
  (net 4 MIC-BIAS)
  (net 5 TVOUT)
  (net 6 LINEOUTL)
  (net 7 LINEOUTR)
  (net 8 USB-DP3)
  (net 9 USB-DM3)
  (net 10 USB-DP2)
  (net 11 USB-DM2)
  (net 12 GND)
  (net 13 5V)
  (net 14 "Net-(J2-Pad8)")
  (net 15 "Net-(J2-Pad7)")
  (net 16 "Net-(J2-Pad6)")
  (net 17 PA12)
  (net 18 PA11)
  (net 19 "Net-(J2-Pad2)")
  (net 20 UART1_RX)
  (net 21 UART1_TX)
  (net 22 PA10)
  (net 23 UART3_RX)
  (net 24 UART3_TX)
  (net 25 UART2_RTS)
  (net 26 SPI1_MISO)
  (net 27 SPI1_MOSI)
  (net 28 PA18)
  (net 29 3.3v)
  (net 30 PA19)
  (net 31 UART2_CTS)
  (net 32 UART2_TX)
  (net 33 PA07)
  (net 34 UART2_RX)
  (net 35 PA06)
  (net 36 "Net-(J3-Pad1)")
  (net 37 "Net-(J3-Pad6)")
  (net 38 "Net-(J1-Pad1)")
  (net 39 "Net-(J1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.6)
    (trace_width 0.6)
    (via_dia 0.6)
    (via_drill 0.2)
    (uvia_dia 0.03)
    (uvia_drill 0.02)
    (add_net 3.3v)
    (add_net CIR-RX)
    (add_net LINEOUTL)
    (add_net LINEOUTR)
    (add_net MIC-BIAS)
    (add_net MIC1N)
    (add_net MIC1P)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad6)")
    (add_net PA06)
    (add_net PA07)
    (add_net PA10)
    (add_net PA11)
    (add_net PA12)
    (add_net PA18)
    (add_net PA19)
    (add_net SPI1_MISO)
    (add_net SPI1_MOSI)
    (add_net TVOUT)
    (add_net UART1_RX)
    (add_net UART1_TX)
    (add_net UART2_CTS)
    (add_net UART2_RTS)
    (add_net UART2_RX)
    (add_net UART2_TX)
    (add_net UART3_RX)
    (add_net UART3_TX)
    (add_net USB-DM2)
    (add_net USB-DM3)
    (add_net USB-DP2)
    (add_net USB-DP3)
  )
  (net_class Power ""
    (clearance 0.6)
    (trace_width 0.6)
    (via_dia 0.6)
    (via_drill 0.2)
    (uvia_dia 0.03)
    (uvia_drill 0.02)
    (add_net 5V)
    (add_net GND)
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593E088B)
    (at 197.195 55.0393)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (attr virtual)
    (fp_text reference HOLE03 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593E084C)
    (at 237.307 55.0316)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (attr virtual)
    (fp_text reference HOLE02 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593E0880)
    (at 237.292 97.155)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (attr virtual)
    (fp_text reference HOLE01 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_2pol (layer F.Cu) (tedit 0)
    (at 246.347 96.2685)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J5 (at 1.27 -4.50088) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x02 (at 1.27 4.50088) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 13 5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 12 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_2pol.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x13_Pitch2.54mm (layer B.Cu) (tedit 58CD5446)
    (at 195.834 91.3257)
    (descr "Through hole straight socket strip, 1x13, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x13 2.54mm single row")
    (fp_text reference J1 (at 0 2.33) (layer B.SilkS))
    (fp_text value CONN_01X13 (at 0 -32.81) (layer B.Fab))
    (fp_text user %R (at 0 2.33) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 USB-DM2))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 USB-DP2))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 USB-DM3))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 USB-DP3))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 LINEOUTR))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 LINEOUTL))
    (pad 9 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 TVOUT))
    (pad 10 thru_hole oval (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 MIC-BIAS))
    (pad 11 thru_hole oval (at 0 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 MIC1P))
    (pad 12 thru_hole oval (at 0 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 MIC1N))
    (pad 13 thru_hole oval (at 0 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 CIR-RX))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x13_Pitch2.54mm.wrl
      (at (xyz 0 -0.6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 200.899 70.4825)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 PA11))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 PA12))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad8)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x06_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 225.704 95.3008 270)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 4.315 -2.27 270) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 4.315 14.97 270) (layer F.Fab))
    (fp_text user %R (at 4.315 -2.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 5V))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 UART1_RX))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 UART1_TX))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 GND))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J3-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x13_Pitch2.54mm (layer B.Cu) (tedit 58CD5449)
    (at 239.007 91.3308)
    (descr "Through hole straight socket strip, 2x13, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x13 2.54mm double row")
    (fp_text reference J4 (at -1.27 2.33) (layer B.SilkS))
    (fp_text value CONN_02X13 (at -1.27 -32.81) (layer B.Fab))
    (fp_text user %R (at -1.27 2.33) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 3.3v))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 5V))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 PA12))
    (pad 4 thru_hole oval (at -2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 5V))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 PA11))
    (pad 6 thru_hole oval (at -2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 GND))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 PA06))
    (pad 8 thru_hole oval (at -2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 UART1_TX))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 GND))
    (pad 10 thru_hole oval (at -2.54 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 UART1_RX))
    (pad 11 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 UART2_RX))
    (pad 12 thru_hole oval (at -2.54 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 PA07))
    (pad 13 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 UART2_TX))
    (pad 14 thru_hole oval (at -2.54 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 GND))
    (pad 15 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 UART2_CTS))
    (pad 16 thru_hole oval (at -2.54 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 PA19))
    (pad 17 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 3.3v))
    (pad 18 thru_hole oval (at -2.54 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 PA18))
    (pad 19 thru_hole oval (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 SPI1_MOSI))
    (pad 20 thru_hole oval (at -2.54 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 GND))
    (pad 21 thru_hole oval (at 0 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 SPI1_MISO))
    (pad 22 thru_hole oval (at -2.54 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 UART2_RTS))
    (pad 23 thru_hole oval (at 0 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 UART3_TX))
    (pad 24 thru_hole oval (at -2.54 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 UART3_RX))
    (pad 25 thru_hole oval (at 0 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 GND))
    (pad 26 thru_hole oval (at -2.54 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 PA10))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x13_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 245.923 61.468)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (fp_text reference J6 (at 4.315 -2.27) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 4.315 9.89) (layer F.Fab))
    (fp_text user %R (at 4.315 -2.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 UART3_RX))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 UART3_TX))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 245.923 77.6732)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (fp_text reference J7 (at 4.315 -2.27) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 4.315 9.89) (layer F.Fab))
    (fp_text user %R (at 4.315 -2.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 UART2_RX))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 UART2_TX))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593E0876)
    (at 197.206 97.1093)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (attr virtual)
    (fp_text reference HOLE00 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (gr_line (start 233.5784 52.0192) (end 250.952 52.07) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 250.952 100.076) (end 194.1068 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 250.952 52.07) (end 250.952 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 233.5784 65.9384) (end 233.5784 52.0192) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.2536 65.9384) (end 233.5784 65.9384) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.2536 52.0192) (end 200.2536 65.9384) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 194.1068 52.0192) (end 200.2536 52.0192) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 194.1068 100.076) (end 194.1068 52.0192) (angle 90) (layer Edge.Cuts) (width 0.15))
)
