(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 36)
    (no_connects 0)
    (area 129.221191 48.988809 177.205715 115.207143)
    (thickness 1.6)
    (drawings 31)
    (tracks 96)
    (zones 0)
    (modules 18)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.794 2.794)
    (pad_drill 2.7)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF3F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 Rx)
  (net 5 D0)
  (net 6 RESET)
  (net 7 D2)
  (net 8 Tx)
  (net 9 "Net-(P2-Pad2)")
  (net 10 "Net-(P2-Pad6)")
  (net 11 "Net-(P3-Pad1)")
  (net 12 "Net-(P4-Pad1)")
  (net 13 "Net-(P6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net D0)
    (add_net D2)
    (add_net GND)
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net RESET)
    (add_net Rx)
    (add_net Tx)
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 57DEF597)
    (at 161.29 56.515)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 0.635 -6.35) (layer F.SilkS))
    (fp_text value 47uF (at 4.445 -5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 57DEF591)
    (at 140.97 56.515)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at 0.635 -5.715) (layer F.SilkS))
    (fp_text value 47uF (at -1.905 -6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:BARREL_JACK (layer F.Cu) (tedit 57DEF5F0)
    (at 152.4 107.315 90)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference CON1 (at 13.335 -20.955 180) (layer F.SilkS))
    (fp_text value Power (at 3.175 -17.145 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 6.20014 0 90) (size 3.50012 3.50012) (drill oval 1.00076 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole rect (at 0.20066 0 90) (size 3.50012 3.50012) (drill oval 1.00076 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at 3.2004 4.699 90) (size 3.50012 3.50012) (drill oval 2.99974 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 57DEF8AC)
    (at 156.21 55.245 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -5.08 -3.81 270) (layer F.SilkS))
    (fp_text value ESP8266 (at -3.175 3.937 540) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 Rx))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 D0))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 RESET))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 D2))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 Tx))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 57DEF5B4)
    (at 140.335 88.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -8.255 -5.715) (layer F.SilkS))
    (fp_text value FTDI (at -8.255 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 Rx))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 Tx))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P2-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57DEF5D0)
    (at 166.37 82.55)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 5.08 -5.715) (layer F.SilkS))
    (fp_text value Hours (at 5.715 -1.905) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57DEF5D2)
    (at 166.37 93.98)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 5.715 -5.715) (layer F.SilkS))
    (fp_text value Minutes (at 5.715 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57DEF8B1)
    (at 152.4 69.215 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 20.32 -2.54 180) (layer F.SilkS))
    (fp_text value "WS2812 Ring" (at 17.399 3.937 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 D0))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57DEF5E0)
    (at 166.37 105.41)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 4.445 -5.08) (layer F.SilkS))
    (fp_text value Seconds (at 6.985 -1.905) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp (layer F.Cu) (tedit 57DEF5D7)
    (at 161.925 85.09)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV1 (at 12.065 -10.795) (layer F.SilkS))
    (fp_text value 10k (at 10.16 5.08) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P3-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 Rx))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp (layer F.Cu) (tedit 57DEF5DD)
    (at 161.925 96.52)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV2 (at 10.16 -11.43) (layer F.SilkS))
    (fp_text value 10k (at 9.525 5.715) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P4-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 D2))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp (layer F.Cu) (tedit 57DEF5E8)
    (at 161.925 107.95)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV3 (at 10.16 -10.16) (layer F.SilkS))
    (fp_text value 10k (at 10.16 4.445) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P6-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 Tx))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:Button-SPST-Throughhole (layer F.Cu) (tedit 57DEF5B1)
    (at 140.335 84.455 90)
    (fp_text reference SW1 (at 3.81 -6.985 90) (layer F.SilkS))
    (fp_text value Reset (at 4.445 -8.89 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.032 2.032) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 6.35 0 90) (size 2.032 2.032) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 6 RESET))
  )
  (module Libraries:Button-SPST-Throughhole (layer F.Cu) (tedit 57DEF5F4)
    (at 140.335 112.395 90)
    (fp_text reference SW2 (at 4.445 -5.715 90) (layer F.SilkS))
    (fp_text value Program (at 3.81 -5.08 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.032 2.032) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 6.35 0 90) (size 2.032 2.032) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 5 D0))
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 57DEF5ED)
    (at 152.4 93.345)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at -20.32 3.175) (layer F.SilkS))
    (fp_text value AP1117D33 (at 20.32 0.635) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_ISO14580_Pad (layer F.Cu) (tedit 57DEF8C2)
    (at 152.4 101.092)
    (descr "Mounting Hole 2.7mm, M2.5, ISO14580")
    (tags "mounting hole 2.7mm m2.5 iso14580")
    (fp_text reference REF** (at 18.542 -2.159) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm_M2.5_ISO14580_Pad (at -18.034 -11.303 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.794 2.794) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_ISO14580_Pad (layer F.Cu) (tedit 57DEF8BD)
    (at 152.4 107.188)
    (descr "Mounting Hole 2.7mm, M2.5, ISO14580")
    (tags "mounting hole 2.7mm m2.5 iso14580")
    (fp_text reference REF** (at 19.304 0) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm_M2.5_ISO14580_Pad (at -18.034 -12.954 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.794 2.794) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_ISO14580_Pad (layer F.Cu) (tedit 57DEF8BB)
    (at 157.099 104.14)
    (descr "Mounting Hole 2.7mm, M2.5, ISO14580")
    (tags "mounting hole 2.7mm m2.5 iso14580")
    (fp_text reference REF** (at 14.732 1.524) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm_M2.5_ISO14580_Pad (at -22.987 -9.271 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.794 2.794) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (gr_text S (at 166.37 102.235) (layer F.SilkS))
  (gr_text M (at 166.37 90.805) (layer F.SilkS))
  (gr_text H (at 166.37 79.375) (layer F.SilkS))
  (gr_text 5vDC (at 146.685 109.22 270) (layer F.SilkS))
  (gr_text Reset (at 143.51 81.28 270) (layer F.SilkS))
  (gr_text Program (at 143.51 109.22 270) (layer F.SilkS))
  (gr_text Rx (at 142.24 99.06) (layer F.SilkS))
  (gr_text Tx (at 142.24 96.52) (layer F.SilkS))
  (gr_text 3.3v (at 142.24 93.98) (layer F.SilkS))
  (gr_text GND (at 142.24 88.9) (layer F.SilkS))
  (gr_text FTDI (at 145.415 95.25 270) (layer F.SilkS))
  (gr_text Seconds (at 158.115 110.49 90) (layer F.SilkS))
  (gr_text Minutes (at 158.115 93.345 90) (layer F.SilkS))
  (gr_text Hours (at 158.115 82.55 90) (layer F.SilkS))
  (gr_text 10k (at 161.925 99.695) (layer F.SilkS))
  (gr_text 10k (at 161.925 88.265) (layer F.SilkS))
  (gr_text 10k (at 161.925 76.835) (layer F.SilkS))
  (gr_text 47uF (at 162.56 60.325) (layer F.SilkS))
  (gr_text 47uF (at 142.24 60.325) (layer F.SilkS))
  (gr_text "WS2812\nRing" (at 154.305 66.675) (layer F.SilkS))
  (gr_text ESP8266 (at 152.4 60.325) (layer F.SilkS))
  (gr_line (start 136.525 114.935) (end 152.4 114.935) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.525 53.34) (end 136.525 114.935) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.275 53.34) (end 136.525 53.34) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.275 114.935) (end 168.275 53.34) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 114.935) (end 168.275 114.935) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.305 74.93) (end 154.305 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 152.4 82.55) (end 147.955 82.55) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.495 74.93) (end 150.495 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.4 74.93) (end 150.495 74.93) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.4 74.93) (end 152.4 73.025) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.525 53.34) (xy 168.275 53.34) (xy 168.275 114.935) (xy 136.525 114.935)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.275 114.935) (xy 136.525 114.935) (xy 136.525 104.14) (xy 147.32 104.14) (xy 147.32 99.06)
        (xy 153.67 99.06) (xy 153.67 93.98) (xy 155.575 93.98) (xy 155.575 83.185) (xy 150.495 83.185)
        (xy 150.495 62.23) (xy 159.385 62.23) (xy 159.385 53.34) (xy 168.275 53.34)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.525 53.34) (xy 158.75 53.34) (xy 158.75 61.595) (xy 149.86 61.595) (xy 149.86 83.82)
        (xy 154.94 83.82) (xy 154.94 93.345) (xy 153.035 93.345) (xy 153.035 98.425) (xy 146.685 98.425)
        (xy 146.685 103.505) (xy 136.525 103.505)
      )
    )
  )
)
