(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 8)
    (no_connects 0)
    (area 128.393475 79.248 170.818525 114.300001)
    (thickness 1.6)
    (drawings 4)
    (tracks 8)
    (zones 0)
    (modules 9)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (user_trace_width 2.032)
    (user_trace_width 2.54)
    (user_trace_width 5.08)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.54 2.54)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C7-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C12-Pad1)")
  (net 4 "Net-(C15-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C7-Pad1)")
  )
  (module Capacitors_THT:C_Radial_D10_L25_P5 (layer F.Cu) (tedit 5A1A033F)
    (at 155.067 94.488 30)
    (descr "Radial Electrolytic Capacitor Diameter 10mm x Length 25mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C7 (at 3.099044 -6.129702 30) (layer F.SilkS))
    (fp_text value "16uF 400v" (at 3.07169 0.013677 120) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 30) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 30) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L25_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_THT:C_Radial_D10_L25_P5 (layer F.Cu) (tedit 5A1A034F)
    (at 146.304 93.091 150)
    (descr "Radial Electrolytic Capacitor Diameter 10mm x Length 25mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C12 (at 3.784761 -6.144601 150) (layer F.SilkS))
    (fp_text value "16uf 400v" (at 3.19869 0.206293 240) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 150) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C12-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 150) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L25_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_THT:C_Radial_D10_L25_P5 (layer F.Cu) (tedit 5A1A0316)
    (at 149.479 100.965 270)
    (descr "Radial Electrolytic Capacitor Diameter 10mm x Length 25mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C15 (at 3.937 -5.969 270) (layer F.SilkS))
    (fp_text value "16uf 400v" (at 3.175 0 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C15-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.54 2.54) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L25_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wire_Pads:SolderWirePad_single_1-5mmDrill (layer F.Cu) (tedit 5A1A03C9)
    (at 154.178 98.552)
    (fp_text reference J7 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 1 "Net-(C7-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1-5mmDrill (layer F.Cu) (tedit 5A19B2E0)
    (at 150.368 91.948)
    (fp_text reference J12 (at 0 -3.81) (layer F.SilkS))
    (fp_text value Conn_01x01 (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 3 "Net-(C12-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1-5mmDrill (layer F.Cu) (tedit 5A1A03BF)
    (at 146.304 98.298)
    (fp_text reference J15 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 4 "Net-(C15-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1-5mmDrill (layer F.Cu) (tedit 5A1A030E)
    (at 150.622 86.614)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_1-5mmDrill (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Wire_Pads:SolderWirePad_single_1-5mmDrill (layer F.Cu) (tedit 5A1A0300)
    (at 158.369 101.473)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_1-5mmDrill (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Wire_Pads:SolderWirePad_single_1-5mmDrill (layer F.Cu) (tedit 5A1A02EC)
    (at 142.113 101.092)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_1-5mmDrill (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (gr_text SDS (at 150.368 96.52) (layer F.SilkS))
  (gr_circle (center 150.368 96.012) (end 163.068 96.266) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.163 81.534) (xy 168.402 90.932) (xy 168.148 101.219) (xy 163.703 110.617) (xy 152.273 113.792)
        (xy 134.366 114.3) (xy 131.572 107.061) (xy 132.461 85.217) (xy 133.477 83.439) (xy 147.955 79.248)
      )
    )
  )
)
