(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 89)
    (no_connects 1)
    (area 35.509999 27.889999 73.710001 47.040001)
    (thickness 1.6)
    (drawings 38)
    (tracks 139)
    (zones 0)
    (modules 45)
    (nets 51)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.762 0.381)
    (user_via 1.016 0.635)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.65 2)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00008_00000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory meta/))
  )
  (net 0 "")
  (net 1 "Net-(R1-Pad1)")
  (net 2 "Net-(R3-Pad1)")
  (net 3 "Net-(U1-Pad3)")
  (net 4 "Net-(U1-Pad6)")
  (net 5 "Net-(U1-Pad7)")
  (net 6 "Net-(U2-Pad7)")
  (net 7 +3V3)
  (net 8 "Net-(R5-Pad2)")
  (net 9 "Net-(U2-Pad11)")
  (net 10 "Net-(R2-Pad1)")
  (net 11 "Net-(R6-Pad2)")
  (net 12 "Net-(R7-Pad2)")
  (net 13 "Net-(U3-Pad2)")
  (net 14 "Net-(U3-Pad3)")
  (net 15 "Net-(U3-Pad9)")
  (net 16 "Net-(U3-Pad10)")
  (net 17 "Net-(U3-Pad11)")
  (net 18 "Net-(U3-Pad12)")
  (net 19 "Net-(U3-Pad13)")
  (net 20 "Net-(U3-Pad14)")
  (net 21 "Net-(U3-Pad15)")
  (net 22 "Net-(U3-Pad16)")
  (net 23 "Net-(U3-Pad19)")
  (net 24 "Net-(U3-Pad20)")
  (net 25 "Net-(U3-Pad21)")
  (net 26 "Net-(U3-Pad22)")
  (net 27 "Net-(U3-Pad27)")
  (net 28 "Net-(U3-Pad28)")
  (net 29 "Net-(U3-Pad29)")
  (net 30 "Net-(U2-Pad4)")
  (net 31 /+12V)
  (net 32 /VOUT2+)
  (net 33 /VOUT1+)
  (net 34 /ACC1)
  (net 35 /ACC2)
  (net 36 "Net-(C10-Pad1)")
  (net 37 "Net-(D2-Pad2)")
  (net 38 "Net-(U3-Pad5)")
  (net 39 "Net-(U3-Pad6)")
  (net 40 GNDD)
  (net 41 GND)
  (net 42 V1EN)
  (net 43 V2EN)
  (net 44 /PDI_DATA)
  (net 45 /PDI_CLK)
  (net 46 "Net-(J9-Pad3)")
  (net 47 "Net-(J9-Pad4)")
  (net 48 "Net-(U3-Pad30)")
  (net 49 "Net-(U3-Pad31)")
  (net 50 ACC1_IN)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net /+12V)
    (add_net /ACC1)
    (add_net /ACC2)
    (add_net /PDI_CLK)
    (add_net /PDI_DATA)
    (add_net /VOUT1+)
    (add_net /VOUT2+)
    (add_net ACC1_IN)
    (add_net GND)
    (add_net GNDD)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J9-Pad3)")
    (add_net "Net-(J9-Pad4)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad19)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad20)")
    (add_net "Net-(U3-Pad21)")
    (add_net "Net-(U3-Pad22)")
    (add_net "Net-(U3-Pad27)")
    (add_net "Net-(U3-Pad28)")
    (add_net "Net-(U3-Pad29)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad30)")
    (add_net "Net-(U3-Pad31)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad9)")
    (add_net V1EN)
    (add_net V2EN)
  )
  (net_class +3V3 ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net +3V3)
  )
  (module Housings_SOIC_ML:Infineon_PG-TSDSO-14-22 (layer F.Cu) (tedit 598BB7ED)
    (at 61.595 33.64)
    (descr Infineon_PG-TSDSO-14-22)
    (tags "DSO DSO-14 TSDSO TSDSO-14 SOIC SOIC-14")
    (attr smd)
    (fp_text reference U2 (at -2.54 -3.287) (layer F.SilkS))
    (fp_text value BTS7008-2EPA (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.85 -1.95) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R7-Pad2)"))
    (pad 2 smd rect (at -2.85 -1.3) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R2-Pad1)"))
    (pad 3 smd rect (at -2.85 -0.65) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R5-Pad2)"))
    (pad 4 smd rect (at -2.85 0) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -2.85 0.65) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (pad 6 smd rect (at -2.85 1.3) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(R3-Pad1)"))
    (pad 7 smd rect (at -2.85 1.95) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at 2.85 1.95) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 /VOUT2+))
    (pad 15 smd rect (at 0 1) (size 2.65 2) (layers F.Cu F.Paste F.Mask)
      (net 31 /+12V) (solder_paste_margin_ratio -0.2))
    (pad 15 smd rect (at 0 -1) (size 2.65 2) (layers F.Cu F.Paste F.Mask)
      (net 31 /+12V) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 2.85 1.3) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 /VOUT2+))
    (pad 10 smd rect (at 2.85 0.65) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 /VOUT2+))
    (pad 11 smd rect (at 2.85 0) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at 2.85 -0.65) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 /VOUT1+))
    (pad 13 smd rect (at 2.85 -1.3) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 /VOUT1+))
    (pad 14 smd rect (at 2.85 -1.95) (size 1.31 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 /VOUT1+))
  )
  (module Wire_Connections_Bridges:WireConnection_0.80mmDrill_ThinPad (layer F.Cu) (tedit 598BAE39)
    (at 47.244 45.974)
    (descr "WireConnection with thin pad and 0.8mm drill")
    (fp_text reference JP1 (at 1.27 -1.905) (layer F.SilkS) hide)
    (fp_text value GND (at 1.27 -1.27) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8001) (layers *.Cu *.Mask)
      (net 41 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8001) (layers *.Cu *.Mask)
      (net 40 GNDD))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 598BAD4A)
    (at 52.705 43.815 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -2.032 0 360) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 598BA867)
    (at 48.895 36.195)
    (fp_text reference TP1 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.0541 1.0541) (drill 0.8001) (layers *.Cu *.Mask)
      (net 50 ACC1_IN))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 598BAD40)
    (at 51.816 31.115)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.127 5.842) (layer F.SilkS))
    (fp_text value 2.15M (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 598BAD7D)
    (at 55.88 31.877 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.032 0 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 V1EN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 598BAD72)
    (at 55.88 36.068 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.032 0 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 V2EN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 598BAD3D)
    (at 51.816 29.718 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.127 -5.715 180) (layer F.SilkS))
    (fp_text value 1.27M (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 598BACE1)
    (at 44.704 32.385 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.413 0 360) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 31 /+12V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 598BAD75)
    (at 51.816 33.655)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -0.127 6.35) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 598BAD43)
    (at 51.816 32.385)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -0.127 6.096) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 598BAD63)
    (at 60.96 37.37 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -2 0 180) (layer F.SilkS))
    (fp_text value 68nF (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 41 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 /+12V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill locked (layer F.Cu) (tedit 5989E9B0)
    (at 40.64 30.48)
    (fp_text reference J1 (at -6.35 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 31 /+12V))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill locked (layer F.Cu) (tedit 5989E9AE)
    (at 38.1 34.925)
    (fp_text reference J2 (at -3.81 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 34 /ACC1))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 598BAD7A)
    (at 55.88 33.274)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.032 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-8-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 5988D914)
    (at 48.26 31.369 180)
    (descr "DD Package; 8-Lead Plastic DFN (3mm x 3mm) (see Linear Technology DFN_8_05-08-1698.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 2.413 180) (layer F.SilkS))
    (fp_text value LT3014IDD (at 0 2.55 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 -0.75 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at -1.4 -0.25 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(R1-Pad1)"))
    (pad 3 smd rect (at -1.4 0.25 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -1.4 0.75 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 5 smd rect (at 1.4 0.75 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 /+12V))
    (pad 6 smd rect (at 1.4 0.25 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at 1.4 -0.25 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 1.4 -0.75 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 /+12V))
    (pad 9 smd rect (at 0.415 0.595 180) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.415 -0.595 180) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.415 0.595 180) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.415 -0.595 180) (size 0.83 1.19) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill locked (layer F.Cu) (tedit 5989EAE3)
    (at 68.58 30.48)
    (fp_text reference J3 (at 6.35 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 33 /VOUT1+))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill locked (layer F.Cu) (tedit 5989EADD)
    (at 71.12 40.005)
    (fp_text reference J4 (at 3.81 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 41 GND))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill locked (layer F.Cu) (tedit 5989EAE0)
    (at 71.12 34.925)
    (fp_text reference J5 (at 3.81 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 32 /VOUT2+))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill locked (layer F.Cu) (tedit 5989EADB)
    (at 68.58 44.45)
    (fp_text reference J6 (at 6.35 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 41 GND))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 598BAD55)
    (at 63.5 38.1 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -2.667 0 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 32 /VOUT2+))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill locked (layer F.Cu) (tedit 5989EAD7)
    (at 38.1 40.005)
    (fp_text reference J7 (at -3.81 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 35 /ACC2))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill locked (layer F.Cu) (tedit 5989EAD3)
    (at 40.64 44.45)
    (fp_text reference J8 (at -6.35 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 41 GND))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 598BAD77)
    (at 55.88 34.671)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2.032 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 598BAD81)
    (at 55.88 30.48)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -2.032 0) (layer F.SilkS))
    (fp_text value 47 (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 598BAD60)
    (at 63.5 36.83)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 2.667 0) (layer F.SilkS))
    (fp_text value 47k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /VOUT2+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 598BAD6F)
    (at 63.5 30.48)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 2.032 0) (layer F.SilkS))
    (fp_text value 47k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 /VOUT1+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-32-1EP_4x4mm_Pitch0.4mm (layer F.Cu) (tedit 5989EACA)
    (at 55.8525 40.6125 90)
    (descr "L32.4x4A; 32 LEAD QUAD FLAT NO-LEAD PLASTIC PACKAGE; (see Intersil l32.4x4a.pdf)")
    (tags "QFN 0.4")
    (attr smd)
    (fp_text reference U3 (at -3.2025 1.1705 360) (layer F.SilkS))
    (fp_text value ATXMEGA8E5-M4U (at 0 3.2 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.9 -1.4 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 2 smd rect (at -1.9 -1 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U3-Pad2)"))
    (pad 3 smd rect (at -1.9 -0.6 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U3-Pad3)"))
    (pad 4 smd rect (at -1.9 -0.2 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C10-Pad1)"))
    (pad 5 smd rect (at -1.9 0.2 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at -1.9 0.6 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at -1.9 1 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 44 /PDI_DATA))
    (pad 8 smd rect (at -1.9 1.4 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 45 /PDI_CLK))
    (pad 9 smd rect (at -1.4 1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U3-Pad9)"))
    (pad 10 smd rect (at -1 1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U3-Pad10)"))
    (pad 11 smd rect (at -0.6 1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U3-Pad11)"))
    (pad 12 smd rect (at -0.2 1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U3-Pad12)"))
    (pad 13 smd rect (at 0.2 1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U3-Pad13)"))
    (pad 14 smd rect (at 0.6 1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U3-Pad14)"))
    (pad 15 smd rect (at 1 1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U3-Pad15)"))
    (pad 16 smd rect (at 1.4 1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U3-Pad16)"))
    (pad 17 smd rect (at 1.9 1.4 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 18 smd rect (at 1.9 1 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 19 smd rect (at 1.9 0.6 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U3-Pad19)"))
    (pad 20 smd rect (at 1.9 0.2 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U3-Pad20)"))
    (pad 21 smd rect (at 1.9 -0.2 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U3-Pad21)"))
    (pad 22 smd rect (at 1.9 -0.6 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U3-Pad22)"))
    (pad 23 smd rect (at 1.9 -1 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 43 V2EN))
    (pad 24 smd rect (at 1.9 -1.4 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 42 V1EN))
    (pad 25 smd rect (at 1.4 -1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 50 ACC1_IN))
    (pad 26 smd rect (at 1 -1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 50 ACC1_IN))
    (pad 27 smd rect (at 0.6 -1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U3-Pad27)"))
    (pad 28 smd rect (at 0.2 -1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U3-Pad28)"))
    (pad 29 smd rect (at -0.2 -1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U3-Pad29)"))
    (pad 30 smd rect (at -0.6 -1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U3-Pad30)"))
    (pad 31 smd rect (at -1 -1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U3-Pad31)"))
    (pad 32 smd rect (at -1.4 -1.9 180) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 33 smd rect (at 0.6625 0.6625 90) (size 1.325 1.325) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.6625 -0.6625 90) (size 1.325 1.325) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.6625 0.6625 90) (size 1.325 1.325) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.6625 -0.6625 90) (size 1.325 1.325) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-32-1EP_4x4mm_Pitch0.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 598BAD6A)
    (at 63.373 29.21 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -2.159 0 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 /VOUT1+))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMC_Handsoldering (layer B.Cu) (tedit 58642B03)
    (at 53.975 37.465 270)
    (descr "Diode SMC (DO-214AB) Handsoldering")
    (tags "Diode SMC (DO-214AB) Handsoldering")
    (attr smd)
    (fp_text reference D1 (at 0 0 360) (layer B.SilkS))
    (fp_text value SM15T33CA (at 0 -4.2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -4.4 0 180) (size 3.3 4.5) (layers B.Cu B.Paste B.Mask)
      (net 31 /+12V))
    (pad 2 smd rect (at 4.4 0 180) (size 3.3 4.5) (layers B.Cu B.Paste B.Mask)
      (net 41 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 598BAD5C)
    (at 58.42 37.465)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -2.159 0) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 598BACE5)
    (at 42.545 34.925 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 2.032 0.254 360) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 50 ACC1_IN))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 598BAD2C)
    (at 42.545 40.005 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 1.8415 0.127 540) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 598BACF2)
    (at 45.085 36.195)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D2 (at 1.905 1.27) (layer F.SilkS))
    (fp_text value BAT54S (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 50 ACC1_IN))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 598BAD18)
    (at 45.085 40.005)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D3 (at 1.905 -1.27) (layer F.SilkS))
    (fp_text value BAT54S (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 598BACEA)
    (at 41.275 34.925 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 5.08 -4.699 90) (layer F.SilkS))
    (fp_text value 47k (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 ACC1_IN))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 /ACC1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 598BAD08)
    (at 41.275 40.005 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 5.207 4.699 270) (layer F.SilkS))
    (fp_text value 47k (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 /ACC2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 598BAD34)
    (at 45.085 43.815)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D4 (at -0.635 2.413) (layer F.SilkS))
    (fp_text value ZRC330 (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 598B8988)
    (at 48.895 40.005)
    (fp_text reference TP2 (at 0 2.032 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.0541 1.0541) (drill 0.8001) (layers *.Cu *.Mask)
      (net 36 "Net-(C10-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 598B8991)
    (at 47.625 40.64)
    (fp_text reference TP3 (at 0 2.032 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.0541 1.0541) (drill 0.8001) (layers *.Cu *.Mask)
      (net 37 "Net-(D2-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 598BAD47)
    (at 50.8 43.053 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -0.381 1.143 360) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 598BAD58)
    (at 58.928 40.894 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 1.143 -1.397 450) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch1.27mm_SMD (layer F.Cu) (tedit 598BAD4E)
    (at 63.627 42.926 90)
    (descr "surface-mounted straight pin header, 2x03, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 1.27mm double row")
    (attr smd)
    (fp_text reference J9 (at 1.524 3.048 180) (layer F.SilkS))
    (fp_text value Header (at 0 2.965 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 44 /PDI_DATA))
    (pad 2 smd rect (at 1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 3 smd rect (at -1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J9-Pad3)"))
    (pad 4 smd rect (at 1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J9-Pad4)"))
    (pad 5 smd rect (at -1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 45 /PDI_CLK))
    (pad 6 smd rect (at 1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch1.27mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 598DABCE)
    (at 41.795 36.83)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -4.711 -4.826) (layer F.SilkS))
    (fp_text value 47k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 ACC1_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 598DABD6)
    (at 41.795 38.1)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at -4.711 5.08) (layer F.SilkS))
    (fp_text value 47k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 GNDD))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text V2- (at 74.93 44.45) (layer F.Fab))
  (gr_text V1- (at 74.93 40.132) (layer F.Fab))
  (gr_text V2+ (at 74.93 35.052) (layer F.Fab))
  (gr_text V1+ (at 74.93 30.48) (layer F.Fab))
  (gr_text GND (at 34.29 44.45) (layer F.Fab))
  (gr_text ACC2 (at 34.29 39.878) (layer F.Fab))
  (gr_text "ACC1\n" (at 34.544 34.798) (layer F.Fab))
  (gr_text +12V (at 34.29 30.48) (layer F.Fab))
  (gr_text PDI (at 60.071 45.339) (layer F.SilkS))
  (gr_text "Mike Lawrence" (at 44.831 37.465 90) (layer B.SilkS))
  (gr_text "Aug 2017" (at 58.674 37.338 90) (layer B.SilkS))
  (gr_text "Rev 2.2" (at 64.77 37.084 90) (layer B.SilkS))
  (gr_text "LED Relay" (at 53.975 29.337) (layer B.SilkS))
  (gr_text V1- (at 67.945 40.005 90) (layer B.SilkS))
  (gr_text V2- (at 71.755 44.45 90) (layer B.SilkS))
  (gr_text V2+ (at 67.945 34.925 90) (layer B.SilkS))
  (gr_text V1+ (at 71.755 30.48 90) (layer B.SilkS))
  (gr_text GND (at 37.465 44.45 90) (layer B.SilkS))
  (gr_text ACC2 (at 41.275 40.005 90) (layer B.SilkS))
  (gr_text ACC1 (at 41.275 34.925 90) (layer B.SilkS))
  (gr_text +12V (at 37.465 30.48 90) (layer B.SilkS))
  (dimension 19.05 (width 0.3) (layer F.Fab)
    (gr_text "0.7500 in" (at 24.05 37.465 90) (layer F.Fab))
    (feature1 (pts (xy 34.29 27.94) (xy 22.7 27.94)))
    (feature2 (pts (xy 34.29 46.99) (xy 22.7 46.99)))
    (crossbar (pts (xy 25.4 46.99) (xy 25.4 27.94)))
    (arrow1a (pts (xy 25.4 27.94) (xy 25.986421 29.066504)))
    (arrow1b (pts (xy 25.4 27.94) (xy 24.813579 29.066504)))
    (arrow2a (pts (xy 25.4 46.99) (xy 25.986421 45.863496)))
    (arrow2b (pts (xy 25.4 46.99) (xy 24.813579 45.863496)))
  )
  (gr_line (start 35.56 29.21) (end 35.56 45.72) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.39 46.99) (end 36.83 46.99) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.66 29.21) (end 73.66 45.72) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.83 27.94) (end 72.39 27.94) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 38.1 (width 0.3) (layer F.Fab)
    (gr_text "1.50 in" (at 54.61 21.51) (layer F.Fab))
    (feature1 (pts (xy 73.66 26.67) (xy 73.66 20.16)))
    (feature2 (pts (xy 35.56 26.67) (xy 35.56 20.16)))
    (crossbar (pts (xy 35.56 22.86) (xy 73.66 22.86)))
    (arrow1a (pts (xy 73.66 22.86) (xy 72.533496 23.446421)))
    (arrow1b (pts (xy 73.66 22.86) (xy 72.533496 22.273579)))
    (arrow2a (pts (xy 35.56 22.86) (xy 36.686504 23.446421)))
    (arrow2b (pts (xy 35.56 22.86) (xy 36.686504 22.273579)))
  )
  (gr_arc (start 36.83 29.21) (end 35.56 29.21) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 36.83 45.72) (end 36.83 46.99) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 72.39 45.72) (end 73.66 45.72) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 72.39 29.21) (end 72.39 27.94) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 40) (net_name GNDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 63.5 38.862) (xy 66.04 38.862) (xy 66.04 46.99) (xy 43.18 46.99) (xy 35.56 46.99)
        (xy 35.56 41.91) (xy 35.56 27.94) (xy 63.5 27.94)
      )
    )
  )
  (zone (net 33) (net_name /VOUT1+) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 63.754 27.94) (xy 63.754 33.274) (xy 73.66 33.274) (xy 73.66 27.94)
      )
    )
  )
  (zone (net 32) (net_name /VOUT2+) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 63.754 33.528) (xy 73.66 33.528) (xy 73.66 38.608) (xy 63.754 38.608)
      )
    )
  )
  (zone (net 31) (net_name /+12V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 35.56 27.94) (xy 73.66 27.94) (xy 73.66 39.37) (xy 35.56 39.37)
      )
    )
  )
  (zone (net 41) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 35.56 39.624) (xy 73.66 39.624) (xy 73.66 46.99) (xy 35.56 46.99)
      )
    )
  )
)
