(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-4")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 7)
    (zones 0)
    (modules 6)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.3048)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 1.016)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 1.016)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 "Net-(JP2-Pad2)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 GND)
  (net 4 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
  )
  (module TestPoint:TestPoint_Pad_1.5x1.5mm (layer F.Cu) (tedit 5C05E185)
    (at 226.06 82.55)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference GND (at 1.905 1.905 90) (layer F.SilkS))
    (fp_text value Conn_01x01_Female (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 3 GND))
  )
  (module TestPoint:TestPoint_Pad_1.5x1.5mm (layer F.Cu) (tedit 5C05E1C2)
    (at 226.06 96.52)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference CHG (at 1.905 -0.635 90) (layer F.SilkS))
    (fp_text value Conn_01x01_Female (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 4 +5V))
  )
  (module Diode_SMD:D_SOD-523 (layer F.Cu) (tedit 586419F0)
    (at 226.06 93.345 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D1 (at 1.27 1.905 90) (layer F.SilkS))
    (fp_text value 1N914WT (at 0 1.4 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.3 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C05E193)
    (at 226.06 85.725 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Open (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 "Net-(JP2-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 3 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5C05E19A)
    (at 223.52 86.36)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP_GND1 (at 0 -4.445 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 1 "Net-(JP2-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5C05E1A8)
    (at 223.52 93.98)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP_CHG1 (at 1.905 -3.175) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 2 "Net-(D1-Pad2)"))
  )
  (gr_text "Chg Adapt 1" (at 226.06 90.17 90) (layer B.SilkS))
  (dimension 6.35 (width 0.3) (layer Dwgs.User)
    (gr_text "0.2500 in" (at 225.425 102.579903) (layer Dwgs.User))
    (feature1 (pts (xy 228.6 99.06) (xy 228.6 101.066324)))
    (feature2 (pts (xy 222.25 99.06) (xy 222.25 101.066324)))
    (crossbar (pts (xy 222.25 100.479903) (xy 228.6 100.479903)))
    (arrow1a (pts (xy 228.6 100.479903) (xy 227.473496 101.066324)))
    (arrow1b (pts (xy 228.6 100.479903) (xy 227.473496 99.893482)))
    (arrow2a (pts (xy 222.25 100.479903) (xy 223.376504 101.066324)))
    (arrow2b (pts (xy 222.25 100.479903) (xy 223.376504 99.893482)))
  )
  (dimension 7.62 (width 0.3) (layer Dwgs.User)
    (gr_text "0.3000 in" (at 211.118357 89.594381 90) (layer Dwgs.User))
    (feature1 (pts (xy 219.568357 85.784381) (xy 212.631936 85.784381)))
    (feature2 (pts (xy 219.568357 93.404381) (xy 212.631936 93.404381)))
    (crossbar (pts (xy 213.218357 93.404381) (xy 213.218357 85.784381)))
    (arrow1a (pts (xy 213.218357 85.784381) (xy 213.804778 86.910885)))
    (arrow1b (pts (xy 213.218357 85.784381) (xy 212.631936 86.910885)))
    (arrow2a (pts (xy 213.218357 93.404381) (xy 213.804778 92.277877)))
    (arrow2b (pts (xy 213.218357 93.404381) (xy 212.631936 92.277877)))
  )
  (dimension 16.51 (width 0.3) (layer Dwgs.User)
    (gr_text "0.6500 in" (at 270.07 89.535 90) (layer Dwgs.User))
    (feature1 (pts (xy 228.6 81.28) (xy 268.556421 81.28)))
    (feature2 (pts (xy 228.6 97.79) (xy 268.556421 97.79)))
    (crossbar (pts (xy 267.97 97.79) (xy 267.97 81.28)))
    (arrow1a (pts (xy 267.97 81.28) (xy 268.556421 82.406504)))
    (arrow1b (pts (xy 267.97 81.28) (xy 267.383579 82.406504)))
    (arrow2a (pts (xy 267.97 97.79) (xy 268.556421 96.663496)))
    (arrow2b (pts (xy 267.97 97.79) (xy 267.383579 96.663496)))
  )
  (gr_line (start 222.25 81.28) (end 228.6 81.28) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 222.25 97.79) (end 222.25 81.28) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 228.6 97.79) (end 222.25 97.79) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 228.6 81.28) (end 228.6 97.79) (layer Edge.Cuts) (width 0.15))
)
