<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="26.34" y2="0" width="0" layer="20"/>
<wire x1="26.34" y1="0" x2="26.34" y2="38.09" width="0" layer="20"/>
<wire x1="26.34" y1="38.09" x2="0" y2="38.09" width="0" layer="20"/>
<wire x1="0" y1="38.09" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="IRL80A">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
IR transmitter Siemens</description>
</package>
<package name="TO92-EBC-OVAL">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="PNA460XM">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="DZ">
<description>Doug's custom made parts library</description>
<packages>
<package name="HUZZAH_OUTSIDE">
</package>
<package name="DHT11-VERT">
</package>
<package name="3_PIN_HEADER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="adafruit" package="IRL80A" value=""/>
<element name="R3" library="SparkFun-Passives" package="0402-RES" value="10"/>
<element name="R4" library="SparkFun-Passives" package="0402-RES" value="25k"/>
<element name="R5" library="SparkFun-Passives" package="0402-RES" value="1K"/>
<element name="T1" library="adafruit" package="TO92-EBC-OVAL" value="2N2222"/>
<element name="U$1" library="DZ" package="HUZZAH_OUTSIDE" value="HUZZAH_SHIELDOUTSIDE"/>
<element name="IRRCVR" library="adafruit" package="PNA460XM" value="PNA460XM"/>
<element name="U$3" library="DZ" package="DHT11-VERT" value="DHT11VERT"/>
<element name="U$4" library="DZ" package="3_PIN_HEADER" value="PIR"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="LED1" pad="K"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="T1" pad="C"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="T1" pad="E"/>
<contactref element="IRRCVR" pad="2"/>
<contactref element="U$3" pad="GND"/>
<contactref element="U$4" pad="-"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND2"/>
</signal>
<signal name="+5V">
<contactref element="LED1" pad="A"/>
<contactref element="U$1" pad="V+"/>
</signal>
<signal name="N$3">
<contactref element="T1" pad="B"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="2"/>
<contactref element="U$1" pad="#2"/>
</signal>
<signal name="+3V3">
<contactref element="IRRCVR" pad="3"/>
<contactref element="R4" pad="2"/>
<contactref element="U$3" pad="VCC"/>
<contactref element="U$4" pad="+"/>
<contactref element="U$1" pad="3V"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="13"/>
<contactref element="IRRCVR" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$3" pad="DATA"/>
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="N$7">
<contactref element="U$4" pad="D"/>
<contactref element="U$1" pad="#5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
