<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="-1.016" y1="-2.54" x2="66.853" y2="-2.286" width="0" layer="20"/>
<wire x1="66.853" y1="-2.286" x2="66.726" y2="74.031" width="0" layer="20"/>
<wire x1="66.726" y1="74.031" x2="-1.143" y2="73.777" width="0" layer="20"/>
<wire x1="-1.143" y1="73.777" x2="-1.016" y2="-2.54" width="0" layer="20"/>
<text>Buzz Super 8xVRX main Board</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="AVRISP">
</package>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LOCK_NO_SILK">
</package>
<package name="1X04-1MM-RA">
</package>
<package name="BM08B-SRSS-TB">
<description>JST crimp connector: 1mm pitch, top entry</description>
</package>
</packages>
</library>
<library name="con-jack">
<description>&lt;b&gt;Jacks&lt;/b&gt;&lt;p&gt;
Power Connectors&lt;br&gt;
Phone Connectors&lt;br&gt;
Cinch Connectors&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DCJ0202">
<description>&lt;b&gt;DC POWER JACK&lt;/b&gt;&lt;p&gt;
Source: DCJ0202.pdf</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="micro-philips">
<description>&lt;b&gt;Philips Microcontroller Devices&lt;/b&gt;&lt;p&gt;
http://www-eu2.semiconductors.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="I2C">
<description>&lt;b&gt;I2C LOGO&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C2.5-2">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 2.5 mm, grid 2.54 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun" package="1206" value="22pf"/>
<element name="C2" library="SparkFun" package="1206" value="22pf"/>
<element name="C3" library="SparkFun" package="1206" value="22pf"/>
<element name="C4" library="SparkFun" package="1206" value="22pf"/>
<element name="IC1" library="linear" package="TO220H" value="7805T"/>
<element name="IR1" library="SparkFun-Connectors" package="1X03_LOCK_NO_SILK" value="IR"/>
<element name="ISP1" library="adafruit" package="AVRISP" value="AVRISP-6"/>
<element name="J1" library="con-jack" package="DCJ0202" value="POWERIN">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="LED1" library="led" package="CHIPLED_1206" value="red"/>
<element name="LED2" library="led" package="CHIPLED_1206" value="red"/>
<element name="OLED" library="pinhead" package="1X04" value="oled"/>
<element name="Q1" library="adafruit" package="CTS406" value="16mhz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R1" library="SparkFun-Passives" package="1206" value="330"/>
<element name="R4" library="SparkFun-Passives" package="1206" value="330"/>
<element name="RS232" library="SparkFun-Connectors" package="1X04-1MM-RA" value="SERIAL"/>
<element name="S1" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="B3F-1000"/>
</element>
<element name="S2" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="B3F-1000"/>
</element>
<element name="S3" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="B3F-1000"/>
</element>
<element name="U$1" library="atmel" package="TQFP32-08" value="ATMEGA328P"/>
<element name="RX4" library="SparkFun-Connectors" package="BM08B-SRSS-TB" value="rxmodule4"/>
<element name="RX3" library="SparkFun-Connectors" package="BM08B-SRSS-TB" value="rxmodule3"/>
<element name="RX1" library="SparkFun-Connectors" package="BM08B-SRSS-TB" value="rxmodule1"/>
<element name="RX2" library="SparkFun-Connectors" package="BM08B-SRSS-TB" value="rxmodule2"/>
<element name="JP2" library="pinhead" package="1X08" value="VID OUT EXT"/>
<element name="JP1" library="pinhead" package="1X08" value="AUDIO OUT EXT"/>
<element name="JP5" library="pinhead" package="1X04" value=""/>
<element name="RX5" library="SparkFun-Connectors" package="BM08B-SRSS-TB" value="rxmodule5"/>
<element name="RX6" library="SparkFun-Connectors" package="BM08B-SRSS-TB" value="rxmodule6"/>
<element name="RX7" library="SparkFun-Connectors" package="BM08B-SRSS-TB" value="rxmodule7"/>
<element name="RX8" library="SparkFun-Connectors" package="BM08B-SRSS-TB" value="rxmodule8"/>
<element name="U$2" library="micro-philips" package="I2C" value=""/>
<element name="R2" library="SparkFun-Passives" package="1206" value="330"/>
<element name="LED3" library="led" package="CHIPLED_1206" value="red"/>
<element name="R3" library="SparkFun-Passives" package="1206" value="330"/>
<element name="LED4" library="led" package="CHIPLED_1206" value="red"/>
<element name="R5" library="SparkFun-Passives" package="1206" value="330"/>
<element name="LED5" library="led" package="CHIPLED_1206" value="red"/>
<element name="R6" library="SparkFun-Passives" package="1206" value="330"/>
<element name="LED6" library="led" package="CHIPLED_1206" value="red"/>
<element name="R7" library="SparkFun-Passives" package="1206" value="330"/>
<element name="LED7" library="led" package="CHIPLED_1206" value="red"/>
<element name="R8" library="SparkFun-Passives" package="1206" value="330"/>
<element name="LED8" library="led" package="CHIPLED_1206" value="red"/>
<element name="R9" library="SparkFun-Passives" package="1206" value="330"/>
<element name="LED9" library="led" package="CHIPLED_1206" value="red"/>
<element name="R10" library="SparkFun-Passives" package="1206" value="330"/>
<element name="LED10" library="led" package="CHIPLED_1206" value="red"/>
<element name="C5" library="capacitor-wima" package="C2.5-2" value="FILTR1"/>
<element name="C6" library="capacitor-wima" package="C2.5-2" value="FILTR2"/>
<element name="C7" library="capacitor-wima" package="C2.5-2" value="FILTR3"/>
<element name="C8" library="capacitor-wima" package="C2.5-2" value="FILTR4"/>
<element name="C9" library="capacitor-wima" package="C2.5-2" value="FILTR5"/>
<element name="C10" library="capacitor-wima" package="C2.5-2" value="FILTR6"/>
<element name="C11" library="capacitor-wima" package="C2.5-2" value="FILTR7"/>
<element name="C12" library="capacitor-wima" package="C2.5-2" value="FILTR8"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="7"/>
<contactref element="C2" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="21"/>
<contactref element="U$1" pad="5"/>
<contactref element="LED1" pad="C"/>
<contactref element="OLED" pad="1"/>
<contactref element="ISP1" pad="6"/>
<contactref element="RS232" pad="2"/>
<contactref element="IR1" pad="2"/>
<contactref element="LED2" pad="C"/>
<contactref element="S1" pad="3"/>
<contactref element="S3" pad="3"/>
<contactref element="S2" pad="3"/>
<contactref element="IC1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="RX3" pad="4"/>
<contactref element="RX4" pad="4"/>
<contactref element="RX1" pad="4"/>
<contactref element="RX2" pad="4"/>
<contactref element="RX5" pad="4"/>
<contactref element="RX6" pad="4"/>
<contactref element="RX7" pad="4"/>
<contactref element="RX8" pad="4"/>
<contactref element="JP5" pad="4"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED6" pad="C"/>
<contactref element="LED7" pad="C"/>
<contactref element="LED8" pad="C"/>
<contactref element="LED9" pad="C"/>
<contactref element="LED10" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="5V">
<contactref element="OLED" pad="2"/>
<contactref element="ISP1" pad="2"/>
<contactref element="RS232" pad="1"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="6"/>
<contactref element="IR1" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="JP5" pad="1"/>
<contactref element="U$1" pad="23"/>
</signal>
<signal name="SCL">
<contactref element="OLED" pad="3"/>
<contactref element="U$1" pad="28"/>
<contactref element="RX1" pad="2"/>
<contactref element="RX2" pad="2"/>
<contactref element="RX3" pad="2"/>
<contactref element="RX4" pad="2"/>
<contactref element="RX5" pad="2"/>
<contactref element="RX6" pad="2"/>
<contactref element="RX7" pad="2"/>
<contactref element="RX8" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="OLED" pad="4"/>
<contactref element="U$1" pad="27"/>
<contactref element="RX1" pad="1"/>
<contactref element="RX2" pad="1"/>
<contactref element="RX3" pad="1"/>
<contactref element="RX4" pad="1"/>
<contactref element="RX5" pad="1"/>
<contactref element="RX6" pad="1"/>
<contactref element="RX7" pad="1"/>
<contactref element="RX8" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="ISP1" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="29"/>
<contactref element="ISP1" pad="5"/>
</signal>
<signal name="TX">
<contactref element="RS232" pad="4"/>
<contactref element="U$1" pad="30"/>
</signal>
<signal name="RX">
<contactref element="RS232" pad="3"/>
<contactref element="U$1" pad="31"/>
</signal>
<signal name="SIG">
<contactref element="IR1" pad="1"/>
<contactref element="U$1" pad="32"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="S1">
<contactref element="S1" pad="1"/>
<contactref element="U$1" pad="9"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="S2">
<contactref element="S2" pad="1"/>
<contactref element="U$1" pad="10"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="S3">
<contactref element="S3" pad="1"/>
<contactref element="U$1" pad="11"/>
<contactref element="S3" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="IC1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="RX1" pad="5"/>
<contactref element="RX2" pad="5"/>
<contactref element="RX3" pad="5"/>
<contactref element="RX4" pad="5"/>
<contactref element="RX5" pad="5"/>
<contactref element="RX6" pad="5"/>
<contactref element="RX7" pad="5"/>
<contactref element="RX8" pad="5"/>
</signal>
<signal name="2O">
<contactref element="U$1" pad="15"/>
<contactref element="ISP1" pad="4"/>
</signal>
<signal name="3O">
<contactref element="ISP1" pad="1"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="VIDEOOUT1">
<contactref element="RX1" pad="8"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="VIDEOOUT2">
<contactref element="RX2" pad="8"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="VIDEOOUT3">
<contactref element="RX3" pad="8"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="VIDEOOUT4">
<contactref element="RX4" pad="8"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="AUDIO1">
<contactref element="RX1" pad="7"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="AUDIO2">
<contactref element="RX2" pad="7"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="AUDIO3">
<contactref element="RX3" pad="7"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="AUDIO4">
<contactref element="RX4" pad="7"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="AUDIO5">
<contactref element="JP1" pad="2"/>
<contactref element="RX5" pad="7"/>
</signal>
<signal name="AUDIO6">
<contactref element="JP1" pad="4"/>
<contactref element="RX6" pad="7"/>
</signal>
<signal name="AUDIO7">
<contactref element="JP1" pad="6"/>
<contactref element="RX7" pad="7"/>
</signal>
<signal name="AUDIO8">
<contactref element="JP1" pad="8"/>
<contactref element="RX8" pad="7"/>
</signal>
<signal name="VIDEOOUT5">
<contactref element="RX5" pad="8"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="VIDEOOUT6">
<contactref element="RX6" pad="8"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="VIDEOOUT7">
<contactref element="RX7" pad="8"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="VIDEOOUT8">
<contactref element="RX8" pad="8"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="RF433">
<contactref element="JP5" pad="2"/>
<contactref element="JP5" pad="3"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="2"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="2"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="R6" pad="2"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="R7" pad="2"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="R8" pad="2"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="R9" pad="2"/>
<contactref element="LED9" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="R10" pad="2"/>
<contactref element="LED10" pad="A"/>
</signal>
<signal name="MOD1">
<contactref element="R2" pad="1"/>
<contactref element="RX1" pad="6"/>
</signal>
<signal name="MOD2">
<contactref element="R3" pad="1"/>
<contactref element="RX2" pad="6"/>
</signal>
<signal name="MOD3">
<contactref element="R5" pad="1"/>
<contactref element="RX3" pad="6"/>
</signal>
<signal name="MOD4">
<contactref element="R6" pad="1"/>
<contactref element="RX4" pad="6"/>
</signal>
<signal name="MOD5">
<contactref element="R7" pad="1"/>
<contactref element="RX5" pad="6"/>
</signal>
<signal name="MOD6">
<contactref element="R8" pad="1"/>
<contactref element="RX6" pad="6"/>
</signal>
<signal name="MOD7">
<contactref element="R9" pad="1"/>
<contactref element="RX7" pad="6"/>
</signal>
<signal name="MOD8">
<contactref element="R10" pad="1"/>
<contactref element="RX8" pad="6"/>
</signal>
<signal name="VIDEOOUT5X">
<contactref element="C9" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="VIDEOOUT1X">
<contactref element="JP2" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="VIDEOOUT2X">
<contactref element="JP2" pad="3"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="VIDEOOUT3X">
<contactref element="JP2" pad="5"/>
</signal>
<signal name="VIDEOOUT4X">
<contactref element="JP2" pad="7"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="VIDEOOUT6X">
<contactref element="JP1" pad="3"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="VIDEOOUT7X">
<contactref element="JP1" pad="5"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="VIDEOOUT8X">
<contactref element="JP1" pad="7"/>
<contactref element="C12" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
