<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="32.69" y2="0" width="0" layer="20"/>
<wire x1="32.69" y1="0" x2="32.69" y2="46.98" width="0" layer="20"/>
<wire x1="32.69" y1="46.98" x2="0" y2="46.98" width="0" layer="20"/>
<wire x1="0" y1="46.98" x2="0" y2="0" width="0" layer="20"/>
<text>ACT</text>
<text>3V0</text>
<text>GND</text>
<text>RX</text>
<text>TX</text>
<text>SCK</text>
<text>REQn</text>
<text>MOSI</text>
<text>MISO</text>
<text>RDYn</text>
<text>RST</text>
<text>3V0</text>
<text>GND</text>
<text>MOSI</text>
<text>Oct2014</text>
<text>Bluetooth</text>
<text>PulseOx</text>
<text>Sensor</text>
<text>Will Eccles</text>
<text>Mike Litster</text>
</plain>
<libraries>
<library name="myq - CR2032 battery clip">
<packages>
<package name="BK-912">
</package>
</packages>
</library>
<library name="Atmega168 Dev Board rev1">
<description>Generated from &lt;b&gt;Atmega168 Dev Board rev1.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="0805">
</package>
<package name="AVRISP">
</package>
<package name="TACTILE_SWITCH_SMD">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="Texas Instruments_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="SOT95P280X145-6N">
</package>
</packages>
</library>
<library name="con-subd">
<description>&lt;b&gt;SUB-D Connectors&lt;/b&gt;&lt;p&gt;
Harting&lt;br&gt;
NorComp&lt;br&gt;
&lt;p&gt;
PREFIX :&lt;br&gt;
H = High density&lt;br&gt;
F = Female&lt;br&gt;
M = Male&lt;p&gt;
NUMBER: Number of pins&lt;p&gt;
SUFFIX :&lt;br&gt;
H = Horizontal&lt;br&gt;
V = Vertical &lt;br&gt;
P = Shield pin on housing&lt;br&gt;
B = No mounting holes&lt;br&gt;
S = Pins individually placeable (Single)&lt;br&gt;
D = Direct mounting &lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="M09HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="myq-connectors">
<packages>
<package name="1X11">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BATTERY" library="myq - CR2032 battery clip" package="BK-912" value="BK-912_CR2032_CLIP"/>
<element name="C1" library="Atmega168 Dev Board rev1" package="0805" value="0.1uF"/>
<element name="C2" library="Atmega168 Dev Board rev1" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISP1" library="Atmega168 Dev Board rev1" package="AVRISP" value="AVRISP-6">
<attribute name="NAME"/>
</element>
<element name="R1" library="Atmega168 Dev Board rev1" package="0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Atmega168 Dev Board rev1" package="0805" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Atmega168 Dev Board rev1" package="0805" value="10M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="S1" library="Atmega168 Dev Board rev1" package="TACTILE_SWITCH_SMD" value=""/>
<element name="U$3" library="Atmega168 Dev Board rev1" package="TQFP32-08" value="ATMEGA168">
<attribute name="VALUE"/>
</element>
<element name="U1" library="Texas Instruments_By_element14_Batch_1" package="SOT95P280X145-6N" value="OPA835IDBVT">
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="OC_NEWARK" value="48T0415"/>
<attribute name="MPN" value="OPA835IDBVT"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="1903635"/>
</element>
<element name="X1" library="con-subd" package="M09HP" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="NRF8001" library="myq-connectors" package="1X11" value="NRF8001_JAYCON"/>
</elements>
<signals>
<signal name="LED1">
<contactref element="X1" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="LED2">
<contactref element="X1" pad="3"/>
<contactref element="U$3" pad="11"/>
</signal>
<signal name="GND">
<contactref element="X1" pad="7"/>
<contactref element="X1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="2"/>
<contactref element="BATTERY" pad="-"/>
<contactref element="R7" pad="1"/>
<contactref element="U$3" pad="5"/>
<contactref element="U$3" pad="3"/>
<contactref element="U$3" pad="21"/>
<contactref element="ISP1" pad="6"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="NRF8001" pad="10"/>
</signal>
<signal name="+3V0">
<contactref element="U1" pad="6"/>
<contactref element="BATTERY" pad="+"/>
<contactref element="BATTERY" pad="3"/>
<contactref element="U$3" pad="6"/>
<contactref element="R2" pad="2"/>
<contactref element="U$3" pad="18"/>
<contactref element="U$3" pad="4"/>
<contactref element="ISP1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="NRF8001" pad="9"/>
</signal>
<signal name="PHOTO+">
<contactref element="X1" pad="9"/>
<contactref element="U1" pad="4"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="ADC">
<contactref element="R1" pad="2"/>
<contactref element="U$3" pad="23"/>
</signal>
<signal name="PD">
<contactref element="U1" pad="5"/>
<contactref element="U$3" pad="24"/>
</signal>
<signal name="N$13">
<contactref element="S1" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="SW">
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="U$3" pad="32"/>
</signal>
<signal name="OPAMP_OUT">
<contactref element="R4" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="ISP1" pad="4"/>
<contactref element="U$3" pad="15"/>
<contactref element="NRF8001" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="ISP1" pad="1"/>
<contactref element="U$3" pad="16"/>
<contactref element="NRF8001" pad="3"/>
</signal>
<signal name="RST">
<contactref element="ISP1" pad="5"/>
<contactref element="U$3" pad="29"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="ISP1" pad="3"/>
<contactref element="U$3" pad="17"/>
<contactref element="NRF8001" pad="6"/>
</signal>
<signal name="RDYN">
<contactref element="U$3" pad="14"/>
<contactref element="NRF8001" pad="2"/>
</signal>
<signal name="REQN">
<contactref element="U$3" pad="13"/>
<contactref element="NRF8001" pad="5"/>
</signal>
<signal name="ACT">
<contactref element="U$3" pad="12"/>
<contactref element="NRF8001" pad="11"/>
</signal>
<signal name="N$1">
<contactref element="C2" pad="1"/>
<contactref element="U$3" pad="20"/>
</signal>
<signal name="N$2">
<contactref element="U$3" pad="10"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="RX">
<contactref element="U$3" pad="30"/>
<contactref element="NRF8001" pad="8"/>
</signal>
<signal name="TX">
<contactref element="U$3" pad="31"/>
<contactref element="NRF8001" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
