(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+15V")
	(net 2 "GND")
	(net 3 "unconnected-(U1B-Q3-Pad13)")
	(net 4 "unconnected-(U1A-Q4-Pad6)")
	(net 5 "unconnected-(U1A-Q3-Pad5)")
	(net 6 "unconnected-(U1B-Q2-Pad12)")
	(net 7 "unconnected-(U1B-Q4-Pad14)")
	(net 8 "unconnected-(U2B-Q4-Pad14)")
	(net 9 "unconnected-(U2B-Q3-Pad13)")
	(net 10 "unconnected-(U2A-Q2-Pad4)")
	(net 11 "unconnected-(U2A-Q3-Pad5)")
	(net 12 "unconnected-(U2A-Q4-Pad6)")
	(net 13 "Net-(J1-Pin_12)")
	(net 14 "Net-(J1-Pin_14)")
	(net 15 "Net-(J1-Pin_4)")
	(net 16 "unconnected-(J1-Pin_5-Pad5)")
	(net 17 "Net-(J1-Pin_3)")
	(net 18 "Net-(J1-Pin_13)")
	(net 19 "Net-(J1-Pin_2)")
	(net 20 "Net-(J1-Pin_6)")
	(net 21 "Net-(J1-Pin_11)")
	(net 22 "Net-(J1-Pin_9)")
	(net 23 "unconnected-(J1-Pin_1-Pad1)")
	(net 24 "Net-(J1-Pin_10)")
	(footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 139.0575 103.839)
		(descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U1"
			(at 2.4713 3.8062 0)
			(layer "F.SilkS")
		)
		(property "Value" "CD4520"
			(at -1.6943 3.7554 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd45/cd4518bms-20bms.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual Binary Up-Counter"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?16*")
		(sheetname "/")
		(sheetfile "mm5283_cd4520.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(J1-Pin_6)")
			(pinfunction "CK")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+15V")
			(pinfunction "Enable")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(J1-Pin_9)")
			(pinfunction "Q1")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(J1-Pin_10)")
			(pinfunction "Q2")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "unconnected-(U1A-Q3-Pad5)")
			(pinfunction "Q3")
			(pintype "output+no_connect")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "unconnected-(U1A-Q4-Pad6)")
			(pinfunction "Q4")
			(pintype "output+no_connect")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Reset")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.8625 2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 2.8625 2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(J1-Pin_4)")
			(pinfunction "CK")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.8625 1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+15V")
			(pinfunction "Enable")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.8625 0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(J1-Pin_11)")
			(pinfunction "Q1")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 2.8625 0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "unconnected-(U1B-Q2-Pad12)")
			(pinfunction "Q2")
			(pintype "output+no_connect")
		)
		(pad "13" smd roundrect
			(at 2.8625 -0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "unconnected-(U1B-Q3-Pad13)")
			(pinfunction "Q3")
			(pintype "output+no_connect")
		)
		(pad "14" smd roundrect
			(at 2.8625 -0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "unconnected-(U1B-Q4-Pad14)")
			(pinfunction "Q4")
			(pintype "output+no_connect")
		)
		(pad "15" smd roundrect
			(at 2.8625 -1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Reset")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 2.8625 -2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+15V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 110.8613 103.7844 180)
		(descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U2"
			(at -1.6894 3.591302 0)
			(layer "F.SilkS")
		)
		(property "Value" "CD4520"
			(at 2.527 3.692902 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd45/cd4518bms-20bms.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual Binary Up-Counter"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?16*")
		(sheetname "/")
		(sheetfile "mm5283_cd4520.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(J1-Pin_3)")
			(pinfunction "CK")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+15V")
			(pinfunction "Enable")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(J1-Pin_12)")
			(pinfunction "Q1")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "unconnected-(U2A-Q2-Pad4)")
			(pinfunction "Q2")
			(pintype "output+no_connect")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "unconnected-(U2A-Q3-Pad5)")
			(pinfunction "Q3")
			(pintype "output+no_connect")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "unconnected-(U2A-Q4-Pad6)")
			(pinfunction "Q4")
			(pintype "output+no_connect")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Reset")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(J1-Pin_2)")
			(pinfunction "CK")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+15V")
			(pinfunction "Enable")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(J1-Pin_13)")
			(pinfunction "Q1")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(J1-Pin_14)")
			(pinfunction "Q2")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "unconnected-(U2B-Q3-Pad13)")
			(pinfunction "Q3")
			(pintype "output+no_connect")
		)
		(pad "14" smd roundrect
			(at 2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "unconnected-(U2B-Q4-Pad14)")
			(pinfunction "Q4")
			(pintype "output+no_connect")
		)
		(pad "15" smd roundrect
			(at 2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Reset")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+15V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric_Pad0.64x0.40mm_HandSolder"
		(layer "F.Cu")
		(at 142.0216 100.425601)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at -0.0356 -1.213201 0)
			(layer "F.SilkS")
		)
		(property "Value" ".1uf"
			(at -2.9312 -1.289401 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "mm5283_cd4520.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.680001 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.4325 0)
			(size 0.458 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.4325 0)
			(size 0.458 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.4075 0)
			(size 0.635 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.4075 0)
			(size 0.635 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric_Pad0.64x0.40mm_HandSolder"
		(layer "F.Cu")
		(at 107.9326 107.1678 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0.0842 -1.2394 0)
			(layer "F.SilkS")
		)
		(property "Value" ".1uf"
			(at -2.5066 -1.1886 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "mm5283_cd4520.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.680001 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.4325 0 180)
			(size 0.458 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.4325 0 180)
			(size 0.458 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.4075 0 180)
			(size 0.635 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.4075 0 180)
			(size 0.635 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:CERDIP-14_W7.62mm_SideBrazed_LongPads_Socket"
		(layer "F.Cu")
		(at 117.312 107.69 90)
		(descr "14-lead through-hole mounted CERDIP, JEDEC MS-015-AB package, row spacing 7.62mm (300 mils), SideBrazed, LongPads, Socket, https://www.jedec.org/system/files/docs/Ms-015a.pdf")
		(tags "THT DIP DIL CERDIP ceramic 2.54mm 7.62mm 300mil SideBrazed LongPads Socket")
		(property "Reference" "J1"
			(at -1.53 -3.2152 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x14_Pin"
			(at 12.3892 7.0464 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x14, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "mm5283_cd4520.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(J1-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.079999 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J1-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(J1-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J1-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+15V")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J1-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J1-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J1-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J1-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J1-Pin_13)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 7.62 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J1-Pin_14)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/CERDIP-14_W7.62mm_SideBrazed_LongPads_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "rat_footprints:timotetfx_25"
		(layer "F.Cu")
		(at 131.354101 102.98971 90)
		(property "Reference" "G***"
			(at 0.127 4.318001 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "rat_footprints:timotetfx"
		(layer "B.Cu")
		(at 111.8108 103.3018 90)
		(property "Reference" "G***"
			(at -1.143 -7.62 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(gr_line
		(start 143.256 96.52)
		(end 106.68 96.52)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.78 108.712)
		(end 144.78 98.044)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 144.78 108.712)
		(mid 144.333631 109.789631)
		(end 143.256 110.236)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 143.256 96.52)
		(mid 144.333631 96.966369)
		(end 144.78 98.044)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 105.156 98.044)
		(mid 105.602369 96.966369)
		(end 106.68 96.52)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.156 98.044)
		(end 105.156 108.712)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 106.68 110.236)
		(mid 105.602369 109.789631)
		(end 105.156 108.712)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.68 110.236)
		(end 143.256 110.236)
		(layer "Edge.Cuts")
	)
	(gr_text "1"
		(at 116.1288 108.1786 90)
		(layer "F.SilkS")
	)
	(gr_text "14"
		(at 116.3066 101.0158 90)
		(layer "F.SilkS")
	)
	(gr_text "MM5283 conversion board V1\n             6/18/25"
		(at 126.746 98.6282 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.127)
			(thermal_bridge_width 0.127)
		)
		(polygon
			(pts
				(xy 144.8816 110.236) (xy 105.156 110.236) (xy 105.2068 96.5708) (xy 144.8816 96.52) (xy 144.9324 110.1852)
			)
		)
	)
	(embedded_fonts no)
)
