(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "GND")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(J2-Pin_1)")
  (net 6 "Net-(C4-Pad2)")
  (net 7 "Net-(J1-Pin_1)")
  (net 8 "unconnected-(J3-Pad6)")
  (net 9 "unconnected-(J3-Pad3)")
  (footprint "Connector_Coaxial:SMA_Amphenol_132134-11_Vertical" (layer "F.Cu")
    (at 75.8723 48.1584)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/3406/product/2975/132134_11_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical ExtendedLegs")
    (property "Sheetfile" "FEMB SiPM test board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -4.75) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134-11_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 84.9147 44.4464 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "FEMB SiPM test board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (at 90.3249 44.5498 90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "FEMB SiPM test board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 -2.3 90) (layer "F.SilkS"))
    (fp_text value "C" (at 0 2.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 96.9949 71.633)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "FEMB SiPM test board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "Charge injection" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 103.5837 72.583 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "FEMB SiPM test board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "C_det" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 110.4823 49.1236)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "FEMB SiPM test board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "Cb" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 89.5394 50.165)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "FEMB SiPM test board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 84.434 50.1904)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "FEMB SiPM test board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 7 "Net-(J1-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_132134-11_Vertical" (layer "F.Cu")
    (at 75.8469 64.6684)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/3406/product/2975/132134_11_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical ExtendedLegs")
    (property "Sheetfile" "FEMB SiPM test board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -4.75) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J2-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134-11_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SiPM:SiPM array" (layer "F.Cu")
    (at 100.4087 59.7408)
    (property "Sheetfile" "FEMB SiPM test board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 9.3701 0.4572 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at -0.4872 13.3632 unlocked) (layer "F.Fab"))
    (fp_text user "A4" (at 3.12 -2.89 unlocked) (layer "F.SilkS"))
    (fp_text user "K2" (at -4.95 7.03 unlocked) (layer "F.SilkS"))
    (fp_text user "K4" (at 3.06 -5.56 unlocked) (layer "F.SilkS"))
    (fp_text user "A2" (at -4.89 4.36 unlocked) (layer "F.SilkS"))
    (fp_text user "K3" (at 2.74 4.42 unlocked) (layer "F.SilkS"))
    (fp_text user "A3" (at 2.93 7.03 unlocked) (layer "F.SilkS"))
    (fp_text user "K1" (at -4.64 -3.14 unlocked) (layer "F.SilkS"))
    (fp_text user "A1" (at -4.57 -5.69 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.8235 0.4572 unlocked) (layer "F.Fab"))
    (pad "A1" thru_hole circle (at -6.35 -6.35) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "unspecified"))
    (pad "A2" thru_hole circle (at -6.35 3.81) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "unspecified"))
    (pad "A3" thru_hole circle (at 6.35 6.35) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "unspecified"))
    (pad "A4" thru_hole circle (at 6.35 -3.81) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "unspecified"))
    (pad "K1" thru_hole circle (at -6.35 -3.81) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(C2-Pad1)") (pintype "unspecified"))
    (pad "K2" thru_hole circle (at -6.35 6.35) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(C2-Pad1)") (pintype "unspecified"))
    (pad "K3" thru_hole circle (at 6.35 3.81) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(C2-Pad1)") (pintype "unspecified"))
    (pad "K4" thru_hole circle (at 6.35 -6.35) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(C2-Pad1)") (pintype "unspecified"))
  )
  (footprint "TSW_102_07_G_T:CON6_3X2_TU_TSW_SAI" (layer "B.Cu")
    (at 118.3411 54.7624 90)
    (tags "TSW-102-07-G-T ")
    (property "Sheetfile" "FEMB SiPM test board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "TSW-102-07-G-T")
    (attr through_hole)
    (fp_text reference "J3" (at 0.0762 4.9251 270 unlocked) (layer "B.SilkS"))
    (fp_text value "TSW-102-07-G-T" (at 0 0 270 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 4.9251 270 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 1.27 -2.54) (size 1.397 1.397) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(C3-Pad2)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 1.27 2.54) (size 1.397 1.397) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(J3-Pad3)") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at -1.27 -2.54) (size 1.397 1.397) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C4-Pad2)") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at -1.27 2.54) (size 1.397 1.397) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 8 "unconnected-(J3-Pad6)") (pinfunction "6") (pintype "unspecified"))
  )
  (gr_rect (start 70.0786 40.9956) (end 124.3076 75.2602)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "+HV" (at 73.914 54.0004) (layer "F.SilkS"))
  (gr_text "Charge\ninjection" (at 72.9996 71.9328) (layer "F.SilkS"))
  (gr_text "SLAC FEMB SiPM test board 02\n" (at 96.0374 44.5516) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 70.2056 41.148)
        (xy 124.0536 41.2496)
        (xy 124.1044 75.0316)
        (xy 70.2564 75.0824)
      )
    )
  )
)
