(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 31)
    (tracks 915)
    (zones 0)
    (modules 82)
    (nets 80)
  )
  (page A)
  (title_block
    (title "Beetje 32U4 Blok")
    (date 2018-08-10)
    (rev 0.0)
    (company www.MakersBox.us)
    (comment 1 648.ken@gmail.com)
  )
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.3556)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (trace_clearance 0.2)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 0.508)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f8_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /D4)
  (net 3 /D6)
  (net 4 /D8)
  (net 5 /D13)
  (net 6 /D12)
  (net 7 /D10)
  (net 8 /D9)
  (net 9 /D7)
  (net 10 /A0)
  (net 11 /A3)
  (net 12 /A5)
  (net 13 /SCK)
  (net 14 /MOSI)
  (net 15 /MISO)
  (net 16 /D5)
  (net 17 /RXLED)
  (net 18 /TXLED)
  (net 19 /~RESET)
  (net 20 /D+)
  (net 21 /D-)
  (net 22 "Net-(F1-Pad2)")
  (net 23 +5V)
  (net 24 "Net-(D4-Pad2)")
  (net 25 "Net-(R6-Pad2)")
  (net 26 "Net-(R7-Pad2)")
  (net 27 "Net-(R9-Pad2)")
  (net 28 "Net-(D1-Pad2)")
  (net 29 "Net-(D2-Pad2)")
  (net 30 "Net-(D3-Pad2)")
  (net 31 "Net-(D5-Pad2)")
  (net 32 "Net-(D6-Pad2)")
  (net 33 "Net-(D7-Pad2)")
  (net 34 "Net-(D8-Pad2)")
  (net 35 "Net-(D9-Pad2)")
  (net 36 "Net-(D10-Pad2)")
  (net 37 "Net-(D11-Pad2)")
  (net 38 "Net-(D12-Pad2)")
  (net 39 "Net-(D13-Pad2)")
  (net 40 "Net-(D14-Pad2)")
  (net 41 "Net-(D15-Pad2)")
  (net 42 "Net-(D16-Pad2)")
  (net 43 "Net-(D17-Pad2)")
  (net 44 "Net-(D18-Pad2)")
  (net 45 "Net-(D19-Pad2)")
  (net 46 "Net-(D20-Pad2)")
  (net 47 "Net-(D22-Pad1)")
  (net 48 "Net-(D23-Pad1)")
  (net 49 "Net-(J1-Pad2)")
  (net 50 "Net-(J1-Pad3)")
  (net 51 "Net-(R1-Pad2)")
  (net 52 "Net-(R2-Pad2)")
  (net 53 "Net-(R3-Pad2)")
  (net 54 "Net-(R4-Pad2)")
  (net 55 "Net-(R5-Pad2)")
  (net 56 "Net-(R8-Pad2)")
  (net 57 "Net-(R10-Pad2)")
  (net 58 "Net-(R11-Pad2)")
  (net 59 "Net-(R12-Pad2)")
  (net 60 "Net-(R13-Pad2)")
  (net 61 "Net-(R14-Pad2)")
  (net 62 "Net-(R15-Pad2)")
  (net 63 "Net-(R16-Pad2)")
  (net 64 "Net-(R17-Pad2)")
  (net 65 "Net-(R18-Pad2)")
  (net 66 "Net-(R19-Pad2)")
  (net 67 "Net-(R20-Pad2)")
  (net 68 "Net-(D21-Pad1)")
  (net 69 "Net-(R26-Pad2)")
  (net 70 "Net-(R26-Pad1)")
  (net 71 /D3_SCL)
  (net 72 /D2_SDA)
  (net 73 /D0)
  (net 74 /D1)
  (net 75 /D11)
  (net 76 /A1)
  (net 77 /A2)
  (net 78 /A4)
  (net 79 /Vin)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /D+)
    (add_net /D-)
    (add_net /D0)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D2_SDA)
    (add_net /D3_SCL)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RXLED)
    (add_net /SCK)
    (add_net /TXLED)
    (add_net /Vin)
    (add_net /~RESET)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D17-Pad2)")
    (add_net "Net-(D18-Pad2)")
    (add_net "Net-(D19-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D20-Pad2)")
    (add_net "Net-(D21-Pad1)")
    (add_net "Net-(D22-Pad1)")
    (add_net "Net-(D23-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R20-Pad2)")
    (add_net "Net-(R26-Pad1)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 638D3D71)
    (at 161 89.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R30 (at 1.905 0 90) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:DFN-8-1EP_3x2mm (layer F.Cu) (tedit 638D3D4D)
    (at 158 89.5 180)
    (descr "8-Lead Plastic Dual Flat, No Lead Package (8MA2) - 2x3x0.6 mm Body [UDFN] (see Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U3 (at 0 -2.55) (layer F.SilkS) hide)
    (fp_text value 24LC32 (at 0 2) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 0.325 0.375 180) (size 0.5 0.6) (layers F.Paste))
    (pad "" smd rect (at 0.325 -0.375 180) (size 0.5 0.6) (layers F.Paste))
    (pad "" smd rect (at -0.325 0.375 180) (size 0.5 0.6) (layers F.Paste))
    (pad "" smd rect (at -0.325 -0.375 180) (size 0.5 0.6) (layers F.Paste))
    (pad 9 smd rect (at 0 0 180) (size 1.3 1.5) (layers F.Cu F.Mask))
    (pad 8 smd rect (at 1.45 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.45 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.45 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.45 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -1.45 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.45 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.45 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.45 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 110 91 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at -2.54 0 180) (layer Dwgs.User))
    (fp_text value 1K (at -2.5 0 180) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D21-Pad1)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 127 104 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 4K7 (at -2.5 1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 /D2_SDA))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 637975D3)
    (at 154.94 80.645)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value ISP (at 1.31 -2.395) (layer F.SilkS))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 0.508) (layers *.Cu F.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 0.508) (layers *.Cu F.Mask)
      (net 19 /~RESET))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 0.508) (layers *.Cu F.Mask)
      (net 14 /MOSI))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 0.508) (layers *.Cu F.Mask)
      (net 13 /SCK))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 0.508) (layers *.Cu F.Mask)
      (net 23 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 0.508) (layers *.Cu F.Mask)
      (net 15 /MISO))
  )
  (module footprints:INPI33TBTPRPGPB (layer F.Cu) (tedit 0)
    (at 110 108 180)
    (descr IN-PI33TBTPRPGPB-5)
    (tags LED)
    (attr smd)
    (fp_text reference LED1 (at 0.53 0) (layer F.SilkS) hide)
    (fp_text value IN-PI33TBTPRPGPB (at 0.53 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0.53 0) (layer F.Fab))
    (pad 1 smd rect (at 1.59 1.07 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.59 -1.07 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /D13))
    (pad 3 smd rect (at -1.59 -1.07 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 4 smd rect (at -1.59 1.07 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask))
    (model IN-PI33TBTPRPGPB.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/3D/IN-PI33TBTPRPGPB.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 636FC06B)
    (at 110.5 94 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference F1 (at -3.17 0) (layer F.SilkS))
    (fp_text value Polyfuse (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(F1-Pad2)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 79 /Vin))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/3D/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 110 89 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D22 (at 2.032 0) (layer F.SilkS) hide)
    (fp_text value TX (at 2 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D22-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SW_TS10-63-26-BE-250-SMT-TR (layer F.Cu) (tedit 63700F95)
    (at 169 100.33 90)
    (fp_text reference SW1 (at 0 -0.09 90) (layer F.SilkS))
    (fp_text value RESET (at -5.67 0) (layer F.SilkS))
    (pad 1 smd rect (at -3.25 0 90) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.25 0 90) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 19 /~RESET))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_FSMSM.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 133.65 83.1 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 2.54 0 180) (layer Dwgs.User))
    (fp_text value 1K (at -2.1 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D22-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 /TXLED))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:M25standoff (layer F.Cu) (tedit 636FF644)
    (at 168 88)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (fp_text reference P5 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value Standoff (at 0 5.08) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.7) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/3D/standoff9774027151R (rev1).stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3D/99607A263_Stainless Steel Flared-Collar Knurled-Head Thumb Screw.STEP"
      (offset (xyz 0 0 4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:M25standoff (layer F.Cu) (tedit 636FF644)
    (at 168 110)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (fp_text reference P6 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value Standoff (at 0 5.08) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.7) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/3D/standoff9774027151R (rev1).stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/3D/M2_5X6MM.step
      (offset (xyz 0 0 6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:M3mount (layer F.Cu) (tedit 636FC1C2)
    (at 110.49 80.01)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (fp_text reference P1 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 5.08) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask))
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 114.935 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 1 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D1-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 110 85 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D21 (at 2.032 0) (layer F.SilkS) hide)
    (fp_text value PWR (at 0 1.25 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D21-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 110 87 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D23 (at 2.032 0) (layer F.SilkS) hide)
    (fp_text value RX (at 2 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D23-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 140.335 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D11 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 11 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D11-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 117.475 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 2 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D2-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 142.875 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D12 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 12 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D12-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 120.015 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 3 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D3-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 145.415 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D13 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 13 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D13-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 122.555 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 4 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D4-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 147.955 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D14 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 14 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D14-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 125.095 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 5 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D5-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 150.495 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D15 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 15 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D15-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 127.635 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 6 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D6-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 153.035 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D16 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 16 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D16-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 130.175 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 7 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D7-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 155.575 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D17 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 17 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D17-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 132.715 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D8 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 8 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D8-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 158.115 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D18 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 18 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D18-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 135.255 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D9 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 9 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D9-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 160.655 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D19 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 19 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D19-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 137.795 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D10 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 10 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D10-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 163.195 123.66 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D20 (at 2.032 0 90) (layer F.SilkS) hide)
    (fp_text value 20 (at -2.286 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D20-Pad2)"))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 140.335 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R11-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D11-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 133.65 81.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at -0.127 1.27 180) (layer Dwgs.User))
    (fp_text value 1K (at -2.032 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D23-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /RXLED))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 120 100 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at 1.905 0 180) (layer Dwgs.User) hide)
    (fp_text value 22 (at -2 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J1-Pad3)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 /D+))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 120 98 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 22 (at -2 -0.055 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /D-))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 139.7 80.01 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at 3.175 0 180) (layer Dwgs.User))
    (fp_text value 1M (at -1.905 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R26-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R26-Pad1)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 116.25 100 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference RV1 (at 2 -0.75 180) (layer F.SilkS))
    (fp_text value Varistor (at -1.905 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J1-Pad3)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 116.25 98 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference RV2 (at 2.25 0.75 180) (layer F.SilkS))
    (fp_text value Varistor (at -1.905 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J1-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 114.935 120 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D1-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 117.475 120 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R2-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D2-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 142.875 119.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R12-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D12-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 120.015 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R3-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D3-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 145.415 119.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R13-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D13-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 122.555 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R4-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D4-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 147.955 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R14-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D14-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 125.095 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R5-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D5-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 150.495 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R15-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D15-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 127.635 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R6-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D6-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 153.035 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R16-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D16-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 130.175 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R7-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D7-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 155.575 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R17-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D17-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 132.715 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R8-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D8-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 158.115 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R18-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D18-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 135.255 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R9-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D9-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 160.655 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R19-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D19-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 137.795 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R10-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D10-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 163.195 120.015 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R20-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D20-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Resonator_SMD_CTSC_1.3mmx3.2mm (layer F.Cu) (tedit 636FC12A)
    (at 139.77 81.915)
    (descr "SMD Resomator/Filter Murata TPSKA, http://cdn-reichelt.de/documents/datenblatt/B400/SFECV-107.pdf, hand-soldering, 7.9x3.8mm^2 package")
    (tags "SMD SMT ceramic resonator filter filter hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at -0.127 -1.27) (layer F.SilkS) hide)
    (fp_text value "16 Mhz" (at -0.07 1.397) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1.2 0) (size 0.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R26-Pad1)"))
    (pad 2 smd rect (at 0 0) (size 0.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.2 0) (size 0.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R26-Pad2)"))
    (model ${KIPRJMOD}/3D/resontator_CSTNE16M0V530000R0.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:TQFP-44_10x10mm_Pitch0.8mm (layer F.Cu) (tedit 636FBFD2)
    (at 139.7 90.805 180)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 5.45 6.27 180) (layer F.SilkS))
    (fp_text value ATMEGA32U4-AU (at -0.127 -4.195 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 /D7))
    (pad 2 smd rect (at -5.7 -3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -5.7 -2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 /D-))
    (pad 4 smd rect (at -5.7 -1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /D+))
    (pad 5 smd rect (at -5.7 -0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -5.7 0 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 7 smd rect (at -5.7 0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 8 smd rect (at -5.7 1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 /RXLED))
    (pad 9 smd rect (at -5.7 2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 /SCK))
    (pad 10 smd rect (at -5.7 3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /MOSI))
    (pad 11 smd rect (at -5.7 4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 /MISO))
    (pad 12 smd rect (at -4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 75 /D11))
    (pad 13 smd rect (at -3.2 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /~RESET))
    (pad 14 smd rect (at -2.4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 15 smd rect (at -1.6 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -0.8 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R26-Pad1)"))
    (pad 17 smd rect (at 0 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R26-Pad2)"))
    (pad 18 smd rect (at 0.8 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 71 /D3_SCL))
    (pad 19 smd rect (at 1.6 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 72 /D2_SDA))
    (pad 20 smd rect (at 2.4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 73 /D0))
    (pad 21 smd rect (at 3.2 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 74 /D1))
    (pad 22 smd rect (at 4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 /TXLED))
    (pad 23 smd rect (at 5.7 4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 5.7 3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 25 smd rect (at 5.7 2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 /D4))
    (pad 26 smd rect (at 5.7 1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /D12))
    (pad 27 smd rect (at 5.7 0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 /D6))
    (pad 28 smd rect (at 5.7 0 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 /D8))
    (pad 29 smd rect (at 5.7 -0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 /D9))
    (pad 30 smd rect (at 5.7 -1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 /D10))
    (pad 31 smd rect (at 5.7 -2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /D5))
    (pad 32 smd rect (at 5.7 -3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 /D13))
    (pad 33 smd rect (at 5.7 -4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 34 smd rect (at 4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 35 smd rect (at 3.2 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 2.4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 /A0))
    (pad 37 smd rect (at 1.6 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 76 /A1))
    (pad 38 smd rect (at 0.8 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 77 /A2))
    (pad 39 smd rect (at 0 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /A3))
    (pad 40 smd rect (at -0.8 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 78 /A4))
    (pad 41 smd rect (at -1.6 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /A5))
    (pad 42 smd rect (at -2.4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 43 smd rect (at -3.2 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 44 smd rect (at -4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model ${KIPRJMOD}/3D/TQFP-44_10x10mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:USB_Micro-B_Molex-105017-0001 locked (layer F.Cu) (tedit 636FBEAD)
    (at 109.22 100.33 270)
    (descr http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf)
    (tags "Micro-USB SMD Typ-B")
    (attr smd)
    (fp_text reference J1 (at 4.699 -2.032) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at 0.3 3.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 1.8 270) (layer Dwgs.User))
    (pad 6 smd rect (at -2.9 0.35 270) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.9 0.35 270) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 3.5 0.35 270) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -3.5 0.35 90) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -1 0.35 270) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 2.5 -2.35 270) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 0.65 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.3 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.3 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(F1-Pad2)"))
    (pad 2 smd rect (at -0.65 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J1-Pad2)"))
    (pad 6 thru_hole circle (at -2.5 -2.35 270) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1 0.35 270) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/3D/USB_micro_105017-0001.stp
      (offset (xyz 0 0 1.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:C_0805 (layer F.Cu) (tedit 636FC0BD)
    (at 131.445 95.885 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.75 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model ${KIPRJMOD}/3D/C_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:M3mount (layer F.Cu) (tedit 636FC1C2)
    (at 167.64 80.01)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (fp_text reference P2 (at 0 -3.3) (layer F.SilkS) hide)
    (fp_text value M3 (at 0.1 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask))
  )
  (module footprints:M3mount (layer F.Cu) (tedit 636FC1C2)
    (at 110.49 123.19)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (fp_text reference P3 (at 0 -3.3) (layer F.SilkS) hide)
    (fp_text value M3 (at 0.1 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask))
  )
  (module footprints:M3mount (layer F.Cu) (tedit 636FC1C2)
    (at 167.64 123.19)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (fp_text reference P4 (at 0 -3.3) (layer F.SilkS) hide)
    (fp_text value M3 (at 0.1 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask))
  )
  (module footprints:MadeInOregonRev25 (layer F.Cu) (tedit 0)
    (at 124 118.11)
    (fp_text reference MadeInOregon1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value SYM_Arrow_Large (at 0 0) (layer F.SilkS) hide)
  )
  (module footprints:KiCad-Logo2_8mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 140 121.92 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference MadeWithKiCAD1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value SYM_Arrow_Large (at 0.75 0) (layer B.Fab) hide)
  )
  (module footprints:OSHW-Logo_11.4x12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 157.5 118.5 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference OSHW1 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value SYM_Arrow_Large (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module footprints:SAMTEC_MEC8-113-TOP-BOTTOM (layer F.Cu) (tedit 63786631)
    (at 119 88 90)
    (fp_text reference X1 (at -0.5 -5.75 90) (layer F.SilkS))
    (fp_text value MEC8-113 (at 8.21 6.135 90) (layer F.Fab))
    (pad 1 smd rect (at -6.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 7 /D10))
    (pad 14 smd rect (at -6.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 12 /A5))
    (pad 2 smd rect (at -5.6 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 /D9))
    (pad 15 smd rect (at -5.6 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 78 /A4))
    (pad 3 smd rect (at -4.8 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 4 /D8))
    (pad 16 smd rect (at -4.8 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 11 /A3))
    (pad 4 smd rect (at -4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 3 /D6))
    (pad 17 smd rect (at -4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 77 /A2))
    (pad 5 smd rect (at -3.2 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 6 /D12))
    (pad 18 smd rect (at -3.2 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 76 /A1))
    (pad 6 smd rect (at -2.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 /D4))
    (pad 19 smd rect (at -2.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 10 /A0))
    (pad 7 smd rect (at 1.6 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 74 /D1))
    (pad 20 smd rect (at 1.6 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 9 /D7))
    (pad 8 smd rect (at 2.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 15 /MISO))
    (pad 21 smd rect (at 2.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 5 /D13))
    (pad 9 smd rect (at 3.2 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 14 /MOSI))
    (pad 22 smd rect (at 3.2 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 16 /D5))
    (pad 10 smd rect (at 4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 13 /SCK))
    (pad 23 smd rect (at 4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 75 /D11))
    (pad None np_thru_hole circle (at -7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at 7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad 11 smd rect (at 4.8 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 19 /~RESET))
    (pad 24 smd rect (at 4.8 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 71 /D3_SCL))
    (pad 12 smd rect (at 5.6 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 25 smd rect (at 5.6 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 72 /D2_SDA))
    (pad 13 smd rect (at 6.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 26 smd rect (at 6.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/3D/mec8-113-02-l-d-ra1.stp
      (offset (xyz -8 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:SAMTEC_MEC8-113-TOP-BOTTOM (layer F.Cu) (tedit 63786631)
    (at 119 110 90)
    (fp_text reference X2 (at -0.5 -5.75 90) (layer F.SilkS))
    (fp_text value MEC8-113 (at 8.21 6.135 90) (layer F.Fab))
    (pad 26 smd rect (at 6.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 6.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 25 smd rect (at 5.6 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 72 /D2_SDA))
    (pad 12 smd rect (at 5.6 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 4.8 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 71 /D3_SCL))
    (pad 11 smd rect (at 4.8 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 19 /~RESET))
    (pad None np_thru_hole circle (at 7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at -7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad 23 smd rect (at 4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R20-Pad2)"))
    (pad 10 smd rect (at 4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R10-Pad2)"))
    (pad 22 smd rect (at 3.2 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R19-Pad2)"))
    (pad 9 smd rect (at 3.2 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R9-Pad2)"))
    (pad 21 smd rect (at 2.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R18-Pad2)"))
    (pad 8 smd rect (at 2.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R8-Pad2)"))
    (pad 20 smd rect (at 1.6 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R17-Pad2)"))
    (pad 7 smd rect (at 1.6 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R7-Pad2)"))
    (pad 19 smd rect (at -2.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R16-Pad2)"))
    (pad 6 smd rect (at -2.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R6-Pad2)"))
    (pad 18 smd rect (at -3.2 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R15-Pad2)"))
    (pad 5 smd rect (at -3.2 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R5-Pad2)"))
    (pad 17 smd rect (at -4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R14-Pad2)"))
    (pad 4 smd rect (at -4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R4-Pad2)"))
    (pad 16 smd rect (at -4.8 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R13-Pad2)"))
    (pad 3 smd rect (at -4.8 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R3-Pad2)"))
    (pad 15 smd rect (at -5.6 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R12-Pad2)"))
    (pad 2 smd rect (at -5.6 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R2-Pad2)"))
    (pad 14 smd rect (at -6.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R11-Pad2)"))
    (pad 1 smd rect (at -6.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R1-Pad2)"))
    (model ${KIPRJMOD}/3D/mec8-113-02-l-d-ra1.stp
      (offset (xyz -8 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 127 102.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 4K7 (at -2.5 -1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 /D3_SCL))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SW_TS10-63-26-BE-250-SMT-TR (layer F.Cu) (tedit 63700F76)
    (at 110 115 90)
    (fp_text reference SW2 (at 0.075 0 90) (layer F.SilkS))
    (fp_text value SCK (at 14.045 3.615 90) (layer F.Fab))
    (pad 1 smd rect (at -3.25 0 90) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 73 /D0))
    (pad 2 smd rect (at 3.25 0 90) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_FSMSM.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 157 103.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 -1.25) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Jumper (layer F.Cu) (tedit 5B6DD72B)
    (at 151.5 106.75 270)
    (attr smd)
    (fp_text reference JP1 (at 0 1.143 90) (layer F.SilkS) hide)
    (fp_text value JMP (at 0 1.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.2 90) (layer F.Fab))
    (pad 1 smd rect (at -0.3 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 2 smd rect (at 0.3 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 79 /Vin))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_1206 (layer F.Cu) (tedit 5B6DD6EF)
    (at 151.5 106.75 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R29 (at 0.127 1.651 90) (layer F.SilkS) hide)
    (fp_text value 0.1 (at 0 1.95 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 79 /Vin))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 157 107.5 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at 2.5 3.5) (layer F.SilkS) hide)
    (fp_text value INA219AxD (at 0 -3.25) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 /D2_SDA))
    (pad 4 smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 /D3_SCL))
    (pad 5 smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +5V))
    (pad 6 smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 /Vin))
    (pad 8 smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:MEC8-113-CARD_2outline locked (layer F.Cu) (tedit 637EA855)
    (at 116.459 120 90)
    (fp_text reference CardOutline1 (at 4.375 -1.25 90) (layer F.Fab))
    (fp_text value SYM_Arrow_Large (at 10.9 -1 90) (layer F.Fab))
  )
  (module footprints:MEC8-113-CARD_2outline locked (layer F.Cu) (tedit 637EA855)
    (at 116.5 98 90)
    (fp_text reference CardOutline2 (at 4.375 -1.25 90) (layer F.Fab))
    (fp_text value SYM_Arrow_Large (at 10.9 -1 90) (layer F.Fab))
  )
  (module footprints:Snake (layer B.Cu) (tedit 0)
    (at 140.1 92.1 180)
    (fp_text reference SnakeBack1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value SYM_Arrow_Large (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_text 0x40 (at 156.75 112) (layer F.SilkS))
  (gr_text "Keep It\nSimple\nStupid" (at 164.5 99.5) (layer B.Mask))
  (gr_text github.com/aspro648/RPB (at 140.5 107.5) (layer B.SilkS))
  (gr_text "Killroy was\nhere!" (at 133 114.5) (layer B.Cu))
  (gr_text "Don't get bit!" (at 181.25 118.25) (layer F.Mask))
  (gr_text M3 (at 161.75 84) (layer F.SilkS))
  (gr_text D13 (at 110 105.5) (layer F.SilkS))
  (gr_text D15 (at 110 119.75) (layer F.SilkS))
  (dimension 57.15 (width 0.15) (layer Dwgs.User)
    (gr_text "2.25 in" (at 139.065 130.84) (layer Dwgs.User))
    (feature1 (pts (xy 167.64 123.19) (xy 167.64 130.126421)))
    (feature2 (pts (xy 110.49 123.19) (xy 110.49 130.126421)))
    (crossbar (pts (xy 110.49 129.54) (xy 167.64 129.54)))
    (arrow1a (pts (xy 167.64 129.54) (xy 166.513496 130.126421)))
    (arrow1b (pts (xy 167.64 129.54) (xy 166.513496 128.953579)))
    (arrow2a (pts (xy 110.49 129.54) (xy 111.616504 130.126421)))
    (arrow2b (pts (xy 110.49 129.54) (xy 111.616504 128.953579)))
  )
  (dimension 43.18 (width 0.15) (layer Dwgs.User)
    (gr_text "1.70 in" (at 90.14 101.6 90) (layer Dwgs.User))
    (feature1 (pts (xy 110.49 80.01) (xy 90.853579 80.01)))
    (feature2 (pts (xy 110.49 123.19) (xy 90.853579 123.19)))
    (crossbar (pts (xy 91.44 123.19) (xy 91.44 80.01)))
    (arrow1a (pts (xy 91.44 80.01) (xy 92.026421 81.136504)))
    (arrow1b (pts (xy 91.44 80.01) (xy 90.853579 81.136504)))
    (arrow2a (pts (xy 91.44 123.19) (xy 92.026421 122.063496)))
    (arrow2b (pts (xy 91.44 123.19) (xy 90.853579 122.063496)))
  )
  (gr_text "Rapid Prototyping\nBoard" (at 142.5 115.25) (layer F.SilkS))
  (gr_text 648.ken@gmail.com (at 140.335 110) (layer B.SilkS))
  (gr_text M2.5 (at 158.115 92.075) (layer F.SilkS))
  (dimension 64.77 (width 0.15) (layer F.SilkS)
    (gr_text "2.55 in" (at 139.065 134.015) (layer F.SilkS))
    (feature1 (pts (xy 171.45 126.365) (xy 171.45 133.301421)))
    (feature2 (pts (xy 106.68 126.365) (xy 106.68 133.301421)))
    (crossbar (pts (xy 106.68 132.715) (xy 171.45 132.715)))
    (arrow1a (pts (xy 171.45 132.715) (xy 170.323496 133.301421)))
    (arrow1b (pts (xy 171.45 132.715) (xy 170.323496 132.128579)))
    (arrow2a (pts (xy 106.68 132.715) (xy 107.806504 133.301421)))
    (arrow2b (pts (xy 106.68 132.715) (xy 107.806504 132.128579)))
  )
  (gr_text "Rapid Prototyping Board" (at 139.7 104.14) (layer B.SilkS))
  (gr_text - (at 159.5 86) (layer F.SilkS))
  (gr_text + (at 159.5 80.5) (layer F.SilkS))
  (gr_arc (start 110.49 80.01) (end 110.49 76.2) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 110.49 123.19) (end 106.68 123.19) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.45 80.01) (end 171.45 123.19) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 167.64 80.01) (end 171.45 80.01) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 167.64 123.19) (end 167.64 127) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 76.2) (end 110.49 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.49 127) (end 167.64 127) (layer Edge.Cuts) (width 0.15))
  (dimension 50.8 (width 0.15) (layer F.SilkS)
    (gr_text "2.0 in" (at 99.03 101.6 -90) (layer F.SilkS))
    (feature1 (pts (xy 102.87 127) (xy 99.743579 127)))
    (feature2 (pts (xy 102.87 76.2) (xy 99.743579 76.2)))
    (crossbar (pts (xy 100.33 76.2) (xy 100.33 127)))
    (arrow1a (pts (xy 100.33 127) (xy 99.743579 125.873496)))
    (arrow1b (pts (xy 100.33 127) (xy 100.916421 125.873496)))
    (arrow2a (pts (xy 100.33 76.2) (xy 99.743579 77.326504)))
    (arrow2b (pts (xy 100.33 76.2) (xy 100.916421 77.326504)))
  )
  (gr_text "Rev 1.0\nNov 2022" (at 124.46 123.19) (layer B.SilkS))
  (gr_line (start 106.68 123.19) (end 106.68 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.958 127) (xy 106.68 127) (xy 106.68 76.2) (xy 171.958 75.946)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.466 127.762) (xy 105.664 127.762) (xy 106.172 75.438) (xy 105.918 75.438) (xy 172.72 75.184)
      )
    )
  )
)
