<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="95" x2="0" y2="15" width="0.1524" layer="20"/>
<wire x1="0" y1="15" x2="0.5" y2="14.5" width="0.1524" layer="20"/>
<wire x1="0.5" y1="14.5" x2="0.5" y2="6" width="0.1524" layer="20"/>
<wire x1="0.5" y1="6" x2="0" y2="5.5" width="0.1524" layer="20"/>
<wire x1="0" y1="5.5" x2="0" y2="5" width="0.1524" layer="20"/>
<wire x1="0" y1="5" x2="5" y2="0" width="0.1524" layer="20" curve="90"/>
<wire x1="5" y1="0" x2="19" y2="0" width="0.1524" layer="20"/>
<wire x1="19" y1="0" x2="24" y2="5" width="0.1524" layer="20" curve="90"/>
<wire x1="24" y1="5" x2="24" y2="7.8357875" width="0.1524" layer="20"/>
<wire x1="24" y1="7.8357875" x2="23.70710625" y2="8.54289375" width="0.1524" layer="20" curve="45"/>
<wire x1="23.70710625" y1="8.54289375" x2="23.29289375" y2="8.95710625" width="0.1524" layer="20"/>
<wire x1="23.29289375" y1="8.95710625" x2="23" y2="9.6642125" width="0.1524" layer="20" curve="-45"/>
<wire x1="23" y1="9.6642125" x2="23" y2="11.5857875" width="0.1524" layer="20"/>
<wire x1="23" y1="11.5857875" x2="23.29289375" y2="12.29289375" width="0.1524" layer="20" curve="-45"/>
<wire x1="23.29289375" y1="12.29289375" x2="23.70710625" y2="12.70710625" width="0.1524" layer="20"/>
<wire x1="23.70710625" y1="12.70710625" x2="24" y2="13.4142125" width="0.1524" layer="20" curve="45"/>
<wire x1="24" y1="13.4142125" x2="24" y2="18.0857875" width="0.1524" layer="20"/>
<wire x1="24" y1="18.0857875" x2="23.70710625" y2="18.79289375" width="0.1524" layer="20" curve="45"/>
<wire x1="23.70710625" y1="18.79289375" x2="23.54289375" y2="18.95710625" width="0.1524" layer="20"/>
<wire x1="23.54289375" y1="18.95710625" x2="23.25" y2="19.6642125" width="0.1524" layer="20" curve="-45"/>
<wire x1="23.25" y1="19.6642125" x2="23.25" y2="21.8357875" width="0.1524" layer="20"/>
<wire x1="23.25" y1="21.8357875" x2="23.54289375" y2="22.54289375" width="0.1524" layer="20" curve="-45"/>
<wire x1="23.54289375" y1="22.54289375" x2="23.70710625" y2="22.70710625" width="0.1524" layer="20"/>
<wire x1="23.70710625" y1="22.70710625" x2="24" y2="23.4142125" width="0.1524" layer="20" curve="45"/>
<wire x1="24" y1="23.4142125" x2="24" y2="95" width="0.1524" layer="20"/>
<wire x1="24" y1="95" x2="19" y2="100" width="0.1524" layer="20" curve="90"/>
<wire x1="19" y1="100" x2="5" y2="100" width="0.1524" layer="20"/>
<wire x1="5" y1="100" x2="0" y2="95" width="0.1524" layer="20" curve="90"/>
<text>GND</text>
<text>RST</text>
<text>TMS</text>
<text>TCLK</text>
<text>RX</text>
<text>TX</text>
<text>3.3V</text>
<text>5V</text>
<wire x1="5" y1="3.5" x2="6.5" y2="2" width="0.254" layer="20" curve="90"/>
<wire x1="6.5" y1="2" x2="17.5" y2="2" width="0.254" layer="20"/>
<wire x1="5" y1="3.5" x2="6.5" y2="5" width="0.254" layer="20" curve="-90"/>
<wire x1="6.5" y1="5" x2="17.5" y2="5" width="0.254" layer="20"/>
<wire x1="19" y1="3.5" x2="17.5" y2="2" width="0.254" layer="20" curve="-90"/>
<wire x1="19" y1="3.5" x2="17.5" y2="5" width="0.254" layer="20" curve="90"/>
<text>Blinky Pendant by BlinkinLabs</text>
<text>OE</text>
<text>STB</text>
<text>S0</text>
<text>CLK</text>
<text>S1</text>
<text>DATA</text>
<text>SDA</text>
<text>INT1</text>
<text>SCL</text>
<text>ON</text>
<text>OFF</text>
<text>Rev D
2015-05-05</text>
<text>D-</text>
<text>D+</text>
<text>VBAT</text>
<text>for more info:
blinkypendant.com</text>
</plain>
<libraries>
<library name="teensy_adapter">
<packages>
<package name="SMD-24-1MM">
</package>
<package name="VFDFN-10">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="blinkinlabs">
<description>Library of parts that we use for our Blinkinlabs designs. Some parts copied (and modified) from the excellent Sparkfun libraries.
</description>
<packages>
<package name="USB_MICRO_THRUHOLE">
</package>
<package name="CRYSTAL_3225">
</package>
<package name="QFN32_5X5_LONGLEADS">
</package>
<package name="CR2032X2">
</package>
<package name="BUTTON_MOMENTARY_MP5">
</package>
<package name="LED-TRICOLOR-5050-FIXED">
</package>
<package name="SWITCH_SMD_90_DEGREE">
</package>
</packages>
</library>
<library name="74xx-little-us">
<description>&lt;b&gt;Single and Dual Gates Family, US symbols&lt;/b&gt;&lt;p&gt;
Little logic devices from Texas Instruments&lt;br&gt;
TinyLogic(R) from FAIRCHILD Semiconductor TM
&lt;p&gt;
&lt;author&gt;Created by evgeni@eniks.com&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Extended by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SC70-5">
<description>&lt;b&gt;SMT SC70-5&lt;/b&gt;&lt;p&gt;
SOT353 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="zetex">
<description>&lt;b&gt;Zetex Power MOS FETs, Bridges, Diodes&lt;/b&gt;&lt;p&gt;
http://www.zetex.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U3" library="teensy_adapter" package="SMD-24-1MM" value="ICN2026DF"/>
<element name="C1" library="adafruit" package="C0402" value="100nF"/>
<element name="R1" library="adafruit" package="R0402" value="2000"/>
<element name="U2" library="teensy_adapter" package="VFDFN-10" value="MMA8653FC"/>
<element name="R2" library="adafruit" package="R0402" value="4.7k"/>
<element name="R3" library="adafruit" package="R0402" value="4.7k"/>
<element name="C2" library="adafruit" package="C0402" value="100nF"/>
<element name="C3" library="adafruit" package="C0402" value="100nF"/>
<element name="C4" library="adafruit" package="C0402" value="100nF"/>
<element name="D1" library="blinkinlabs" package="LED-TRICOLOR-5050-FIXED" value="LED-RGB5050">
<attribute name="VALUE"/>
</element>
<element name="D2" library="blinkinlabs" package="LED-TRICOLOR-5050-FIXED" value="LED-RGB5050">
<attribute name="VALUE"/>
</element>
<element name="D3" library="blinkinlabs" package="LED-TRICOLOR-5050-FIXED" value="LED-RGB5050">
<attribute name="VALUE"/>
</element>
<element name="D4" library="blinkinlabs" package="LED-TRICOLOR-5050-FIXED" value="LED-RGB5050">
<attribute name="VALUE"/>
</element>
<element name="D6" library="blinkinlabs" package="LED-TRICOLOR-5050-FIXED" value="LED-RGB5050">
<attribute name="VALUE"/>
</element>
<element name="D7" library="blinkinlabs" package="LED-TRICOLOR-5050-FIXED" value="LED-RGB5050">
<attribute name="VALUE"/>
</element>
<element name="D8" library="blinkinlabs" package="LED-TRICOLOR-5050-FIXED" value="LED-RGB5050">
<attribute name="VALUE"/>
</element>
<element name="D9" library="blinkinlabs" package="LED-TRICOLOR-5050-FIXED" value="LED-RGB5050">
<attribute name="VALUE"/>
</element>
<element name="C6" library="adafruit" package="C0402" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="R0402" value="33">
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="R0402" value="33">
<attribute name="VALUE"/>
</element>
<element name="CON1" library="blinkinlabs" package="USB_MICRO_THRUHOLE" value="USB_MICROSMT+THRUHULE">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="blinkinlabs" package="CRYSTAL_3225" value="16MHz">
<attribute name="VALUE"/>
</element>
<element name="C10" library="adafruit" package="C0402" value="2.2uF">
<attribute name="VALUE"/>
</element>
<element name="C5" library="adafruit" package="C0402" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="C8" library="adafruit" package="C0402" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="U1" library="blinkinlabs" package="QFN32_5X5_LONGLEADS" value="MK20D--VFM5">
<attribute name="VALUE"/>
</element>
<element name="C7" library="adafruit" package="C0402" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="C9" library="adafruit" package="C0603" value="10uF">
<attribute name="VALUE"/>
</element>
<element name="U5" library="74xx-little-us" package="SC70-5" value="74LVC1G17DCK">
<attribute name="VALUE"/>
</element>
<element name="U4" library="74xx-little-us" package="SC70-5" value="74LVC1G17DCK">
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="R0402" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="R0402" value="10k">
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP3" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP4" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP5" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP6" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP7" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP8" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP1" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="CON2" library="blinkinlabs" package="CR2032X2" value="CR2032X2"/>
<element name="T1" library="zetex" package="SOT-23" value="SSM3J328R,LF">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="T2" library="zetex" package="SOT-23" value="SSM3J328R,LF">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="blinkinlabs" package="BUTTON_MOMENTARY_MP5" value="SW2">
<attribute name="VALUE"/>
</element>
<element name="D5" library="blinkinlabs" package="LED-TRICOLOR-5050-FIXED" value="LED-RGB5050">
<attribute name="VALUE"/>
</element>
<element name="D10" library="blinkinlabs" package="LED-TRICOLOR-5050-FIXED" value="LED-RGB5050">
<attribute name="VALUE"/>
</element>
<element name="SW1" library="blinkinlabs" package="SWITCH_SMD_90_DEGREE" value="SWITCH_SPDT_SHIELD">
<attribute name="VALUE"/>
</element>
<element name="TP9" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP11" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP12" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP13" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP14" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP15" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP16" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP10" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP17" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP18" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP19" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP20" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP21" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP22" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP23" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP24" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP25" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP26" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP27" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP28" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP29" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP30" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP31" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP32" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP33" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP34" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP35" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP36" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP37" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
</elements>
<signals>
<signal name="S0">
<contactref element="D1" pad="4"/>
<contactref element="D2" pad="4"/>
<contactref element="D3" pad="4"/>
<contactref element="D4" pad="4"/>
<contactref element="T1" pad="1"/>
<contactref element="D5" pad="4"/>
<contactref element="D1" pad="5"/>
<contactref element="D1" pad="6"/>
<contactref element="D2" pad="5"/>
<contactref element="D2" pad="6"/>
<contactref element="D3" pad="5"/>
<contactref element="D3" pad="6"/>
<contactref element="D4" pad="5"/>
<contactref element="D4" pad="6"/>
<contactref element="D5" pad="5"/>
<contactref element="D5" pad="6"/>
<contactref element="TP33" pad="TP"/>
</signal>
<signal name="S1">
<contactref element="D6" pad="4"/>
<contactref element="D7" pad="4"/>
<contactref element="D8" pad="4"/>
<contactref element="D9" pad="4"/>
<contactref element="T2" pad="1"/>
<contactref element="D10" pad="4"/>
<contactref element="D6" pad="5"/>
<contactref element="D6" pad="6"/>
<contactref element="D7" pad="5"/>
<contactref element="D7" pad="6"/>
<contactref element="D8" pad="5"/>
<contactref element="D8" pad="6"/>
<contactref element="D9" pad="5"/>
<contactref element="D9" pad="6"/>
<contactref element="D10" pad="5"/>
<contactref element="D10" pad="6"/>
<contactref element="TP34" pad="TP"/>
</signal>
<signal name="R0">
<contactref element="D1" pad="2"/>
<contactref element="D6" pad="2"/>
<contactref element="U3" pad="5"/>
<contactref element="TP18" pad="TP"/>
</signal>
<signal name="R1">
<contactref element="D2" pad="2"/>
<contactref element="D7" pad="2"/>
<contactref element="U3" pad="8"/>
<contactref element="TP21" pad="TP"/>
</signal>
<signal name="R2">
<contactref element="D3" pad="2"/>
<contactref element="D8" pad="2"/>
<contactref element="U3" pad="11"/>
<contactref element="TP24" pad="TP"/>
</signal>
<signal name="R3">
<contactref element="D4" pad="2"/>
<contactref element="D9" pad="2"/>
<contactref element="U3" pad="14"/>
<contactref element="TP27" pad="TP"/>
</signal>
<signal name="B4">
<contactref element="U3" pad="19"/>
<contactref element="D5" pad="1"/>
<contactref element="D10" pad="1"/>
<contactref element="TP32" pad="TP"/>
</signal>
<signal name="G4">
<contactref element="U3" pad="18"/>
<contactref element="D5" pad="3"/>
<contactref element="D10" pad="3"/>
<contactref element="TP31" pad="TP"/>
</signal>
<signal name="B3">
<contactref element="D4" pad="1"/>
<contactref element="D9" pad="1"/>
<contactref element="U3" pad="16"/>
<contactref element="TP29" pad="TP"/>
</signal>
<signal name="G3">
<contactref element="D4" pad="3"/>
<contactref element="D9" pad="3"/>
<contactref element="U3" pad="15"/>
<contactref element="TP28" pad="TP"/>
</signal>
<signal name="G1">
<contactref element="D2" pad="3"/>
<contactref element="D7" pad="3"/>
<contactref element="U3" pad="9"/>
<contactref element="TP22" pad="TP"/>
</signal>
<signal name="B1">
<contactref element="D2" pad="1"/>
<contactref element="D7" pad="1"/>
<contactref element="U3" pad="10"/>
<contactref element="TP23" pad="TP"/>
</signal>
<signal name="G2">
<contactref element="D3" pad="3"/>
<contactref element="D8" pad="3"/>
<contactref element="U3" pad="12"/>
<contactref element="TP26" pad="TP"/>
</signal>
<signal name="B2">
<contactref element="D3" pad="1"/>
<contactref element="D8" pad="1"/>
<contactref element="U3" pad="13"/>
<contactref element="TP25" pad="TP"/>
</signal>
<signal name="G0">
<contactref element="D1" pad="3"/>
<contactref element="D6" pad="3"/>
<contactref element="U3" pad="6"/>
<contactref element="TP19" pad="TP"/>
</signal>
<signal name="B0">
<contactref element="D1" pad="1"/>
<contactref element="D6" pad="1"/>
<contactref element="U3" pad="7"/>
<contactref element="TP20" pad="TP"/>
</signal>
<signal name="GND">
<contactref element="U3" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="P$6"/>
<contactref element="U2" pad="P$7"/>
<contactref element="U2" pad="P$9"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="CON1" pad="PIN$5"/>
<contactref element="C10" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="Q1" pad="P$2"/>
<contactref element="Q1" pad="P$4"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="PAD@9"/>
<contactref element="U1" pad="PAD@4"/>
<contactref element="U1" pad="PAD@1"/>
<contactref element="U1" pad="PAD@11"/>
<contactref element="U1" pad="8"/>
<contactref element="C9" pad="2"/>
<contactref element="U5" pad="3"/>
<contactref element="U4" pad="3"/>
<contactref element="TP5" pad="TP"/>
<contactref element="CON2" pad="-"/>
<contactref element="SW2" pad="SHEILD_1"/>
<contactref element="SW1" pad="SHIELD_1"/>
<contactref element="SW1" pad="SHIELD_3"/>
<contactref element="SW1" pad="SHIELD_2"/>
<contactref element="SW1" pad="SHIELD_4"/>
<contactref element="SW2" pad="1"/>
<contactref element="SW2" pad="SHEILD_2"/>
<contactref element="SW2" pad="SHEILD_3"/>
<contactref element="SW2" pad="SHEILD_4"/>
<contactref element="CON1" pad="PAD$5"/>
<contactref element="CON1" pad="PAD$8"/>
<contactref element="CON1" pad="PAD$3"/>
<contactref element="CON1" pad="PAD$2"/>
<contactref element="CON1" pad="PAD$4"/>
<contactref element="CON1" pad="PAD$9"/>
<contactref element="CON1" pad="PAD$1"/>
<contactref element="CON1" pad="PAD$6"/>
<contactref element="CON1" pad="PAD$7"/>
<contactref element="CON1" pad="PAD$10"/>
</signal>
<signal name="LED_OE">
<contactref element="U3" pad="21"/>
<contactref element="U1" pad="16"/>
<contactref element="TP16" pad="TP"/>
</signal>
<signal name="N$18">
<contactref element="U3" pad="23"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="U2" pad="P$8"/>
<contactref element="U2" pad="P$1"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U3" pad="24"/>
<contactref element="C1" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="11"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="C7" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="P$4"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="ACC_INT1">
<contactref element="U1" pad="24"/>
<contactref element="U2" pad="P$3"/>
<contactref element="TP17" pad="TP"/>
</signal>
<signal name="+5V">
<contactref element="U1" pad="6"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="U5" pad="5"/>
<contactref element="U4" pad="5"/>
<contactref element="CON1" pad="PIN$1"/>
<contactref element="TP6" pad="TP"/>
<contactref element="T2" pad="2"/>
<contactref element="T1" pad="2"/>
<contactref element="SW1" pad="L1"/>
</signal>
<signal name="I2C0_SCL">
<contactref element="U2" pad="P$2"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="20"/>
<contactref element="TP9" pad="TP"/>
</signal>
<signal name="I2C0_SDA">
<contactref element="U2" pad="P$10"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="21"/>
<contactref element="TP10" pad="TP"/>
</signal>
<signal name="N$8">
<contactref element="Q1" pad="P$3"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$13">
<contactref element="Q1" pad="P$1"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="N$14">
<contactref element="R7" pad="1"/>
<contactref element="CON1" pad="PIN$3"/>
<contactref element="TP36" pad="TP"/>
</signal>
<signal name="N$15">
<contactref element="R6" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$17">
<contactref element="R7" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="TCLK">
<contactref element="U1" pad="12"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="TMS">
<contactref element="U1" pad="15"/>
<contactref element="TP8" pad="TP"/>
<contactref element="SW2" pad="2"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="13"/>
<contactref element="TP7" pad="TP"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="14"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="19"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="N$21">
<contactref element="R6" pad="1"/>
<contactref element="CON1" pad="PIN$2"/>
<contactref element="TP35" pad="TP"/>
</signal>
<signal name="LED_DATA">
<contactref element="U3" pad="2"/>
<contactref element="U1" pad="27"/>
<contactref element="TP12" pad="TP"/>
</signal>
<signal name="LED_CLOCK">
<contactref element="U3" pad="3"/>
<contactref element="U1" pad="26"/>
<contactref element="TP11" pad="TP"/>
</signal>
<signal name="LED_STROBE">
<contactref element="U3" pad="4"/>
<contactref element="U1" pad="31"/>
<contactref element="TP15" pad="TP"/>
</signal>
<signal name="LED_S0">
<contactref element="U1" pad="29"/>
<contactref element="U4" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="TP13" pad="TP"/>
</signal>
<signal name="LED_S1">
<contactref element="U1" pad="30"/>
<contactref element="U5" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="TP14" pad="TP"/>
</signal>
<signal name="N$6">
<contactref element="U4" pad="4"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="U5" pad="4"/>
<contactref element="T2" pad="3"/>
</signal>
<signal name="R4">
<contactref element="U3" pad="17"/>
<contactref element="D5" pad="2"/>
<contactref element="D10" pad="2"/>
<contactref element="TP30" pad="TP"/>
</signal>
<signal name="VBAT">
<contactref element="CON2" pad="+"/>
<contactref element="SW1" pad="COM"/>
<contactref element="TP37" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
