(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" jumper)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "CTR")
  (net 2 "SHLD")
  (footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount" (layer "F.Cu")
    (tedit 5A1C1810)
    (at 149.86 76.2)
    (descr "http://www.amphenolrf.com/132289.html")
    (tags "SMA")
    (property "Sheetfile" "SMA_TestClips.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at -0.762 -1.524 180) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial" (at 5 6) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 4.79 0 270) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "CTR") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "SHLD") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "SHLD") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 90) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "SHLD") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 90) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "SHLD") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 152.654 69.85) (end 133.35 82.55) (layer "Edge.Cuts") (width 0.1) (fill none))
  (zone (net 2) (net_name "SHLD") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.146 73.914)
        (xy 147.32 73.914)
        (xy 147.32 70.104)
        (xy 152.146 70.104)
      )
    )
  )
  (zone (net 2) (net_name "SHLD") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.146 82.296)
        (xy 133.604 82.296)
        (xy 133.604 76.454)
        (xy 145.034 76.454)
        (xy 145.034 77.978)
        (xy 152.146 77.978)
      )
    )
  )
  (zone (net 1) (net_name "CTR") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.558 75.184)
        (xy 152.146 75.184)
        (xy 152.146 77.216)
        (xy 145.542 77.216)
        (xy 145.542 75.946)
        (xy 133.604 75.946)
        (xy 133.604 70.104)
        (xy 146.558 70.104)
      )
    )
  )
  (zone (net 2) (net_name "SHLD") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.146 82.296)
        (xy 147.32 82.296)
        (xy 147.32 77.978)
        (xy 152.146 77.978)
      )
    )
  )
  (zone (net 2) (net_name "SHLD") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.146 73.914)
        (xy 147.32 73.914)
        (xy 147.32 70.104)
        (xy 152.146 70.104)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Mask") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.812 74.422)
        (xy 133.858 74.422)
        (xy 133.858 70.358)
        (xy 146.812 70.358)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Mask") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.558 82.296)
        (xy 133.604 82.296)
        (xy 133.604 77.978)
        (xy 146.558 77.978)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Mask") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.812 77.47)
        (xy 133.858 77.47)
        (xy 133.858 74.93)
        (xy 146.812 74.93)
      )
    )
  )
)
