(kicad_pcb (version 20171130) (host pcbnew 5.0.0-fee4fd1~66~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 111)
    (tracks 451)
    (zones 0)
    (modules 43)
    (nets 63)
  )
  (page A4)
  (title_block
    (rev 1.3)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.19812)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.508 0.762)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 +12V)
  (net 4 /~RESET~)
  (net 5 /~ISP~)
  (net 6 /TXD0)
  (net 7 /RXD0)
  (net 8 "Net-(U1-Pad1)")
  (net 9 "Net-(U1-Pad2)")
  (net 10 /TXE0)
  (net 11 /TXE1)
  (net 12 /RXD1)
  (net 13 /TXD1)
  (net 14 "Net-(U1-Pad45)")
  (net 15 "Net-(U1-Pad46)")
  (net 16 "Net-(U1-Pad4)")
  (net 17 "Net-(U1-Pad15)")
  (net 18 "Net-(U1-Pad19)")
  (net 19 "Net-(U1-Pad20)")
  (net 20 "Net-(U1-Pad21)")
  (net 21 "Net-(U1-Pad33)")
  (net 22 "Net-(U1-Pad42)")
  (net 23 /PORT1A)
  (net 24 /PORT1B)
  (net 25 /PORT0B)
  (net 26 /PORT0A)
  (net 27 /SDA)
  (net 28 /SCL)
  (net 29 /PIO0_27)
  (net 30 /PIO0_28)
  (net 31 /PIO0_29)
  (net 32 "Net-(R10-Pad2)")
  (net 33 "Net-(R11-Pad2)")
  (net 34 "Net-(R12-Pad2)")
  (net 35 "Net-(R13-Pad2)")
  (net 36 /PIO0_20)
  (net 37 /PIO0_21)
  (net 38 /PIO0_22)
  (net 39 /PIO0_23)
  (net 40 /PIO0_24)
  (net 41 /PIO0_25)
  (net 42 /PIO0_26)
  (net 43 /A7)
  (net 44 /A6)
  (net 45 /A5)
  (net 46 /A4)
  (net 47 /MOSI)
  (net 48 /MISO)
  (net 49 /SSEL)
  (net 50 /SCK)
  (net 51 "Net-(Q31-Pad1)")
  (net 52 "Net-(Q32-Pad1)")
  (net 53 /DRV1)
  (net 54 /DRV2)
  (net 55 "Net-(D1-Pad2)")
  (net 56 /A0)
  (net 57 /A1)
  (net 58 /A2)
  (net 59 /A3)
  (net 60 "Net-(R16-Pad2)")
  (net 61 "Net-(R17-Pad2)")
  (net 62 "Net-(R18-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /DRV1)
    (add_net /DRV2)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /PIO0_20)
    (add_net /PIO0_21)
    (add_net /PIO0_22)
    (add_net /PIO0_23)
    (add_net /PIO0_24)
    (add_net /PIO0_25)
    (add_net /PIO0_26)
    (add_net /PIO0_27)
    (add_net /PIO0_28)
    (add_net /PIO0_29)
    (add_net /PORT0A)
    (add_net /PORT0B)
    (add_net /PORT1A)
    (add_net /PORT1B)
    (add_net /RXD0)
    (add_net /RXD1)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SSEL)
    (add_net /TXD0)
    (add_net /TXD1)
    (add_net /TXE0)
    (add_net /TXE1)
    (add_net /~ISP~)
    (add_net /~RESET~)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(Q31-Pad1)")
    (add_net "Net-(Q32-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad46)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical locked (layer F.Cu) (tedit 5BBD5BEA)
    (at 114.554 148.463 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x05 (at 0 12.49 180) (layer F.Fab))
    (fp_text user %R (at 0 5.08 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 43 /A7))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 /A6))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 /A5))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 46 /A4))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 59 /A3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x15_P2.54mm_Vertical locked (layer F.Cu) (tedit 5BBD5B5C)
    (at 114.554 151.003 90)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x15 (at 0 37.89 90) (layer F.Fab))
    (fp_text user %R (at 0 17.78 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 /PIO0_20))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 /PIO0_21))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 /PIO0_22))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 39 /PIO0_23))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 40 /PIO0_24))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 41 /PIO0_25))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 42 /PIO0_26))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 /PIO0_27))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 /PIO0_28))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 /PIO0_29))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 /PORT0B))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 /PORT0A))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x15_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x15_P2.54mm_Vertical locked (layer F.Cu) (tedit 5BBD59EA)
    (at 114.554 135.763 90)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x15 (at 0 37.89 90) (layer F.Fab))
    (fp_text user %R (at 0 17.78 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 58 /A2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 57 /A1))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 56 /A0))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 /SCL))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 /SDA))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 /~RESET~))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /~ISP~))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 /RXD0))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /TXD0))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 /PORT1B))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 /PORT1A))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 /DRV1))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1.1) (layers *.Cu *.Mask)
      (net 54 /DRV2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x15_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5B9D2FA9)
    (at 134.112 146.177)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at -4.318 -0.381) (layer F.SilkS))
    (fp_text value ISL83483 (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /RXD0))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /TXE0))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /TXE0))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /TXD0))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /PORT0A))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /PORT0B))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B9D3009)
    (at 138.684 140.335 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 2.159 -0.127) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B9D63BA)
    (at 117.602 144.921 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at -2.046 0) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B9D2EE6)
    (at 138.684 146.05 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 2.0955 0) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer B.Cu) (tedit 5B9D6302)
    (at 149.1885 147.066 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C5 (at 3.048 0.127) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.28 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B9D635B)
    (at 149.2885 148.0185 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C6 (at -1.4605 1.27) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B9D633B)
    (at 145.8595 148.0185)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C7 (at -1.524 -1.2065 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 133.477 139.827)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -2.032 0) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 /PORT1B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 136.906 140.589 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 2.159 0 90) (layer B.SilkS))
    (fp_text value 120 (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /PORT1A))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 /PORT1B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 133.477 141.351 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 2.032 0 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /PORT1A))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 133.477 145.669)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -2.159 0.127) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 /PORT0B))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 136.906 146.431 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 2.159 0 90) (layer B.SilkS))
    (fp_text value 120 (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 /PORT0B))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 /PORT0A))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 133.463 147.193 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 2.145 0 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 /PORT0A))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:LQFP-48_7x7mm_P0.5mm (layer F.Cu) (tedit 5B9D6092)
    (at 123.952 143.51 90)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U1 (at 4.826 -3.81 180) (layer F.SilkS))
    (fp_text value LPC1225 (at 0 6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -4.35 -2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -4.35 -1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.35 -1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -4.35 -0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 /PIO0_20))
    (pad 6 smd rect (at -4.35 -0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 /PIO0_21))
    (pad 7 smd rect (at -4.35 0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 /PIO0_22))
    (pad 8 smd rect (at -4.35 0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 /PIO0_23))
    (pad 9 smd rect (at -4.35 1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 /PIO0_24))
    (pad 10 smd rect (at -4.35 1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 /PIO0_25))
    (pad 11 smd rect (at -4.35 2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 /PIO0_26))
    (pad 12 smd rect (at -4.35 2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /PIO0_27))
    (pad 13 smd rect (at -2.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 /PIO0_28))
    (pad 14 smd rect (at -2.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 /PIO0_29))
    (pad 15 smd rect (at -1.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at -1.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /RXD0))
    (pad 17 smd rect (at -0.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 /TXD0))
    (pad 18 smd rect (at -0.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /TXE0))
    (pad 19 smd rect (at 0.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 0.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 1.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 1.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /TXE1))
    (pad 23 smd rect (at 2.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /RXD1))
    (pad 24 smd rect (at 2.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /TXD1))
    (pad 25 smd rect (at 4.35 2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /SCL))
    (pad 26 smd rect (at 4.35 2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /SDA))
    (pad 27 smd rect (at 4.35 1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /~ISP~))
    (pad 28 smd rect (at 4.35 1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /~RESET~))
    (pad 29 smd rect (at 4.35 0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 /SCK))
    (pad 30 smd rect (at 4.35 0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 /SSEL))
    (pad 31 smd rect (at 4.35 -0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 /MISO))
    (pad 32 smd rect (at 4.35 -0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 /MOSI))
    (pad 33 smd rect (at 4.35 -1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad33)"))
    (pad 34 smd rect (at 4.35 -1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /A0))
    (pad 35 smd rect (at 4.35 -2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R18-Pad2)"))
    (pad 36 smd rect (at 4.35 -2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R17-Pad2)"))
    (pad 37 smd rect (at 2.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R16-Pad2)"))
    (pad 38 smd rect (at 2.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R13-Pad2)"))
    (pad 39 smd rect (at 1.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R12-Pad2)"))
    (pad 40 smd rect (at 1.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R11-Pad2)"))
    (pad 41 smd rect (at 0.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R10-Pad2)"))
    (pad 42 smd rect (at 0.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad42)"))
    (pad 43 smd rect (at -0.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 44 smd rect (at -0.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 45 smd rect (at -1.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad45)"))
    (pad 46 smd rect (at -1.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad46)"))
    (pad 47 smd rect (at -2.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 48 smd rect (at -2.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-48_7x7mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-89-3_Handsoldering (layer F.Cu) (tedit 5B9D631D)
    (at 147.447 143.7525 90)
    (descr "SOT-89-3 Handsoldering")
    (tags "SOT-89-3 Handsoldering")
    (attr smd)
    (fp_text reference U4 (at 2.921 1.905 90) (layer F.SilkS))
    (fp_text value AP7381-33Y (at 0.5 3.15 90) (layer F.Fab))
    (fp_text user %R (at 0.38 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.98 -1.5) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -1.98 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.98 1.5) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +12V))
    (pad 2 smd rect (at 1.98 0) (size 2 4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd trapezoid (at -0.37 0 180) (size 1.5 0.75) (rect_delta 0 0.5 ) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5B9D2FC5)
    (at 134.112 140.589)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at -4.191 -0.381) (layer F.SilkS))
    (fp_text value ISL83483 (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /PORT1B))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /PORT1A))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /TXD1))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /TXE1))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /TXE1))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /RXD1))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 129.286 140.97 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 2.032 0 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 /SCL))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 129.286 139.446 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 2.032 0 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 /SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B9D8502)
    (at 118.364 146.685)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 2.286 0) (layer B.SilkS))
    (fp_text value 4.7K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 /A7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B9D84E6)
    (at 118.364 145.2245)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 2.286 0) (layer B.SilkS))
    (fp_text value 12K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(R11-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 /A6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B9D84F2)
    (at 118.364 143.764)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 2.286 0) (layer B.SilkS))
    (fp_text value 27K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 /A5))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B9D84B1)
    (at 118.364 142.2908)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at 2.286 0) (layer B.SilkS))
    (fp_text value 47K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(R13-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 /A4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 123.952 146.685)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at 2.286 0) (layer B.SilkS))
    (fp_text value 3.3K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 123.952 145.2245)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R21 (at 2.286 0) (layer B.SilkS))
    (fp_text value 3.3K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 123.952 143.764)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R22 (at 2.286 0) (layer B.SilkS))
    (fp_text value 3.3K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(R12-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 123.952 142.2908)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R23 (at 2.286 0.0127) (layer B.SilkS))
    (fp_text value 3.3K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 146.3675 141.7955)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R31 (at -0.0635 1.2065) (layer B.SilkS))
    (fp_text value 120 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(Q31-Pad1)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 30 /PIO0_28))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 149.9235 141.7955)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R32 (at -0.127 1.2065) (layer B.SilkS))
    (fp_text value 120 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 31 /PIO0_29))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(Q32-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 149.9235 139.319 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q32 (at 1.143 -1.397 180) (layer B.SilkS))
    (fp_text value 2N7002 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(Q32-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 54 /DRV2))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 146.3675 139.319 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q31 (at 1.0795 -1.397 180) (layer B.SilkS))
    (fp_text value 2N7002 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(Q31-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 53 /DRV1))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5BAA0BF8)
    (at 129.286 137.922 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 2.032 0 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 /~RESET~))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5BAA0BE0)
    (at 132.588 137.922)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at 2.286 0.381) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /~ISP~))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5BBCD056)
    (at 129.4905 147.574 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 2.018 0.1905 180) (layer B.SilkS))
    (fp_text value LED_ALT (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5BBCD064)
    (at 129.4905 149.0345)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at -2.3 -0.4445) (layer B.SilkS))
    (fp_text value 330 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(D1-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 29 /PIO0_27))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 118.364 140.843)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at 2.286 0) (layer B.SilkS))
    (fp_text value 47K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 /A3))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 118.364 139.3825)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at 2.286 0) (layer B.SilkS))
    (fp_text value 47K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 58 /A2))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 118.364 137.922)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R18 (at 2.286 0) (layer B.SilkS))
    (fp_text value 47K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(R18-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 57 /A1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 123.952 140.843)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R24 (at 2.286 0) (layer B.SilkS))
    (fp_text value 3.3K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 123.952 139.3825)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R25 (at 2.286 0) (layer B.SilkS))
    (fp_text value 3.3K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 123.952 137.922)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R26 (at 2.2225 0) (layer B.SilkS))
    (fp_text value 3.3K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(R18-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Copyright (C) 2018 John Winans" (at 142.8496 143.7132 90) (layer F.SilkS))
  (gr_text "2037-44-RS485-Gateway rev 1.3" (at 141.9352 143.4084 90) (layer F.SilkS))
  (gr_text "SCINI 44+" (at 140.5636 143.256 90) (layer F.SilkS))
  (gr_text A0 (at 122.174 137.287) (layer B.SilkS))
  (gr_text A1 (at 119.634 137.287) (layer B.SilkS))
  (gr_text A2 (at 117.094 137.287) (layer B.SilkS))
  (gr_text A0 (at 122.174 137.668) (layer F.SilkS))
  (gr_text A1 (at 119.634 137.668) (layer F.SilkS))
  (gr_text A2 (at 117.094 137.668) (layer F.SilkS))
  (gr_text A3 (at 116.459 138.557 90) (layer F.SilkS))
  (gr_text A3 (at 116.078 138.303 90) (layer B.SilkS))
  (gr_text 2 (at 144.399 140.0175) (layer B.SilkS))
  (gr_text 1 (at 144.399 142.0495) (layer B.SilkS))
  (gr_text DRV1 (at 147.574 137.287) (layer B.SilkS))
  (gr_text DRV2 (at 150.114 137.287) (layer B.SilkS))
  (gr_text DRV2 (at 150.114 137.668) (layer F.SilkS))
  (gr_text DRV1 (at 147.574 137.668) (layer F.SilkS))
  (gr_text GND (at 145.0975 137.668) (layer F.SilkS))
  (gr_text GND (at 145.0975 137.287) (layer B.SilkS))
  (gr_text "SCINI 44+" (at 140.335 143.256 90) (layer B.SilkS))
  (gr_text 020 (at 114.554 149.733) (layer B.SilkS))
  (gr_text +V (at 150.114 149.606) (layer B.SilkS))
  (gr_text GND (at 147.574 149.606) (layer B.SilkS))
  (gr_text 3V3 (at 145.034 149.54909) (layer B.SilkS))
  (gr_text 0A (at 142.494 149.606) (layer B.SilkS))
  (gr_text 0B (at 139.954 149.606) (layer B.SilkS))
  (gr_text 029 (at 137.414 149.606) (layer B.SilkS))
  (gr_text 028 (at 134.874 149.606) (layer B.SilkS))
  (gr_text 027 (at 132.334 149.606) (layer B.SilkS))
  (gr_text 026 (at 129.794 149.606) (layer B.SilkS))
  (gr_text 025 (at 127.254 149.606) (layer B.SilkS))
  (gr_text 024 (at 124.714 149.606) (layer B.SilkS))
  (gr_text 023 (at 122.174 149.606) (layer B.SilkS))
  (gr_text 022 (at 119.634 149.606) (layer B.SilkS))
  (gr_text 021 (at 117.094 149.606) (layer B.SilkS))
  (gr_text GND (at 114.6175 137.0965) (layer B.SilkS))
  (gr_text A4 (at 116.078 140.843 90) (layer B.SilkS))
  (gr_text A5 (at 116.078 143.383 90) (layer B.SilkS))
  (gr_text A6 (at 116.078 145.923 90) (layer B.SilkS))
  (gr_text A7 (at 116.078 148.463 90) (layer B.SilkS))
  (gr_text 1A (at 142.494 137.287) (layer B.SilkS))
  (gr_text 1B (at 140.081 137.287) (layer B.SilkS))
  (gr_text +V (at 150.241 149.225) (layer F.SilkS))
  (gr_text 021 (at 117.348 149.225) (layer F.SilkS))
  (gr_text 022 (at 119.634 149.225) (layer F.SilkS))
  (gr_text 023 (at 122.174 149.225) (layer F.SilkS))
  (gr_text 024 (at 124.714 149.225) (layer F.SilkS))
  (gr_text 025 (at 127.254 149.225) (layer F.SilkS))
  (gr_text 026 (at 129.794 149.225) (layer F.SilkS))
  (gr_text 027 (at 132.334 149.1615) (layer F.SilkS))
  (gr_text 028 (at 134.874 149.1615) (layer F.SilkS))
  (gr_text 029 (at 137.414 149.1615) (layer F.SilkS))
  (gr_text 0B (at 139.954 149.1615) (layer F.SilkS))
  (gr_text 0A (at 142.494 149.1615) (layer F.SilkS))
  (gr_text 3V3 (at 145.034 149.225) (layer F.SilkS))
  (gr_text A4 (at 116.459 140.843 90) (layer F.SilkS))
  (gr_text RX (at 134.874 137.287) (layer B.SilkS))
  (gr_text TX (at 137.414 137.287) (layer B.SilkS))
  (gr_text ISP (at 132.207 137.287) (layer B.SilkS))
  (gr_text Reset (at 129.794 137.287) (layer B.SilkS))
  (gr_text SDA (at 127.254 137.287) (layer B.SilkS))
  (gr_text SCL (at 124.714 137.287) (layer B.SilkS))
  (dimension 15.24 (width 0.3) (layer Dwgs.User)
    (gr_text "0.6000 in" (at 104.961 143.383 270) (layer Dwgs.User))
    (feature1 (pts (xy 114.554 151.003) (xy 106.474579 151.003)))
    (feature2 (pts (xy 114.554 135.763) (xy 106.474579 135.763)))
    (crossbar (pts (xy 107.061 135.763) (xy 107.061 151.003)))
    (arrow1a (pts (xy 107.061 151.003) (xy 106.474579 149.876496)))
    (arrow1b (pts (xy 107.061 151.003) (xy 107.647421 149.876496)))
    (arrow2a (pts (xy 107.061 135.763) (xy 106.474579 136.889504)))
    (arrow2b (pts (xy 107.061 135.763) (xy 107.647421 136.889504)))
  )
  (gr_text SCL (at 124.714 137.668) (layer F.SilkS))
  (gr_text SDA (at 127.254 137.668) (layer F.SilkS))
  (gr_text GND (at 147.574 149.225) (layer F.SilkS))
  (gr_text GND (at 114.6175 137.0965) (layer F.SilkS))
  (gr_text A7 (at 116.586 148.463 90) (layer F.SilkS))
  (gr_text A6 (at 116.459 145.923 90) (layer F.SilkS))
  (gr_text A5 (at 116.459 143.383 90) (layer F.SilkS))
  (gr_text "Copyright (C) 2018 John Winans" (at 142.748 143.002 90) (layer B.SilkS))
  (gr_text "2037-44-RS485-Gateway rev 1.3" (at 141.859 143.3195 90) (layer B.SilkS))
  (gr_text Reset (at 129.794 137.668) (layer F.SilkS))
  (gr_text ISP (at 132.334 137.668) (layer F.SilkS))
  (gr_text TX (at 137.414 137.668) (layer F.SilkS))
  (gr_text RX (at 134.874 137.668) (layer F.SilkS))
  (gr_text 1A (at 142.494 137.668) (layer F.SilkS))
  (gr_text 1B (at 139.954 137.668) (layer F.SilkS))
  (gr_line (start 113.03 152.4) (end 151.892 152.4) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 113.03 134.366) (end 113.03 152.4) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 151.892 134.366) (end 113.03 134.366) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 151.892 152.4) (end 151.892 134.366) (layer Edge.Cuts) (width 0.254))
  (dimension 18.034 (width 0.3) (layer Dwgs.User)
    (gr_text "0.7100 in" (at 156.532 143.383 90) (layer Dwgs.User))
    (feature1 (pts (xy 151.892 134.366) (xy 155.018421 134.366)))
    (feature2 (pts (xy 151.892 152.4) (xy 155.018421 152.4)))
    (crossbar (pts (xy 154.432 152.4) (xy 154.432 134.366)))
    (arrow1a (pts (xy 154.432 134.366) (xy 155.018421 135.492504)))
    (arrow1b (pts (xy 154.432 134.366) (xy 153.845579 135.492504)))
    (arrow2a (pts (xy 154.432 152.4) (xy 155.018421 151.273496)))
    (arrow2b (pts (xy 154.432 152.4) (xy 153.845579 151.273496)))
  )
  (dimension 38.862 (width 0.3) (layer Dwgs.User)
    (gr_text "1.5300 in" (at 132.461 157.03028) (layer Dwgs.User))
    (feature1 (pts (xy 113.03 152.4) (xy 113.03 155.516701)))
    (feature2 (pts (xy 151.892 152.4) (xy 151.892 155.516701)))
    (crossbar (pts (xy 151.892 154.93028) (xy 113.03 154.93028)))
    (arrow1a (pts (xy 113.03 154.93028) (xy 114.156504 154.343859)))
    (arrow1b (pts (xy 113.03 154.93028) (xy 114.156504 155.516701)))
    (arrow2a (pts (xy 151.892 154.93028) (xy 150.765496 154.343859)))
    (arrow2b (pts (xy 151.892 154.93028) (xy 150.765496 155.516701)))
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.19812))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.19812) (thermal_bridge_width 1.016))
    (polygon
      (pts
        (xy 113.03 134.62) (xy 151.892 134.62) (xy 151.892 152.4) (xy 113.03 152.4)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.19812))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.19812) (thermal_bridge_width 1.016))
    (polygon
      (pts
        (xy 113.03 134.366) (xy 151.892 134.366) (xy 151.892 152.4) (xy 113.03 152.4)
      )
    )
  )
)
