(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-2")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 57)
    (zones 0)
    (modules 16)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.6)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.75 1.75)
    (pad_drill 0.8001)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 99.71786 112.34166)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(N1-Pad8)")
  (net 3 "Net-(N1-Pad14)")
  (net 4 "Net-(N1-Pad12)")
  (net 5 "Net-(N1-Pad11)")
  (net 6 "Net-(N1-Pad10)")
  (net 7 "Net-(N1-Pad6)")
  (net 8 "Net-(N1-Pad5)")
  (net 9 "Net-(N1-Pad4)")
  (net 10 "Net-(N1-Pad2)")
  (net 11 "Net-(J2-Pad1)")
  (net 12 "Net-(J3-Pad1)")
  (net 13 "Net-(J4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(N1-Pad10)")
    (add_net "Net-(N1-Pad11)")
    (add_net "Net-(N1-Pad12)")
    (add_net "Net-(N1-Pad14)")
    (add_net "Net-(N1-Pad2)")
    (add_net "Net-(N1-Pad4)")
    (add_net "Net-(N1-Pad5)")
    (add_net "Net-(N1-Pad6)")
    (add_net "Net-(N1-Pad8)")
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5FB0728C)
    (at 60.47232 110.49)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference REF** (at -0.01016 -1.31064) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5FB0728C)
    (at 75.52182 110.49762)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0.00254 -1.35636) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module "USB Micro numitronWatch:SolderJumper-2-NixieNecklace" (layer F.Cu) (tedit 5FB062B3)
    (at 73.530749 114.868672 323)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference Π (at 1.344197 0.036976 233 unlocked) (layer F.SilkS))
    (fp_text value "SolderJumper-2 nixieNecklace" (at -0.000001 1.9 143) (layer F.Fab))
    (pad 2 smd rect (at 0.1778 0.0254 323) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (pad 1 smd rect (at -0.635 0.0254 323) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 10 "Net-(N1-Pad2)"))
  )
  (module "USB Micro numitronWatch:SolderJumper-2-NixieNecklace" (layer F.Cu) (tedit 5FB062B3)
    (at 74.57948 112.830686 343)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference A/B (at 1.389419 0.070487 253 unlocked) (layer F.SilkS))
    (fp_text value "SolderJumper-2 nixieNecklace" (at 0 1.9 163) (layer F.Fab))
    (pad 2 smd rect (at 0.1778 0.0254 343) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (pad 1 smd rect (at -0.635 0.0254 343) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 9 "Net-(N1-Pad4)"))
  )
  (module "USB Micro numitronWatch:SolderJumper-2-NixieNecklace" (layer F.Cu) (tedit 5FB062B3)
    (at 63.670894 104.982501 129)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference - (at 1.250854 0.0254 219) (layer F.SilkS))
    (fp_text value "SolderJumper-2 nixieNecklace" (at 0 1.9 129) (layer F.Fab))
    (pad 2 smd rect (at 0.1778 0.0254 129) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (pad 1 smd rect (at -0.635 0.0254 129) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 6 "Net-(N1-Pad10)"))
  )
  (module "USB Micro numitronWatch:SolderJumper-2-NixieNecklace" (layer F.Cu) (tedit 5FB062B3)
    (at 73.89368 106.7816 31)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference ~~~ (at 1.32582 -0.016181 121) (layer F.SilkS))
    (fp_text value "SolderJumper-2 nixieNecklace" (at 0 1.9 31) (layer F.Fab))
    (pad 2 smd rect (at 0.1778 0.0254 31) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (pad 1 smd rect (at -0.635 0.0254 31) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 8 "Net-(N1-Pad5)"))
  )
  (module "USB Micro numitronWatch:SolderJumper-2-NixieNecklace" (layer F.Cu) (tedit 5FB062B3)
    (at 72.338003 104.953483 50)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference < (at 1.306994 0.081471 140 unlocked) (layer F.SilkS))
    (fp_text value "SolderJumper-2 nixieNecklace" (at 0 1.9 50) (layer F.Fab))
    (pad 2 smd rect (at 0.1778 0.0254 50) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (pad 1 smd rect (at -0.635 0.0254 50) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 7 "Net-(N1-Pad6)"))
  )
  (module "USB Micro numitronWatch:SolderJumper-2-NixieNecklace" (layer F.Cu) (tedit 5FB062B3)
    (at 62.086173 106.834134 151)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference > (at 1.314888 0.227065 241 unlocked) (layer F.SilkS))
    (fp_text value "SolderJumper-2 nixieNecklace" (at 0 1.9 151) (layer F.Fab))
    (pad 2 smd rect (at 0.1778 0.0254 151) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (pad 1 smd rect (at -0.635 0.0254 151) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 5 "Net-(N1-Pad11)"))
  )
  (module "USB Micro numitronWatch:SolderJumper-2-NixieNecklace" (layer F.Cu) (tedit 5FB062B3)
    (at 61.4299 112.80902 198)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference + (at 1.253087 0.02601 288) (layer F.SilkS))
    (fp_text value "SolderJumper-2 nixieNecklace" (at 0 1.9 18) (layer F.Fab))
    (pad 2 smd rect (at 0.1778 0.0254 198) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (pad 1 smd rect (at -0.635 0.0254 198) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 4 "Net-(N1-Pad12)"))
  )
  (module "USB Micro numitronWatch:SolderJumper-2-NixieNecklace" (layer F.Cu) (tedit 5FB062B3)
    (at 62.4078 114.75466 215)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference dB (at 1.280639 0.063146 125 unlocked) (layer F.SilkS))
    (fp_text value "SolderJumper-2 nixieNecklace" (at 0.000001 1.9 35) (layer F.Fab))
    (pad 2 smd rect (at 0.1778 0.0254 215) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (pad 1 smd rect (at -0.635 0.0254 215) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 3 "Net-(N1-Pad14)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill0.8mm (layer F.Cu) (tedit 5FB02632)
    (at 71.50862 117.18036)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference cathode (at -1.63576 1.3208 180) (layer F.SilkS))
    (fp_text value cathode (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 0.8001) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill0.8mm (layer F.Cu) (tedit 5FB01FF2)
    (at 66.7893 103.16972)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference GND (at -1.905 -0.0254 90) (layer F.SilkS))
    (fp_text value GND (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill0.8mm (layer F.Cu) (tedit 5FB01FF7)
    (at 69.3293 103.16972)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference 1v5 (at 1.905 -0.1016 90) (layer F.SilkS))
    (fp_text value 1v5 (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad1)"))
  )
  (module nixies-us:IN-19 (layer F.Cu) (tedit 0)
    (at 67.9958 110.5154)
    (fp_text reference N1 (at 2.0828 0.4826 90) (layer F.SilkS) hide)
    (fp_text value IN-19V (at -1.8034 0.0508 90) (layer F.SilkS))
    (pad 14 thru_hole circle (at -1.915 3.7041 333) (size 1.348 1.348) (drill 0.84) (layers *.Cu *.Mask)
      (net 3 "Net-(N1-Pad14)") (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at -3.3517 2.5047 333) (size 1.348 1.348) (drill 0.84) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at -4.1256 0.8007 333) (size 1.348 1.348) (drill 0.84) (layers *.Cu *.Mask)
      (net 4 "Net-(N1-Pad12)") (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at -4.0837 -1.0703 333) (size 1.348 1.348) (drill 0.84) (layers *.Cu *.Mask)
      (net 5 "Net-(N1-Pad11)") (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at -3.234 -2.7379 333) (size 1.348 1.348) (drill 0.84) (layers *.Cu *.Mask)
      (net 6 "Net-(N1-Pad10)") (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at -1.745 -3.8716 333) (size 1.348 1.348) (drill 0.84) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 0.0886 -4.2471 333) (size 1.348 1.348) (drill 0.84) (layers *.Cu *.Mask)
      (net 2 "Net-(N1-Pad8)") (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 1.9034 -3.7897 333) (size 1.348 1.348) (drill 0.84) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 3.34 -2.5904 333) (size 1.348 1.348) (drill 0.84) (layers *.Cu *.Mask)
      (net 7 "Net-(N1-Pad6)") (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 4.114 -0.8863 333) (size 1.348 1.348) (drill 0.84) (layers *.Cu *.Mask)
      (net 8 "Net-(N1-Pad5)") (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 4.0721 0.9847 333) (size 1.348 1.348) (drill 0.84) (layers *.Cu *.Mask)
      (net 9 "Net-(N1-Pad4)") (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 3.2224 2.6523 333) (size 1.348 1.348) (drill 0.84) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 1.7333 3.786 333) (size 1.348 1.348) (drill 0.84) (layers *.Cu *.Mask)
      (net 10 "Net-(N1-Pad2)") (solder_mask_margin 0.1016))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 67.9958 110.5154 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -2.58826 0.09906) (layer F.SilkS))
    (fp_text value R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(N1-Pad8)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill0.8mm (layer F.Cu) (tedit 5FB025FF)
    (at 64.34074 117.08384)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference anode (at 1.72212 1.22682 180) (layer F.SilkS))
    (fp_text value anode (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8001) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (gr_text "this\nside\nup" (at 70.02526 110.51286) (layer F.SilkS))
  (gr_text "tube\nside" (at 68.04406 108.25226) (layer B.SilkS))
  (gr_text "layout by\nAnalogTek" (at 68.00342 110.52302) (layer B.SilkS))
  (gr_circle (center 68.00342 110.52302) (end 77.00342 110.52302) (layer Edge.Cuts) (width 0.12))
  (gr_circle (center 67.9958 110.5154) (end 76.9958 110.5154) (layer Edge.Cuts) (width 0.12))
)
