(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 32)
    (zones 0)
    (modules 18)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.762)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.3 3.3)
    (pad_drill 3.3)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 91.15552 134.38124)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(C3-Pad2)")
  (net 4 +9V)
  (net 5 "Net-(L2-Pad1)")
  (net 6 "Net-(L3-Pad2)")
  (net 7 "Net-(PS1-Pad3)")
  (net 8 "Net-(PS1-Pad5)")
  (net 9 "Net-(C6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +9V)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(L3-Pad2)")
    (add_net "Net-(PS1-Pad3)")
    (add_net "Net-(PS1-Pad5)")
  )
  (module .pretty:CONV_TEC_2-0923 (layer F.Cu) (tedit 62DC198F)
    (at 118.910861 127.442781)
    (fp_text reference PS1 (at -1.176781 0.062679) (layer F.SilkS))
    (fp_text value TEC_2-0923 (at -1.301241 4.403539) (layer F.Fab))
    (pad 1 thru_hole roundrect (at -8.89 0) (size 1.28 2) (drill 0.85) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.28 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.28 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 8 "Net-(PS1-Pad5)"))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.28 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.28 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 7 "Net-(PS1-Pad3)"))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.28 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(L2-Pad1)"))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.28 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 6 "Net-(L3-Pad2)"))
  )
  (module .pretty:22Ga_pad_1_076mm_2mmsq (layer F.Cu) (tedit 60661559)
    (at 95.5167 124.69368)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference +9V (at 0 3.10388 90) (layer F.SilkS))
    (fp_text value CONN_1 (at -0.09652 -0.127) (layer F.SilkS) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 2.032 2.032) (drill 1.076) (layers *.Cu *.Mask F.SilkS) (roundrect_rratio 0.25)
      (net 4 +9V))
  )
  (module .pretty:22Ga_pad_1_076mm_2mmsq (layer F.Cu) (tedit 60661559)
    (at 118.8847 115.2525)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference GND (at -0.00508 2.86512 90) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 -0.2413) (layer F.SilkS) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 2.032 2.032) (drill 1.076) (layers *.Cu *.Mask F.SilkS) (roundrect_rratio 0.25)
      (net 1 GND))
  )
  (module .pretty:22Ga_pad_1_076mm_2mmsq (layer F.Cu) (tedit 60661559)
    (at 110.75162 115.2525)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference +15V (at -3.39852 -0.6731) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0.0889) (layer F.SilkS) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 2.032 2.032) (drill 1.076) (layers *.Cu *.Mask F.SilkS) (roundrect_rratio 0.25)
      (net 2 "Net-(C2-Pad1)"))
  )
  (module .pretty:22Ga_pad_1_076mm_2mmsq (layer F.Cu) (tedit 60661559)
    (at 123.72118 115.2525)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference -15V (at 3.25596 -0.6731) (layer F.SilkS))
    (fp_text value CONN_1 (at 0.16256 0.02032) (layer F.SilkS) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 2.032 2.032) (drill 1.076) (layers *.Cu *.Mask F.SilkS) (roundrect_rratio 0.25)
      (net 3 "Net-(C3-Pad2)"))
  )
  (module .pretty:Choke_Bourns_9mm (layer F.Cu) (tedit 62DBFD67)
    (at 105.75544 120.84558 270)
    (descr "Choke, Axial, 10mm")
    (tags "Choke, Axial, 10mm")
    (fp_text reference L1 (at -0.08636 -0.02032 90) (layer F.SilkS))
    (fp_text value 10uH (at 0.17018 0.98806 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -4.5 0 270) (size 1.88 1.66) (drill 0.72) (layers *.Cu *.Mask)
      (net 4 +9V))
    (pad 2 thru_hole oval (at 4.5 0 270) (size 1.88 1.66) (drill 0.72) (layers *.Cu *.Mask)
      (net 9 "Net-(C6-Pad1)"))
  )
  (module .pretty:Choke_Bourns_9mm (layer F.Cu) (tedit 62DBFD67)
    (at 118.23446 121.98604 180)
    (descr "Choke, Axial, 10mm")
    (tags "Choke, Axial, 10mm")
    (fp_text reference L2 (at 0.00508 0.01016) (layer F.SilkS))
    (fp_text value 10uH (at -0.04064 0.93726) (layer F.Fab))
    (pad 1 thru_hole oval (at -4.5 0 180) (size 1.88 1.66) (drill 0.72) (layers *.Cu *.Mask)
      (net 5 "Net-(L2-Pad1)"))
    (pad 2 thru_hole oval (at 4.5 0 180) (size 1.88 1.66) (drill 0.72) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
  )
  (module .pretty:Choke_Bourns_9mm (layer F.Cu) (tedit 62DBFD67)
    (at 131.7117 122.44616 270)
    (descr "Choke, Axial, 10mm")
    (tags "Choke, Axial, 10mm")
    (fp_text reference L3 (at -0.11138 -0.01016 90) (layer F.SilkS))
    (fp_text value 10uH (at -0.00762 -1.07696 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -4.5 0 270) (size 1.88 1.66) (drill 0.72) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (pad 2 thru_hole oval (at 4.5 0 270) (size 1.88 1.66) (drill 0.72) (layers *.Cu *.Mask)
      (net 6 "Net-(L3-Pad2)"))
  )
  (module .pretty:PassinwindElectronics_100_15mm (layer F.Cu) (tedit 60A18879)
    (at 92.67698 125.82144 90)
    (fp_text reference PWE (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module .pretty:3.3mm_hole (layer F.Cu) (tedit 58B0D899)
    (at 133.0706 131.63042)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value "3.5MM Hole" (at 0.14732 -0.1397) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask F.SilkS))
  )
  (module .pretty:3.3mm_hole (layer F.Cu) (tedit 62DC2131)
    (at 93.62948 115.77574)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value "3.5MM Hole" (at 0.16002 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask F.SilkS))
  )
  (module .pretty:Nichi_8mm_electro_3_5_mm (layer F.Cu) (tedit 62DB5F42)
    (at 100.06584 119.23268 180)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C1 (at 0.04638 1.47574) (layer F.SilkS))
    (fp_text value 100uF (at 0.06096 -1.34366) (layer F.SilkS) hide)
    (fp_text user + (at -1.76784 -1.6764) (layer F.SilkS))
    (pad 2 thru_hole oval (at 1.75 0 180) (size 1.5 1.7) (drill 0.73) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at -1.75 0 180) (size 1.4 1.7) (drill 0.73) (layers *.Cu *.Mask F.SilkS) (roundrect_rratio 0.25)
      (net 4 +9V))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Nichi_22uF_25V_2mm (layer F.Cu) (tedit 60513860)
    (at 114.9223 117.78234)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C4 (at -0.0127 1.4859) (layer F.SilkS))
    (fp_text value 22uF (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text user + (at -1.2 -1.43) (layer F.SilkS))
    (pad 2 thru_hole oval (at 1.1 0) (size 1.397 1.5) (drill 0.72) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at -1.2 0) (size 1.3 1.5) (drill 0.72) (layers *.Cu *.Mask F.SilkS) (roundrect_rratio 0.25)
      (net 2 "Net-(C2-Pad1)"))
    (model discret/c_vert_c1v5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Nichi_22uF_25V_2mm (layer F.Cu) (tedit 62DB6E70)
    (at 127.51054 119.02732 90)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C6 (at -0.0254 1.45786) (layer F.SilkS))
    (fp_text value 22uF (at 0 -1.6 90) (layer F.SilkS) hide)
    (fp_text user + (at -1.2 -1.43 90) (layer F.SilkS))
    (pad 1 thru_hole roundrect (at -1.2 0 90) (size 1.3 1.5) (drill 0.72) (layers *.Cu *.Mask F.SilkS) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 thru_hole oval (at 1.1 0 90) (size 1.397 1.5) (drill 0.72) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C3-Pad2)"))
    (model discret/c_vert_c1v5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:C__Murata_100P_2.5mm_2 (layer F.Cu) (tedit 62DC1F0D)
    (at 110.75162 119.02948 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C3 (at 0.02286 0.77216 90) (layer F.SilkS))
    (fp_text value 100nF (at -0.025 -0.025 270) (layer F.SilkS) hide)
    (fp_text user C (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole oval (at -1.25 0 270) (size 1.4 1.55) (drill 0.68) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 1.25 0 270) (size 1.4 1.55) (drill 0.68) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:C__Murata_100P_2.5mm_2 (layer F.Cu) (tedit 62DC1C60)
    (at 122.47118 118.44782)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C5 (at -0.03556 -0.74168) (layer F.SilkS))
    (fp_text value 100nF (at -0.025 -0.025 180) (layer F.SilkS) hide)
    (fp_text user C (at 1.25 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.25 0) (size 1.4 1.55) (drill 0.68) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (pad 1 thru_hole oval (at -1.25 0) (size 1.4 1.55) (drill 0.68) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:DO-41 (layer F.Cu) (tedit 62DBFE8F)
    (at 98.425 124.69876 270)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 3.93 0.02 90) (layer F.SilkS))
    (fp_text value D_Zener (at 3.82 0.04 90) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.6 1.72) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 4 +9V))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.72) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Diodes_ThroughHole.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Nichi_6.3mm_electro_2_5_mm (layer F.Cu) (tedit 62DB615F)
    (at 103.91394 130.175 180)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C2 (at -0.04826 -1.9304) (layer F.SilkS))
    (fp_text value 47uF (at 0.01524 1.34366) (layer F.SilkS) hide)
    (fp_text user + (at -1.22174 1.62306) (layer F.SilkS))
    (pad 2 thru_hole oval (at 1.25 0 180) (size 1.5 1.65) (drill 0.73) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at -1.25 0 180) (size 1.3 1.6) (drill 0.73) (layers *.Cu *.Mask F.SilkS) (roundrect_rratio 0.25)
      (net 9 "Net-(C6-Pad1)"))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 93.32722 113.284) (end 133.46176 113.284) (layer Edge.Cuts) (width 0.1))
  (gr_text "PWDCDC_V1\nBy CE 2022" (at 126.49708 131.79298) (layer B.SilkS))
  (gr_arc (start 93.35516 132.2197) (end 91.208861 132.199381) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 93.31706 115.43944) (end 93.337379 113.293141) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 133.42366 115.42522) (end 135.569959 115.445539) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 133.4135 132.04444) (end 133.393181 134.190739) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.20124 132.1562) (end 91.17838 115.38966) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.42112 134.18312) (end 93.20022 134.37362) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.56996 115.40998) (end 135.54964 132.08508) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 142.14602 140.80998) (xy 88.53932 141.02588) (xy 88.70442 107.70108) (xy 141.41958 107.03306)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 137.22858 136.3345) (xy 89.45118 137.16254) (xy 89.25814 111.49838) (xy 137.27684 111.17834)
      )
    )
    (polygon
      (pts
        (xy 130.5179 120.12168) (xy 130.5179 124.86894) (xy 130.80238 125.11786) (xy 132.78104 125.11024) (xy 133.02742 124.86894)
        (xy 133.02488 120.12676) (xy 132.75056 119.80418) (xy 130.76174 119.80418)
      )
    )
    (polygon
      (pts
        (xy 104.55656 118.38432) (xy 104.559163 123.39066) (xy 104.68102 123.51766) (xy 106.93908 123.51766) (xy 107.07116 123.39066)
        (xy 107.0737 118.38432) (xy 106.895885 118.206338) (xy 104.767378 118.204186)
      )
    )
    (polygon
      (pts
        (xy 120.7008 120.76938) (xy 115.71732 120.76938) (xy 115.57 120.9421) (xy 115.562565 123.12396) (xy 115.719855 123.306915)
        (xy 120.7008 123.30938) (xy 120.86082 123.1138) (xy 120.86082 120.93448)
      )
    )
  )
)
