(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 0.1916)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "#808080D4")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(color "Polyimide")
				(thickness 0.1016)
				(material "Polyimide")
				(epsilon_r 3.2)
				(loss_tangent 0.004)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "#808080FF")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00210fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "output/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/SCL")
	(net 3 "/SDA")
	(net 4 "/ANT")
	(net 5 "VDD")
	(net 6 "unconnected-(GS1-GS-Pad1)")
	(net 7 "/SWIO")
	(net 8 "/PZ+")
	(net 9 "/PZ-")
	(net 10 "/FD")
	(net 11 "Net-(D1-K)")
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 162.56 97.155)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C14445"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A105KP5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "nfcwchsao.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 151.765 101.6 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -2.032 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DNP"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" ""
			(at 50.165 253.365 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 50.165 253.365 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "nfcwchsao.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/ANT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/ANT")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprint:gs_logo_200mil"
		(layer "F.Cu")
		(at 159.385 88.9 90)
		(property "Reference" "GS1"
			(at 0 -3.175 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GS_logo"
			(at 0 -0.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "footprint:gs_logo_200mil"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" ""
			(at 248.285 -70.485 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 248.285 -70.485 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "nfcwchsao.kicad_sch")
		(attr through_hole)
		(pad "1" smd custom
			(at 0 0 90)
			(size 5.08 5.08)
			(layers "F.Cu")
			(net 6 "unconnected-(GS1-GS-Pad1)")
			(pinfunction "GS")
			(pintype "unspecified")
			(zone_connect 0)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 165.1 107.315 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3.3k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" ""
			(at 276.225 -60.325 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 276.225 -60.325 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "nfcwchsao.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/SWIO")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:KiCad-Logo_8mm"
		(locked yes)
		(layer "F.Cu")
		(at 159.385 116.84)
		(descr "KiCad Logo")
		(tags "Logo KiCad")
		(property "Reference" "REF**"
			(at 0 -6.35 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "KiCad-Logo_8mm"
			(at 0 7.62 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "custom:KiCad-Logo_8mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
	)
	(footprint "custom:Buzzer_Murata_PKLCS1212E_handy"
		(layer "F.Cu")
		(at 159.385 88.9)
		(descr "Murata Buzzer https://www.murata.com/~/media/webrenewal/support/library/catalog/products/sound/p37e.ashx")
		(tags "Murata Buzzer Beeper")
		(property "Reference" "LS1"
			(at -3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Speaker_Crystal"
			(at 0 7 360)
			(layer "F.Fab")
		)
		(property "Footprint" "custom:Buzzer_Murata_PKLCS1212E_handy"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "PKLCS1212E20A0-R1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "nfcwchsao.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -6.6 0)
			(size 3.2 4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/PZ-")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 6.6 0)
			(size 3.2 4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "/PZ+")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${KICAD6_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/Buzzer_Murata_PKLCS1212E.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 163.195 101.6 -90)
		(descr "SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOP SO")
		(property "Reference" "U2"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "CH32V003F4P6"
			(at -0.127 -29.083 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2302231730_WCH-Jiangsu-Qin-Heng-CH32V003F4U6_C5299908.pdf"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C5346354"
			(at 61.595 264.795 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CH32V003J4M6"
			(at 61.595 264.795 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "nfcwchsao.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.625 -1.905 270)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/PZ+")
			(pinfunction "PA1_T1CH2_A1")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -2.625 -0.635 270)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.625 0.635 270)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "/PZ-")
			(pinfunction "PA2_T1CH2N_A0")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.625 1.905 270)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.625 1.905 270)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/SDA")
			(pinfunction "PC1_SDA")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at 2.625 0.635 270)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/SCL")
			(pinfunction "PC2_SCL")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 2.625 -0.635 270)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/FD")
			(pinfunction "PC4_MCO_A2")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.625 -1.905 270)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/SWIO")
			(pinfunction "PD1_SWIO")
			(pintype "bidirectional")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOP-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:PinHeader_2x03_P2.54mm_Staggered"
		(layer "F.Cu")
		(at 168.27 99.075)
		(descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x03 2.54mm double row")
		(property "Reference" "J1"
			(at 1.27 -2.33 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_02x03_Odd_Even"
			(at 1.27 7.41 180)
			(layer "F.Fab")
		)
		(property "Footprint" "custom:PinHeader_2x03_P2.54mm_Staggered"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "nfcwchsao.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.54 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -0.127 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VDD")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.667 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0.127 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.413 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at -0.127 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SWIO")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.667 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/FD")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 159.385 103.505 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" ""
			(at 55.88 262.89 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 55.88 262.89 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "nfcwchsao.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/SCL")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 155.575 101.6 90)
		(descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SO SO")
		(property "Reference" "U1"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "NT3H2211"
			(at 0.127 37.846 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/NT3H2111_2211.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2905792"
			(at 257.175 -53.975 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "NT3H2211W0FT1X"
			(at 257.175 -53.975 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm* DFN*3x2mm*P0.5mm*")
		(sheetname "Root")
		(sheetfile "nfcwchsao.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.575 -1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/ANT")
			(pinfunction "LA")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.575 -0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.575 0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.575 1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/FD")
			(pinfunction "FD")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.575 1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at 2.575 0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "VDD")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.575 -0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "VDD")
			(pinfunction "VOUT")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 2.575 -1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/ANT")
			(pinfunction "LB")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 159.385 99.695 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" ""
			(at 59.69 259.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 59.69 259.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "nfcwchsao.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/SDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "VDD")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:LED_Right_Angle_3x2x1mm"
		(layer "F.Cu")
		(at 159.385 109.22 180)
		(descr "Kingbright surface mount LED, right angle, 3.0 x 2.0 x 1.0 mm, https://www.kingbright.com/attachments/file/psearch/000/00/00/KPA-3010SURCK(Ver.26A).pdf")
		(tags "Kingbright LED right-angle")
		(property "Reference" "D1"
			(at 0 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "Green"
			(at 0 3.9 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "custom:LED_Right_Angle_3x2x1mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "nfcwchsao.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.75 0.5 180)
			(size 1.5 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1666666667)
			(net 11 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.75 0.5 180)
			(size 1.5 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1666666667)
			(net 5 "VDD")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0 1 180)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Kingbright_KPA-3010_3x2x1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 142.24 80.645)
		(mid 143.169936 78.399936)
		(end 145.415 77.47)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 145.415 125.73)
		(mid 143.169936 124.800064)
		(end 142.24 122.555)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 173.355 77.47)
		(mid 175.600064 78.399936)
		(end 176.53 80.645)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.53 80.645)
		(end 176.53 122.555)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 176.53 122.555)
		(mid 175.600064 124.800064)
		(end 173.355 125.73)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.02 109.22)
		(end 158.75 109.22)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 158.75 111.76)
		(mid 157.48 110.49)
		(end 158.75 109.22)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.75 111.76)
		(end 160.02 111.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.415 77.47)
		(end 173.355 77.47)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.24 122.555)
		(end 142.24 80.645)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 160.02 109.22)
		(mid 161.29 110.49)
		(end 160.02 111.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.355 125.73)
		(end 145.415 125.73)
		(layer "Edge.Cuts")
	)
	(gr_text "Beeping\nBlinking\nBadge\nBuddy\n"
		(at 147.955 111.125 90)
		(layer "F.SilkS")
	)
	(gr_text "B4"
		(at 171.45 88.9 90)
		(layer "F.SilkS")
	)
	(gr_text "NTAG I2C Plus\nWCH32V003"
		(at 147.32 89.535 90)
		(layer "F.SilkS")
	)
)
