(kicad_pcb (version 20171130) (host pcbnew 5.1.8-db9833491~88~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 43)
    (zones 0)
    (modules 3)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 0.8)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 111.379 92.202)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "C:/HotWheels/Hotwheels-Firmware/Documents/PCB_Farbsensor/HotwheelsBoard-Farbsensor/Output/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(U1-Pad6)")
  (net 4 "Net-(U1-Pad8)")
  (net 5 "Net-(U1-Pad1)")
  (net 6 "Net-(U1-Pad7)")
  (net 7 "Net-(U1-Pad2)")
  (net 8 "Net-(U2-Pad3)")
  (net 9 "Net-(U2-Pad2)")
  (net 10 VCC)
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net VCC)
  )
  (module SOIC8 (layer F.Cu) (tedit 0)
    (at 105.98676 107.74322 180)
    (descr "<b>Small Outline IC</b>")
    (attr smd)
    (fp_text reference U1 (at 1.5318 -2.84076) (layer F.SilkS))
    (fp_text value TCS3200 (at -1.04884 -2.8941) (layer F.SilkS))
    (pad 5 smd rect (at 2.6 1.905 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC))
    (pad 6 smd rect (at 2.6 0.635 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad6)"))
    (pad 8 smd rect (at 2.6 -1.905 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad8)"))
    (pad 4 smd rect (at -2.6 1.905 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.6 0.635 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.6 -1.905 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad1)"))
    (pad 7 smd rect (at 2.6 -0.635 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad7)"))
    (pad 2 smd rect (at -2.6 -0.635 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad2)"))
  )
  (module LED_SMD:LED_PLCC-2 (layer F.Cu) (tedit 5FC7B933)
    (at 112.514 107.761 90)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (attr smd)
    (fp_text reference D1 (at -2.87632 -0.0555) (layer F.SilkS))
    (fp_text value LED (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.5 0 90) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module castellated_pads_top:DIP-10_244_ELL (layer F.Cu) (tedit 5FC64EE3)
    (at 114.075 111.975 180)
    (fp_text reference U2 (at -1.37054 3.80656 90) (layer Cmts.User))
    (fp_text value Castellated_pads_top (at 6 -1.3) (layer F.Fab))
    (pad 5 thru_hole roundrect (at 10.9 7.4 180) (size 1.7 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(U1-Pad6)"))
    (pad 6 thru_hole roundrect (at 10.9 0.4 180) (size 1.7 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(U1-Pad8)"))
    (pad 4 thru_hole roundrect (at 8.45 7.4 180) (size 1.7 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 VCC))
    (pad 7 thru_hole roundrect (at 8.45 0.4 180) (size 1.7 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(U1-Pad7)"))
    (pad 3 thru_hole roundrect (at 6 7.4 180) (size 1.7 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(U2-Pad3)"))
    (pad 8 thru_hole roundrect (at 6 0.4 180) (size 1.7 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(U1-Pad1)"))
    (pad 2 thru_hole roundrect (at 3.55 7.4 180) (size 1.7 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(U2-Pad2)"))
    (pad 9 thru_hole roundrect (at 3.55 0.4 180) (size 1.7 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(U1-Pad2)"))
    (pad 1 thru_hole roundrect (at 1.1 7.4 180) (size 1.7 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad2)"))
    (pad 10 thru_hole roundrect (at 1.1 0.4 180) (size 1.7 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
  )
  (gr_text "Sotaro v1.0" (at 108.0643 107.95254) (layer B.SilkS))
  (gr_line (start 114.575 104.575) (end 114.575 111.575) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.575 104.575) (end 114.575 104.575) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.575 111.575) (end 114.575 111.575) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.575 104.575) (end 101.575 111.575) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.57432 111.62538) (xy 101.6127 111.6076) (xy 101.59238 104.57434) (xy 114.59464 104.55402)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.58984 104.541324) (xy 114.59464 104.56418) (xy 114.5667 111.57966) (xy 101.5873 111.57712) (xy 101.58984 104.541324)
        (xy 101.5873 104.54132) (xy 101.58984 104.54132)
      )
    )
  )
)
