(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 23)
    (no_connects 0)
    (area 159.461999 83.769999 230.682001 104.698001)
    (thickness 1.6)
    (drawings 9)
    (tracks 92)
    (zones 0)
    (modules 7)
    (nets 49)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(B1-Pad2)")
  (net 3 "Net-(B1-Pad3)")
  (net 4 "Net-(B1-Pad4)")
  (net 5 "Net-(B1-Pad5)")
  (net 6 "Net-(B1-Pad6)")
  (net 7 "Net-(B1-Pad7)")
  (net 8 "Net-(B1-Pad8)")
  (net 9 "Net-(B1-Pad9)")
  (net 10 "Net-(B1-Pad10)")
  (net 11 +3V3)
  (net 12 "Net-(B1-Pad35)")
  (net 13 "Net-(B1-Pad34)")
  (net 14 "Net-(B1-Pad33)")
  (net 15 "Net-(B1-Pad32)")
  (net 16 "Net-(B1-Pad31)")
  (net 17 "Net-(B1-Pad30)")
  (net 18 "Net-(B1-Pad13)")
  (net 19 "Net-(B1-Pad14)")
  (net 20 "Net-(B1-Pad15)")
  (net 21 "Net-(B1-Pad16)")
  (net 22 "Net-(B1-Pad17)")
  (net 23 "Net-(B1-Pad18)")
  (net 24 "Net-(B1-Pad19)")
  (net 25 "Net-(B1-Pad20)")
  (net 26 "Net-(B1-Pad21)")
  (net 27 "Net-(B1-Pad22)")
  (net 28 "Net-(B1-Pad23)")
  (net 29 "Net-(B1-Pad24)")
  (net 30 "Net-(gps1-Pad1)")
  (net 31 "Net-(gps1-Pad2)")
  (net 32 "Net-(gps1-Pad4)")
  (net 33 "Net-(gps1-Pad5)")
  (net 34 "Net-(gps1-Pad7)")
  (net 35 "Net-(gps1-Pad8)")
  (net 36 "Net-(gps1-Pad10)")
  (net 37 "Net-(gps1-Pad11)")
  (net 38 "Net-(gps1-Pad12)")
  (net 39 "Net-(gps1-Pad13)")
  (net 40 "Net-(gps1-Pad14)")
  (net 41 "Net-(gps1-Pad15)")
  (net 42 "Net-(gps1-Pad16)")
  (net 43 "Net-(J1-Pad2)")
  (net 44 "Net-(J1-Pad1)")
  (net 45 "Net-(gps1-Pad19)")
  (net 46 "Net-(gps1-Pad20)")
  (net 47 "Net-(gps1-Pad21)")
  (net 48 "Net-(gps1-Pad22)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(B1-Pad10)")
    (add_net "Net-(B1-Pad13)")
    (add_net "Net-(B1-Pad14)")
    (add_net "Net-(B1-Pad15)")
    (add_net "Net-(B1-Pad16)")
    (add_net "Net-(B1-Pad17)")
    (add_net "Net-(B1-Pad18)")
    (add_net "Net-(B1-Pad19)")
    (add_net "Net-(B1-Pad2)")
    (add_net "Net-(B1-Pad20)")
    (add_net "Net-(B1-Pad21)")
    (add_net "Net-(B1-Pad22)")
    (add_net "Net-(B1-Pad23)")
    (add_net "Net-(B1-Pad24)")
    (add_net "Net-(B1-Pad3)")
    (add_net "Net-(B1-Pad30)")
    (add_net "Net-(B1-Pad31)")
    (add_net "Net-(B1-Pad32)")
    (add_net "Net-(B1-Pad33)")
    (add_net "Net-(B1-Pad34)")
    (add_net "Net-(B1-Pad35)")
    (add_net "Net-(B1-Pad4)")
    (add_net "Net-(B1-Pad5)")
    (add_net "Net-(B1-Pad6)")
    (add_net "Net-(B1-Pad7)")
    (add_net "Net-(B1-Pad8)")
    (add_net "Net-(B1-Pad9)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(gps1-Pad1)")
    (add_net "Net-(gps1-Pad10)")
    (add_net "Net-(gps1-Pad11)")
    (add_net "Net-(gps1-Pad12)")
    (add_net "Net-(gps1-Pad13)")
    (add_net "Net-(gps1-Pad14)")
    (add_net "Net-(gps1-Pad15)")
    (add_net "Net-(gps1-Pad16)")
    (add_net "Net-(gps1-Pad19)")
    (add_net "Net-(gps1-Pad2)")
    (add_net "Net-(gps1-Pad20)")
    (add_net "Net-(gps1-Pad21)")
    (add_net "Net-(gps1-Pad22)")
    (add_net "Net-(gps1-Pad4)")
    (add_net "Net-(gps1-Pad5)")
    (add_net "Net-(gps1-Pad7)")
    (add_net "Net-(gps1-Pad8)")
  )
  (module RF_Modules:RN42 (layer F.Cu) (tedit 58D1E594)
    (at 212.344 93.98 270)
    (descr "Class 2 Bluetooth Module with on-board antenna")
    (tags "Bluetooth Module")
    (attr smd)
    (fp_text reference B1 (at 1.27 2.54 270) (layer F.SilkS))
    (fp_text value Bluetooth (at 0.3 0 270) (layer F.Fab))
    (fp_text user "Antenna Area" (at 0.3 -13 270) (layer Cmts.User))
    (pad 1 smd oval (at -6.4 -6 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd oval (at -6.4 -4.8 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(B1-Pad2)"))
    (pad 3 smd oval (at -6.4 -3.6 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(B1-Pad3)"))
    (pad 4 smd oval (at -6.4 -2.4 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(B1-Pad4)"))
    (pad 5 smd oval (at -6.4 -1.2 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(B1-Pad5)"))
    (pad 6 smd oval (at -6.4 0 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B1-Pad6)"))
    (pad 7 smd oval (at -6.4 1.2 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(B1-Pad7)"))
    (pad 8 smd oval (at -6.4 2.4 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(B1-Pad8)"))
    (pad 9 smd oval (at -6.4 3.6 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(B1-Pad9)"))
    (pad 10 smd oval (at -6.4 4.8 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(B1-Pad10)"))
    (pad 11 smd oval (at -6.4 6 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 12 smd oval (at -6.4 7.2 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 35 smd oval (at -4.1 9.7) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(B1-Pad35)"))
    (pad 29 smd oval (at -3.1 9.7) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 34 smd oval (at -1.8 9.7) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(B1-Pad34)"))
    (pad 33 smd oval (at -0.6 9.7) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(B1-Pad33)"))
    (pad 32 smd oval (at 0.6 9.7) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(B1-Pad32)"))
    (pad 31 smd oval (at 1.8 9.7) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(B1-Pad31)"))
    (pad 28 smd oval (at 3.1 9.7) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 30 smd oval (at 4.1 9.7) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(B1-Pad30)"))
    (pad 13 smd oval (at 6.4 7.2 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(B1-Pad13)"))
    (pad 14 smd oval (at 6.4 6 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B1-Pad14)"))
    (pad 15 smd oval (at 6.4 4.8 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(B1-Pad15)"))
    (pad 16 smd oval (at 6.4 3.6 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(B1-Pad16)"))
    (pad 17 smd oval (at 6.4 2.4 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(B1-Pad17)"))
    (pad 18 smd oval (at 6.4 1.2 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(B1-Pad18)"))
    (pad 19 smd oval (at 6.4 0 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(B1-Pad19)"))
    (pad 20 smd oval (at 6.4 -1.2 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(B1-Pad20)"))
    (pad 21 smd oval (at 6.4 -2.4 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(B1-Pad21)"))
    (pad 22 smd oval (at 6.4 -3.6 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(B1-Pad22)"))
    (pad 23 smd oval (at 6.4 -4.8 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(B1-Pad23)"))
    (pad 24 smd oval (at 6.4 -6 270) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(B1-Pad24)"))
    (pad 36 smd rect (at -5.6 9.3 270) (size 1.8 1) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd rect (at 5.6 9.3 270) (size 1.8 1) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd rect (at 5.6 -9.7 270) (size 1.8 1) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd rect (at -5.6 -9.7 270) (size 1.8 1) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 193.294 88.9 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 182.118 89.662 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprintlibrary:GPS (layer F.Cu) (tedit 58D1E58F)
    (at 177.292 85.852 270)
    (fp_text reference gps1 (at 7.62 6.35 270) (layer F.SilkS))
    (fp_text value GPSReceiver (at 7.62 8.89 270) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(gps1-Pad1)"))
    (pad 2 smd rect (at 0 1.27 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(gps1-Pad2)"))
    (pad 3 smd rect (at 0 2.54 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 4 smd rect (at 0 3.81 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(gps1-Pad4)"))
    (pad 5 smd rect (at 0 5.08 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(gps1-Pad5)"))
    (pad 6 smd rect (at 0 6.35 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 0 7.62 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(gps1-Pad7)"))
    (pad 8 smd rect (at 0 8.89 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(gps1-Pad8)"))
    (pad 9 smd rect (at 0 10.16 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 0 11.43 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(gps1-Pad10)"))
    (pad 11 smd rect (at 0 12.7 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(gps1-Pad11)"))
    (pad 12 smd rect (at 0 13.97 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(gps1-Pad12)"))
    (pad 13 smd rect (at 0 15.24 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(gps1-Pad13)"))
    (pad 14 smd rect (at 15.51 0 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(gps1-Pad14)"))
    (pad 15 smd rect (at 15.51 1.27 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(gps1-Pad15)"))
    (pad 16 smd rect (at 15.51 2.54 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(gps1-Pad16)"))
    (pad 17 smd rect (at 15.51 3.81 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J1-Pad2)"))
    (pad 18 smd rect (at 15.51 5.08 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J1-Pad1)"))
    (pad 19 smd rect (at 15.51 6.35 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(gps1-Pad19)"))
    (pad 20 smd rect (at 15.51 12.7 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(gps1-Pad20)"))
    (pad 21 smd rect (at 15.51 13.97 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(gps1-Pad21)"))
    (pad 22 smd rect (at 15.51 15.24 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(gps1-Pad22)"))
    (pad 23 smd rect (at 3.945 1.905 270) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 6.485 1.905 270) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 25 smd rect (at 9.025 1.905 270) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 26 smd rect (at 11.565 1.905 270) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 27 smd rect (at 3.945 13.335 270) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at 6.485 13.335 270) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at 9.025 13.335 270) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 30 smd rect (at 11.565 13.335 270) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.00mm_SMD_Pin1Left (layer F.Cu) (tedit 58D1E5CF)
    (at 184.912 99.314)
    (descr "surface-mounted straight pin header, 1x02, 2.00mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x02 2.00mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference J1 (at 1.27 -1.27) (layer F.SilkS))
    (fp_text value clkSp (at -1.27 1.27) (layer F.Fab))
    (fp_text user %R (at 1.27 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -2.125 -1) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 2.125 1) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.00mm_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.00mm_SMD_Pin1Right (layer F.Cu) (tedit 58CD4EC9)
    (at 187.96 89.408 90)
    (descr "surface-mounted straight pin header, 1x02, 2.00mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x02 2.00mm single row style2 pin1 right")
    (attr smd)
    (fp_text reference J2 (at 0 -3.06 90) (layer F.SilkS))
    (fp_text value SourceGnd (at 0 3.06 90) (layer F.Fab))
    (fp_text user %R (at 0 -3.06 90) (layer F.Fab))
    (pad 2 smd rect (at -2.125 1 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.125 -1 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.00mm_SMD_Pin1Right.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.00mm_SMD_Pin1Right (layer F.Cu) (tedit 58D1E5B2)
    (at 195.58 97.79)
    (descr "surface-mounted straight pin header, 1x02, 2.00mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x02 2.00mm single row style2 pin1 right")
    (attr smd)
    (fp_text reference J3 (at -2.54 -1.27) (layer F.SilkS))
    (fp_text value RXTX (at 1.27 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -3.06) (layer F.Fab))
    (pad 2 smd rect (at -2.125 1) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(B1-Pad13)"))
    (pad 1 smd rect (at 2.125 -1) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B1-Pad14)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.00mm_SMD_Pin1Right.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 162.052 83.82) (end 162.306 83.82) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.544 83.82) (end 162.052 83.82) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.036 83.82) (end 161.544 83.82) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.512 83.82) (end 161.036 83.82) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.512 104.648) (end 159.512 83.82) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 199.136 104.648) (end 159.512 104.648) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 230.632 104.648) (end 199.136 104.648) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 230.632 83.82) (end 230.632 104.648) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 160.782 83.82) (end 230.632 83.82) (angle 90) (layer Edge.Cuts) (width 0.1))
)
