<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>Mystifier KD0GLS 2021</text>
<text>+5V-</text>
<wire x1="0" y1="22.86" x2="0" y2="0" width="0.254" layer="20"/>
<wire x1="0" y1="0" x2="107.315" y2="0" width="0.254" layer="20"/>
<wire x1="107.315" y1="0" x2="107.315" y2="22.86" width="0.254" layer="20"/>
<wire x1="107.315" y1="22.86" x2="0" y2="22.86" width="0.254" layer="20"/>
<text>ICSP</text>
</plain>
<libraries>
<library name="kd0gls">
<packages>
<package name="INDUCTOR_TDK_SLF7045">
<description>TDK SLF7045 series surface mount inductors
&lt;p&gt;
TDK P/N SLF7032T-101MR45-2PF, Digi-Key P/N 445-1999-1-ND</description>
</package>
<package name="2225">
</package>
<package name="CONN_PHOENIX_TERM_BLOCK_2PIN_100">
</package>
<package name="NE-2">
<description>NE-2</description>
</package>
<package name="SOT223">
</package>
<package name="SMA">
</package>
<package name="1206">
</package>
<package name="0805">
</package>
<package name="EIA7343">
<description>Kemet size D</description>
</package>
<package name="SOT23-3">
<description>Revised pad sizes and spacing per LM3480 data sheet.</description>
</package>
<package name="SOIC14">
<description>Small Outline 14-Pin Narrow (150 mil)</description>
</package>
<package name="CONN_ICSP_PADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="L1" library="kd0gls" package="INDUCTOR_TDK_SLF7045" value="100uH"/>
<element name="C2" library="kd0gls" package="2225" value="1uF/200v"/>
<element name="R2" library="kd0gls" package="1206" value="390K"/>
<element name="R3" library="kd0gls" package="0805" value="10K"/>
<element name="R4" library="kd0gls" package="1206" value="68K"/>
<element name="J1" library="kd0gls" package="CONN_PHOENIX_TERM_BLOCK_2PIN_100" value="CONN_PHOENIX_TERM_BLOCK_2PIN_100"/>
<element name="NL1" library="kd0gls" package="NE-2" value="NE-2"/>
<element name="NL2" library="kd0gls" package="NE-2" value="NE-2"/>
<element name="NL3" library="kd0gls" package="NE-2" value="NE-2"/>
<element name="NL4" library="kd0gls" package="NE-2" value="NE-2"/>
<element name="NL5" library="kd0gls" package="NE-2" value="NE-2"/>
<element name="NL6" library="kd0gls" package="NE-2" value="NE-2"/>
<element name="C1" library="kd0gls" package="EIA7343" value="100uF/10v"/>
<element name="C3" library="kd0gls" package="0805" value="0.1uF"/>
<element name="Q7" library="kd0gls" package="SOT223" value="STN1N20"/>
<element name="Q1" library="kd0gls" package="SOT23-3" value="ZVN3320F"/>
<element name="Q2" library="kd0gls" package="SOT23-3" value="ZVN3320F"/>
<element name="Q3" library="kd0gls" package="SOT23-3" value="ZVN3320F"/>
<element name="Q4" library="kd0gls" package="SOT23-3" value="ZVN3320F"/>
<element name="Q5" library="kd0gls" package="SOT23-3" value="ZVN3320F"/>
<element name="Q6" library="kd0gls" package="SOT23-3" value="ZVN3320F"/>
<element name="D1" library="kd0gls" package="SMA" value="DIODE_US1D"/>
<element name="R1" library="kd0gls" package="0805" value="10K"/>
<element name="U1" library="kd0gls" package="SOIC14" value="PIC16F15224/SL"/>
<element name="ICSP1" library="kd0gls" package="CONN_ICSP_PADS" value="CONN_ICSP_SMT"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="Q7" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q6" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="14"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="ICSP1" pad="VSS"/>
</signal>
<signal name="+5V">
<contactref element="L1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="ICSP1" pad="VDD"/>
</signal>
<signal name="FEEDBACK">
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="B+">
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="PWMOUT">
<contactref element="Q7" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="LAMP1">
<contactref element="Q1" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="LAMP2">
<contactref element="Q2" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="LAMP3">
<contactref element="Q3" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="LAMP4">
<contactref element="Q4" pad="1"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="LAMP5">
<contactref element="Q5" pad="1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="LAMP6">
<contactref element="Q6" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="SW">
<contactref element="L1" pad="2"/>
<contactref element="Q7" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="Q7" pad="4"/>
</signal>
<signal name="NL1">
<contactref element="NL1" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="NL2">
<contactref element="NL2" pad="2"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="NL3">
<contactref element="NL3" pad="2"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="NL4">
<contactref element="NL4" pad="2"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="NL5">
<contactref element="NL5" pad="2"/>
<contactref element="Q5" pad="3"/>
</signal>
<signal name="NL6">
<contactref element="NL6" pad="2"/>
<contactref element="Q6" pad="3"/>
</signal>
<signal name="VLAMP">
<contactref element="R4" pad="2"/>
<contactref element="NL6" pad="1"/>
<contactref element="NL5" pad="1"/>
<contactref element="NL4" pad="1"/>
<contactref element="NL3" pad="1"/>
<contactref element="NL2" pad="1"/>
<contactref element="NL1" pad="1"/>
</signal>
<signal name="ICSPDAT">
<contactref element="U1" pad="13"/>
<contactref element="ICSP1" pad="DAT"/>
</signal>
<signal name="ICSPCLK">
<contactref element="U1" pad="12"/>
<contactref element="ICSP1" pad="CLK"/>
</signal>
<signal name="VPP">
<contactref element="U1" pad="4"/>
<contactref element="ICSP1" pad="VPP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
