(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "USLetter")
	(title_block
		(title "Battery Control Box")
		(date "2025-06-03")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Fabrication/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+9V DC INPUT")
	(net 3 "VOUT (+9 V)")
	(net 4 "ADRUINO INPUT")
	(net 5 "unconnected-(U1-NC-Pad2)")
	(net 6 "unconnected-(U1-NC-Pad5)")
	(footprint "BH9VPC:BAT_BH9VPC"
		(layer "F.Cu")
		(at 115.75 82.75)
		(property "Reference" "BT1"
			(at -23.495 -15.875 0)
			(layer "F.SilkS")
		)
		(property "Value" "BH9VPC"
			(at -0.085 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "F"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "20.62mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "MPD"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "battery_control_1_layer.kicad_sch")
		(attr through_hole)
		(fp_text user "-"
			(at 27.94 -6.35 0)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at 27.94 7.62 0)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 27.94 -6.35 0)
			(layer "F.Fab")
		)
		(fp_text user "+"
			(at 27.94 7.62 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -13.625 -11.09)
			(size 2.29 2.29)
			(drill 2.29)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -0.135 11.26)
			(size 2.29 2.29)
			(drill 2.29)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 13.345 -11.09)
			(size 2.29 2.29)
			(drill 2.29)
			(layers "*.Cu" "*.Mask")
		)
		(pad "+" thru_hole circle
			(at 24.945 6.35)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+9V DC INPUT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "-" thru_hole circle
			(at 24.945 -6.35)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/BH9VPC/BH9VPC.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.5mm_Pad"
		(layer "F.Cu")
		(at 155.75 65.75)
		(descr "Mounting Hole 2.5mm, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole")
		(property "Reference" "H2"
			(at 0 -3.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.45 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "battery_control_1_layer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5 5)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.5mm_Pad"
		(layer "F.Cu")
		(at 155.75 100.75)
		(descr "Mounting Hole 2.5mm, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole")
		(property "Reference" "H4"
			(at 0 -3.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.45 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "battery_control_1_layer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5 5)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "ADG1401BRMZ_REEL7:RM_8_ADI-L"
		(layer "F.Cu")
		(at 147.75 94.224999)
		(tags "ADG1401BRMZ-REEL7 ")
		(property "Reference" "U1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ADG1401BRMZ-REEL7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "ADG1401BRMZ-REEL7"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RM_8_ADI RM_8_ADI-M RM_8_ADI-L")
		(sheetname "/")
		(sheetfile "battery_control_1_layer.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.378199 -2.518 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.119 -1.4238 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.119 -1.4238 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.124199 -0.974999)
			(size 1.2064 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+9V DC INPUT")
			(pinfunction "S")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -2.124199 -0.325001)
			(size 1.2064 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "unconnected-(U1-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd rect
			(at -2.124199 0.325001)
			(size 1.2064 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "4" smd rect
			(at -2.124199 0.974999)
			(size 1.2064 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+9V DC INPUT")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 2.124199 0.974999)
			(size 1.2064 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "unconnected-(U1-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "6" smd rect
			(at 2.124199 0.325001)
			(size 1.2064 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "ADRUINO INPUT")
			(pinfunction "IN")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 2.124199 -0.325001)
			(size 1.2064 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_out")
		)
		(pad "8" smd rect
			(at 2.124199 -0.974999)
			(size 1.2064 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VOUT (+9 V)")
			(pinfunction "D")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.5mm_Pad"
		(layer "F.Cu")
		(at 84.25 100.75)
		(descr "Mounting Hole 2.5mm, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole")
		(property "Reference" "H3"
			(at 0 -3.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.45 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "battery_control_1_layer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5 5)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal"
		(layer "F.Cu")
		(at 148.67 81.83 -90)
		(descr "http://www.farnell.com/datasheets/612848.pdf")
		(tags "BNC Amphenol Horizontal")
		(property "Reference" "J4"
			(at 0 -9.08 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at 0.08 -10.58 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "battery_control_1_layer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VOUT (+9 V)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -5.08 -5.08 270)
			(size 3.5 7)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -2.54 0 270)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5.08 -5.08 270)
			(size 3.5 7)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.5mm_Pad"
		(layer "F.Cu")
		(at 84.25 65.75)
		(descr "Mounting Hole 2.5mm, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole")
		(property "Reference" "H1"
			(at 0 -3.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.45 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "battery_control_1_layer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5 5)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 141.25 100.75 90)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -3 180)
			(layer "F.SilkS")
		)
		(property "Value" "Logic"
			(at 0 2.38 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "battery_control_1_layer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "ADRUINO INPUT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 79.75 61)
		(end 161.75 105.25)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "LOGIC"
		(at 141.25 103.75 0)
		(layer "F.SilkS")
	)
	(gr_text "OUTPUT"
		(at 151.75 73.75 0)
		(layer "F.SilkS")
	)
	(embedded_fonts no)
)
