<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>UCC2500</text>
<text>GND</text>
<text>VCC</text>
<text>SI</text>
<text>SCLK</text>
<text>SO</text>
<text>GDO2</text>
<text>GDO0</text>
<text>CSN</text>
</plain>
<libraries>
<library name="mc18-radio">
<description>&lt;b&gt;Radio&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Radio Transmission and Reception Devices
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
<packages>
<package name="QFN-4X4-20L-EP">
<description>&lt;b&gt;QFN-4X4-20L-EP&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Based on : Nordic nRF24L01P
- &lt;a href="http://www.nordicsemi.com/eng/Products/2.4GHz-RF/nRF24L01P"&gt;Product Page&lt;/a&gt;
- &lt;a href="http://www.nordicsemi.com/eng/content/download/2726/34069/file/nRF24L01P_Product_Specification_1_0.pdf"&gt;Datasheet&lt;/a&gt;
&lt;br&gt;Based on : Richtek WQFN-4x4-20
- &lt;a href="http://www.richtek.com/assets/podfiles/PT-000147_FOOTPRINT.pdf"&gt;Footprint Drawing&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
</packages>
</library>
<library name="mc18-clockgen">
<description>&lt;b&gt;Clock Generators&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Devices used to generate or manage clock or timing signals
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
<packages>
<package name="DFN-2.0X1.6-4L-EXT">
<description>&lt;b&gt;DFN-4 (4-SMD)&lt;/b&gt; : 2.0mm x 1.6mm
&lt;br&gt;
&lt;br&gt;Pads extended for hand soldering
&lt;br&gt;
&lt;br&gt;Based on : Abracon ASA
- &lt;a href="http://www.abracon.com/Support/PackageDrawing/Oscillators/ASA.PDF"&gt;Drawing&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
</packages>
</library>
<library name="mercury-ucc">
<packages>
<package name="UCC2500">
</package>
</packages>
</library>
<library name="mc18-passives">
<description>&lt;b&gt;Passives&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Resistors, Capacitors, Inductors
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;0805&lt;/b&gt; SMD Device
&lt;br&gt;

&lt;br&gt;Based on : &lt;a href="http://www.kemet.com/Lists/TechnicalArticles/Attachments/29/f2100e.pdf"&gt;Kemet dimension document&lt;/a&gt; (device, contact sizes)
&lt;br&gt;Based on : &lt;a href="http://www.resistorguide.com/resistor-sizes-and-packages/"&gt;Resistor Guide&lt;/a&gt; (pad sizes)

&lt;br&gt;
&lt;br&gt;Device outline based on standard dimensions
&lt;br&gt;Device contacts based on 25% of device length
&lt;br&gt;PCB pad centered at end of device and sized to match device contact
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
<package name="C0402">
<description>&lt;b&gt;0402&lt;/b&gt; SMD Device
&lt;br&gt;

&lt;br&gt;Based on : &lt;a href="http://www.kemet.com/Lists/TechnicalArticles/Attachments/29/f2100e.pdf"&gt;Kemet dimension document&lt;/a&gt; (device, contact sizes)
&lt;br&gt;Based on : &lt;a href="http://www.resistorguide.com/resistor-sizes-and-packages/"&gt;Resistor Guide&lt;/a&gt; (pad sizes)

&lt;br&gt;
&lt;br&gt;Device outline based on standard dimensions
&lt;br&gt;Device contacts based on 25% of device length
&lt;br&gt;PCB pad centered at end of device and sized to match device contact
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
<package name="L0402">
<description>&lt;b&gt;0402&lt;/b&gt; SMD Device
&lt;br&gt;

&lt;br&gt;Based on : &lt;a href="http://www.kemet.com/Lists/TechnicalArticles/Attachments/29/f2100e.pdf"&gt;Kemet dimension document&lt;/a&gt; (device, contact sizes)
&lt;br&gt;Based on : &lt;a href="http://www.resistorguide.com/resistor-sizes-and-packages/"&gt;Resistor Guide&lt;/a&gt; (pad sizes)

&lt;br&gt;
&lt;br&gt;Device outline based on standard dimensions
&lt;br&gt;Device contacts based on 25% of device length
&lt;br&gt;PCB pad centered at end of device and sized to match device contact
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
<package name="R0402">
<description>&lt;b&gt;0402&lt;/b&gt; SMD Device
&lt;br&gt;

&lt;br&gt;Based on : &lt;a href="http://www.kemet.com/Lists/TechnicalArticles/Attachments/29/f2100e.pdf"&gt;Kemet dimension document&lt;/a&gt; (device, contact sizes)
&lt;br&gt;Based on : &lt;a href="http://www.resistorguide.com/resistor-sizes-and-packages/"&gt;Resistor Guide&lt;/a&gt; (pad sizes)

&lt;br&gt;
&lt;br&gt;Device outline based on standard dimensions
&lt;br&gt;Device contacts based on 25% of device length
&lt;br&gt;PCB pad centered at end of device and sized to match device contact
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="mc18-radio" package="QFN-4X4-20L-EP" value="CC2500">
<attribute name="MPN" value="CC2500RGP"/>
<attribute name="NAME"/>
</element>
<element name="Y1" library="mc18-clockgen" package="DFN-2.0X1.6-4L-EXT" value="26 MHz">
<attribute name="MPN" value="ASA-26.000MHZ-L-T"/>
<attribute name="NAME"/>
<attribute name="EAGLEUP" value="DFN-2.0X1.6-4L"/>
</element>
<element name="U0" library="mercury-ucc" package="UCC2500" value="UCC2500"/>
<element name="C51" library="mc18-passives" package="C0402" value="100nF">
<attribute name="MPN" value="CC0402KRX5R6BB104"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C121" library="mc18-passives" package="C0402" value="100pF">
<attribute name="MPN" value="CC0402JRNPO9BN101"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C122" library="mc18-passives" package="C0402" value="1.0pF">
<attribute name="MPN" value="CC0402CRNPO9BN1R0"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C123" library="mc18-passives" package="C0402" value="1.8pF">
<attribute name="MPN" value="CL05C1R8CB5NNNC"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C124" library="mc18-passives" package="C0402" value="1.5pF">
<attribute name="MPN" value="CL05C1R5CB5NNNC"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C131" library="mc18-passives" package="C0402" value="100pF">
<attribute name="MPN" value="CC0402JRNPO9BN101"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C132" library="mc18-passives" package="C0402" value="1.0pF">
<attribute name="MPN" value="CC0402CRNPO9BN1R0"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="L121" library="mc18-passives" package="L0402" value="1.2nH">
<attribute name="NAME"/>
<attribute name="MPN" value="LQG15HS1N2S02D"/>
</element>
<element name="L122" library="mc18-passives" package="L0402" value="1.2nH">
<attribute name="NAME"/>
<attribute name="MPN" value="LQG15HS1N2S02D"/>
</element>
<element name="L131" library="mc18-passives" package="L0402" value="1.2nH">
<attribute name="NAME"/>
<attribute name="MPN" value="LQG15HS1N2S02D"/>
</element>
<element name="R171" library="mc18-passives" package="R0402" value="56k">
<attribute name="NAME"/>
<attribute name="MPN" value="RC0402FR-0756KL"/>
</element>
<element name="C1" library="mc18-passives" package="C0805" value="1uF">
<attribute name="MPN" value="CC0805KKX7R7BB105"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="L1" library="mc18-passives" package="L0402" value="BEAD">
<attribute name="NAME"/>
<attribute name="MPN" value="BLM15HG102SN1D"/>
</element>
<element name="C41" library="mc18-passives" package="C0402" value="100nF">
<attribute name="MPN" value="CC0402KRX5R6BB104"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C181" library="mc18-passives" package="C0402" value="220pF">
<attribute name="MPN" value="CC0402KRX7R9BB221"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C91" library="mc18-passives" package="C0402" value="220pF">
<attribute name="MPN" value="CC0402KRX7R9BB221"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C111" library="mc18-passives" package="C0402" value="100nF">
<attribute name="MPN" value="CC0402KRX5R6BB104"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C141" library="mc18-passives" package="C0402" value="100nF">
<attribute name="MPN" value="CC0402KRX5R6BB104"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C151" library="mc18-passives" package="C0402" value="220pF">
<attribute name="MPN" value="CC0402KRX7R9BB221"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U0" pad="10"/>
<contactref element="U0" pad="1"/>
<contactref element="U0" pad="11"/>
<contactref element="U0" pad="9"/>
<contactref element="U1" pad="19"/>
<contactref element="U1" pad="P1"/>
<contactref element="U1" pad="16"/>
<contactref element="Y1" pad="2"/>
<contactref element="C51" pad="1"/>
<contactref element="R171" pad="1"/>
<contactref element="C122" pad="1"/>
<contactref element="C123" pad="1"/>
<contactref element="C124" pad="1"/>
<contactref element="L131" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C151" pad="1"/>
<contactref element="C141" pad="1"/>
<contactref element="C111" pad="1"/>
<contactref element="C91" pad="1"/>
<contactref element="C181" pad="1"/>
<contactref element="C41" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="11"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="15"/>
<contactref element="Y1" pad="1"/>
<contactref element="Y1" pad="4"/>
<contactref element="U1" pad="18"/>
<contactref element="C1" pad="2"/>
<contactref element="L1" pad="2"/>
<contactref element="C151" pad="2"/>
<contactref element="C41" pad="2"/>
<contactref element="C181" pad="2"/>
<contactref element="C91" pad="2"/>
<contactref element="C111" pad="2"/>
<contactref element="C141" pad="2"/>
</signal>
<signal name="SI">
<contactref element="U0" pad="3"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="SCLK">
<contactref element="U0" pad="4"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="SO">
<contactref element="U0" pad="5"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="GDO2">
<contactref element="U0" pad="6"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="GDO0">
<contactref element="U0" pad="7"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="CSN">
<contactref element="U0" pad="8"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="ANT">
<contactref element="U0" pad="12"/>
<contactref element="L122" pad="2"/>
<contactref element="C124" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="8"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="C51" pad="2"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="17"/>
<contactref element="R171" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="C121" pad="2"/>
<contactref element="L121" pad="1"/>
<contactref element="C122" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="C131" pad="2"/>
<contactref element="C132" pad="1"/>
<contactref element="L131" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="L121" pad="2"/>
<contactref element="L122" pad="1"/>
<contactref element="C132" pad="2"/>
<contactref element="C123" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="13"/>
<contactref element="C131" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="12"/>
<contactref element="C121" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="U0" pad="2"/>
<contactref element="L1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
